S. No: 29

BILL OF QUANTITES

(A) Description and rate of items based on composite schedule of rates.

**NAME OF WORK: REPAIR & MAINTENANCE OF EXISTING NONFUNCTIONAL TOILETS & DAMAGED BOUNDARY WALLS OF SECONDARY SCHOOLS IN DISTRICT KHAIRPUR (24 UNITS) @ GGHS SALLAR MUHALLA TALUKA KINGRI DISTRICT KHAIRPUR SEMIS CODE: 415040378 (Lev: Block & C/Wall)**

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

S;NO;DESCRIPTION. QTY; RATE.UNIT.AMOUNT.

1/- DismentlingPacca brick work 1;6.(SI:NO:13-b P-10)

1581.0 Rs:1285/63 %cft. 20326/-

2/- DismentlingR.C.C.work 1;2;4.(SI:NO:20 P-10)

353.0 RS:5445/- %cft. 19221/-

3/- Excavation in foundation of building bridges and other str:with excavated earth lead

Upto 5” ft.(SI:NO:18-b P-4)

90.0 Rs:3176/25 %0cft. 285/-

4/- Cementconcerte brick or stone ballast 1 ½” to 2” guage ratio 1;5;10.(SI:NO:4-c P-14)

18.0 Rs:8694/95 %cft. 1565/-

5/- Pacca brick work in foundation and plinth ratio 1;6.(SI:NO:4-a P-20)

1344.0 Rs:11948/35 %cft. 160586/-

6/- R.C.C. work i/c all labouran material except the cost of steel and its labour for bending

And binding which will be paid sepratelly.This rate also i/c all kind of forms mould lifting

Shuttering curring rendering and finshing the exposed surface i/c screening and washing

Of shingle 1;2;4(SI:NO:6-a P-16)

333.0 Rs:337/- P/sft 179621/-

7. Fabrication of mild steel reinforcement for c.c.i/c cutting bending and binding i/c rust

Removal from bars.(SI:NO:8-d p-20)

23.794 Rs: 5001/70 P/cwt. 119010/-

8. Pacca brick work in other than building ratio 1;6.(SI:NO:7-e p-22).

5589.0 Rs:12346/65 %cft. 690054/-

9. Cement plaster ½” thick upto 20” height ratio 1;6.(SI:NO:13-b P=51)

7800.0 Rs:2206/60 %sft 172115/-

10. Cement plaster 3/8” thick upto 20” height ratio 1;4.(SI:NO:11-a P-51)

7800.0 Rs:2197/52 %sft. 171407/-

11. Cement pointing strickingo f joints on walls ratio 1;2.(SI:NO: P- )

4800.0 Rs:1287/44 %sft. 61797/-

12. M/F steel grated door 1/16” thick i/c angle iron frame with locking arranements.(SI:NO:24 p-91)

140.0 Rs:726/72 P/sft. 101741/-

13. S/F broden glasses on courtyard walls i/c 1;3;6 cement concerte coping.(SI:NO:61 P-104)

600.0 Rs;70/40 %cft. 42240/-

14. P/L “ Halla” or patterns tiles glazed 8”x8” on floor walls in required of specified jointed

White cement sand mortoretc complete.(SI:NO:62 P-47)

256.0 RS:34520/31 %sft. 88372/-

15. Colour wash two coats.(SI:NO:23 p-53)

12600.0 Rs:859/90 %sft. 108347/-

16. Painting guard bars iron gates i/c any type etc.(SI:NO:14-d P-68)

280.0 Rs:977/40 %sft. 2737/-

\_\_\_\_\_\_\_\_\_\_\_\_

Total Rs: 19,39424/-