***SCHEDULE OF QUANTITIES***

***WORK No: 06***

# 

**DISTRICT MUNICIPAL CORPORATION (WEST)**

**KARACHI, BALDIA ZONE**

***Estimated Cost Rs: 9,62,661/- Earnest Money Rs: 19,253/-***

***Time Limit: 45 Days Penalty Per Day Rs: 1,000/-***

**SUBJECT: *Repair & Maintenance of AC Firdos Library in UC-32 DMC (West) Baldia Zone.***

|  |
| --- |
|  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ***S.No:*** | ***DESCRIPTION OF WORK*** | ***QUANTITY*** | ***RATE*** | ***PER*** | ***AMOUNT*** |
| *1.* | *Dismantling cement block nasanary.* | *30* | *1134.38* | *%Sft* | *340/-* |
| *2.* | *Excavation for Foundation of Building Bridges and other structure i/c dag bolling dressing refilling ground structure with excavated earth watering and rounding lead up to 5 feet in ordinary soil.* | *1422* | *3176.25* | *%0Cft* | *4517/-* |
| *3.* | *Cement concrete brick or stone ballast 1 ½” to 2” gauge 1:4:8 ratio.* | *230* | *9416.28* | *%Cft* | *21657/-* |
| *4.* | *RCC work in root slab beams columns ratio lintels and other structured members I aid in situ or precast laid in position complete in cell respects .Ratio (1:2:4) go LBS cement 2Cft . Sand 2 Cft shingle 1/8” to ¼” gauge.* | *488* | *337* | *P-Cft* | *164456/-* |
| *5.* | *Fabrication of mold steel reinforcement cement concrete i/c cutting brick laying in position making joints and listening i/c cast of bending wire also i/c removal rust from bars.* | *13.07* | *4820.20* | *P-Cast* | *63000/-* |
| *6.* | *Cement concrete plain i/c placing compacting finishing and coring complete including screening and wishing at stone aggregate without.* | *1417* | *14429.25* | *%Cft* | *204462/-* |
| *7.* | *Lime Nerd Plaster 1:2 with fine finish of nerd plaster mixed with 1% of cement.*  *(b) ¼” thick.* | *2820/-* | *1007.25* | *%Sft* | *28404/-* |
| *8.* | *P/L 1:3:6 C.C Solid block masonry wall 6” thick and below thickness set in 1:6 cement motor ground floor Superstructure i/c raking out joints and airing etc complete.* | *1010* | *15771.01* | *%Cft* | *159287/-* |
| *9.* | *Providing laying precast slab*  *Precast* | *384* | *185* | *P-Sft* | *71040/-* |
| *10* | *Cement plaster 1:4 up to 12” height.*  *(b) ½” thick* | *3636* | *2283.93* | *%Sft* | *83044/-* |
| *11.* | *Distempering two coats.* | *3636* | *1043.90* | *%Sft* | *37956/-* |
| *12.* | *P/F in position doors window of first class deodar wood frames and 1 ¾” thick commercial ply veneer shutter of first class deodar skeleton (Hallow) and commercial play wood (3 ply) on both Side.* | *45.5* | *1227.36* | *P-Sft* | *55845/-* |
| *13.* | *P/F Colleriable door gate channel framing of See lion ¾” x 5/16” at 4” i/c riveted with ¾”x 2/8” flat iron pafli place diagonally and providing with top and bottom traction 1” by 1” along with roller also packing arrangement and fixing in floor and framing etc .* | *59* | *387.04* | *P-Sft* | *22835/-* |
| *14.* | *Painting door and window any type.*   1. *First Coat* 2. *Each Subsequent coat* | *297* | *1160.06* | *%Sft* | *3445/-* |
| *15* | *P/L Different dia P.E Pipe i/c cutting fitting and jointing and leveling i/c testing water with Specified pressures etc complete.* | *200*  *100* | *148*  *28* | *P-Rft*  *P-Rft* | *29600/-*  *2800/-* |

***PTO***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *.16* | *P/F Squatting type while glazed earthen were w.e pan with i/c the cost of flushing cistern with internal fitting and flush pipe with bend and making requisite number of holes in walls plinth and floor for pipe connection and making good and cement concrete 1:2:4 w.e pan of not less than 23” dar opening blw flushing rims and 3 gallons flushing tank with 4” dia C.I trape.* | *01* | *5044.60* | *Each* | *5045/-* |
| *17.* | *P/F 24”X18” buatory basin in white of laz earthen ware complete with & i/c the cost of W.I or C.I cantilever brackets 6” built into wall, painted white in two coat after a primary cost red lead paint a pair of ½” dia rubber plug and chrome plate brass chain 1 ½” dia malleable iron or C.P Brass traps and i/c pedestal.* | *01* | *4928* | *Each* | *4928/-* |
| ***Total Estimated Cost*** | | | | | ***9,62,661.00*** |

*Nomenclature, Quantities and Rates etc checked*

*and found correct.*

***ASSTT: EX-ENGINEER (B&R) EXECUTIVE ENGINEER (B&R)***

*BALDIA ZONE BALDIA ZONE*

*I/We hereby quoted Rates @ % above/below the S/R*

*The total amount is Rs: (Rupees:*

*(In Figure) (In Word)*

## *Contractor’s Signature:*

## 

## *Address:*