**OFFICE OF THE DIRECTOR PARKS**

**Work 01**

**DISTRICT MUNICIPAL CORPORATION (WEST) KARACHI**

**SUBJECT: - P/L KERB BLOCK & COST IRON BENCHES AT LABOUR COLONY**

**PARK SITE ZONE DMC (WEST)**

**E/Cost: 6,30,721/-+O/R E/Money 20,000/- T/Limit ­30 Days Penalty 500/- PD.**

**S.No Description of Work Quantity Rate Per%**

1. Filling watering and riming earth under floor new earth

(Excavated) from out side lead up to one chain and

lift up to 5ft. 23760/Cft 3630%Cft

2. Excavation in Foundation of building, bridges and

other structures including dagbolling dressing re

ground structure with excavated earth watering and

ramming lead upto 5 feet in ordinary soil. 1182/Cft 3176.25%0Cft

3. P/L 1:4:8 plain i/c placing compacting finishing

curing etc comp: 522/Cft 9416.28%Cft

4. P/F Precast edge block 3750 PSI industrial Made Size

6 inches thick X 18” long X 12” high including the

cost of cartage, excavation, from the work for hunching

lean concrete 2250 PSI Concrete for hunching 1:4

cement sand mortar 1576/Rft 297.01/P.Rft

5. Painting on Surface 1576/Sft 1489.68%Sft

6. Grass Cutting Machine Hand 01 No Open Rate

7. P/F Cast iron wooden benches with pen wood beltns

6-0×2"×1" benches size 6-0 vertical with three footed of

cast iron spiral total weight of foot 65 Kg i/c the coast

of nut bolts painting with ready mixed paid of app: make

and shade etc complete. 12Nos Open Rate

8. P/F Fiber Glass 1-9” dust bin dia with M.S Pipe fitting

Moveable as per approved by Office Incharge 04 Nos Open Rate

**DIRECTOR PARKS**

**DMC (WEST) KARACHI**

**I / we hereby quoted \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Above / Below the SR.**

**Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**OFFICE OF THE DIRECTOR PARKS**

**Work 02**

**DISTRICT MUNICIPAL CORPORATION (WEST) KARACHI**

**SUBJECT: - P/F STEEL GATE AND PHYSICAL APPLIANCES AT UC-02 PARK**

**SITE ZONE DMC (WEST)**

**E/Cost: 4,20,254/-+O/R E/Money 20,000/- T/Limit ­30 Days Penalty 500/- PD.**

**S.No Description of Work Quantity Rate Per%**

1. Making and fixing steel grated door complete with

1 / 16” thick sheeting including angle iron frames

2”×2”×3/8” and ¾” Square bar 1" center to center with

locking arrangement 124/Sft 726.72%Sft

2. Painting Doors & Windows any type 124/Sft 1160.06%Sft

3. Removing of Plaster 7646/Sft 121%Sft

4. Stucco Cement Plaster 1:2:4 (Cement stand and Shingle) 7646/Sft 4178.02%Sft

5. P/F Fiber Canopy as per site incharge 01 No Open Rate

6. P/F Slide out fit covered with G.P Sheet as per app:

drawing size 2'' dia pipe 14g 25' Rft support 1¼dia

pipe 14g 1' Sft feet 1' feet 1¼ dia pipe 14g. 01 No Open Rate

7. P/F Seesaw as per app: drawing size pipe 3"dia 14g

7' long 2 seats. 01 No Open Rate

8. P/F merry –go-round center pipe 4'' dia (100.mm)

angle iron and wooden plod covered with m-s sheet

etc as per app: drawing. 61 Nos Open Rate

9. P/F Swing type as per app: drawing size pipe 2"dia

14g 50 cob 8' long 2 seat. 01 No Open Rate

10. Supply of Conocarpus Plants size 4’ to 6’ height as

per directives by Site Engineer 500 Nos Open Rate

**DIRECTOR PARKS**

**DMC (WEST) KARACHI**

**I / we hereby quoted \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Above / Below the SR.**

**Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**OFFICE OF THE DIRECTOR PARKS**

**Work 03**

**DISTRICT MUNICIPAL CORPORATION (WEST) KARACHI**

**SUBJECT: - IMPROVEMENT OF PARDA PARK AT NEW LABOUR COLONY**

**SITE ZONE DMC (WEST)**

**E/Cost: 2,30,668/-+O/R E/Money 20,000/- T/Limit ­30 Days Penalty 500/- PD.**

**S.No Description of Work Quantity Rate Per%**

1. P/L 1:3:6 CC Solid black Masonry wall 6" & below in

thickness set in 1:6 comate motor in ground flour

complete. 697/Cft 15771.01%Cft

2. ¾" thick cement plaster 1:4 upto 20' height. 2036/Sft 2283.93%Sft

3. Erection or removal centering for Rcc or CC Plain

plain work deador wood 2nd class. 198/Sft 3127.41%Sft

4. CC 1:2:4 Situ plain i/c placing compacting finishing

curing etc comp: 99/Cft 14429.25%Cft

5. P/F of pre cast Rcc slab over pre cast gaiter i/c 2''

thick cc copping on the top of the lab etc complete. 80/Sft 309.78/P.Sft

6. Khapriel of cement concrete 12” x 8’ x 1” approved

design / shape laid flat in 1:3:2 grey cement mortar over

as bed of ¾ thick grey cement mortar (1:2) 80/Sft 8977.80%Sft

7. Supplying stacking and spreading app: garden soil

(S/Earth) free from salt and grass roots etc i/c all lead

and lift. 8592/Cft Open Rate

8. Supplying stacking and spreading wall decayed cow

dung manure from app: source i/c all lead and lift. 3072/Cft Open Rate

9. Supply Line (Dacca) grass in slab with earth intact i/c

all lead and lift. 10380/Sft Open Rate

10. P/F mono Block Pumping set 1 H.P Single Phase 220

Volts with ¼ x 1-4” section and other delivery i/c other

fitting (local Made) 01 No Open Rate

11. P/F piston pump in set 1 H.P single phase 220 volts

with 1¼×1¼ suction and delivery (Local made). 01 No Open Rate

12. Supplying stacking and spreading murrum from

app: quarries to required slop i/c consolidation by famig

and watering etc complete. 2279/Cft Open Rate

13. P/F Tank Cover 24” x 24” as per instruction of SITE

Incharge 01 No Open Rate

14. P/F G.I Sheet 12’ 1.5’ with angle Iron Frame necessary

welding & color embedded instruction of Engineer or

Incharge 01 Job Open Rate

15. P/L PVC Pipe 1”dia i/c cutting fitting fixing etc complete 200/Rft 28/P.Rft

16. Rubber Pipe best quality 1”dia 150/Rft Open Rate

17. Valve (local) China i/c cutting of pipr fitting in trench 05 Nos 365.42/Each

18. Dismantling cement concrete plain 1:2:4 432/Cft 3327.50%Cft

**DIRECTOR PARKS**

**DMC (WEST) KARACHI**

**I / we hereby quoted \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Above / Below the SR.**

**Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**