***SCHEDULE OF QUANTITIES***

***WORK No: 01***

# 

**DISTRICT MUNICIPAL CORPORATION (WEST)**

**KARACHI, BALDIA ZONE**

***Estimated Cost Rs: 9,93,503/- Earnest Money Rs: 19,870/-***

***Time Limit: 45 Days Penalty Per Day Rs: 1,000/-***

**SUBJECT: *Proving Providing & Laying 12” Dia R.C.C Pipe Drain at Patni Muhallah Kutyana***

***Muhallah, Dilawar Muhallah, Ghousiya Muhallah, Ward No.02 in UC-34 DMC (West)***

***Baldia Zone.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| ***S.No:*** | ***DESCRIPTION OF WORK*** | ***QUANTITY*** | ***RATE*** | ***PER*** | ***AMOUNT*** | |
| *1.* | *Excavation for pipe line in trenches, and pits in all kind of soil of Murum Shape Leveling of beds of trenches to correct lever & grade, surplus earth within a one chain as directed by Eng incharge.* | *8100* | *4650* | *%Cft* | *37665/-* | |
| *2.* | *Excavation for pipe line in trenches, and pits in hard rock by hammering and chiseling i/c trimming and dressing sides to true alignment and shape leveling of beds of trenches to correct level and grade cutting joints holes and disposal of surplus earth within a one chain as directed by Engineers Incharge. Providing fence guards. Lights flags and temporary crossings for non-vehicular traffic where ever required lift up to 5ft. (1.52m) and lead upto one chain (30.5m)* | *2700* | *24150* | *P-Cft* | *65205/-* | |
| *3.* | *P/L reinforced cement concrete pipes with rubber rings i/c cartage, loading unloading at site of work fixing in trenches cutting fitting, jointing with rubber rings etc complete KWSB Approved Rate, M/S Balochistan R.C.C Pipe Co. M/S Pakistan construction (Pvt.) Ltd. M/S Kamal R.C.C Pipe Co. 12”dia pipe. 15”dia pipe* | *800* | *412.00* | *P/rft* | *329600/-* | |
| *4.* | *Construction of 4” dia manhole inside complete with 21”dia c c 1:2:4 pre cast C.I frame 15kg i/c the cost of M.S bars reinforcement and two handles 5” clear depth c c 1:2:4 cast in situ walls with 50% screened graded bajri of 9” thick i/c bending and channel i/c inside walls surface complete i/c cutting asphalt roads excavation in all kind of soil back filling and disposal of surplus stuff (KW&SB) approved rate.* | *33* | *14529.29* | *Each* | *479467/-* | |
| *5.* | *Extra depth beyond 5” ft or less then 5 deducted at the same rate (KWSB) approved rate.* | *(-) 16.5* | *2538.60* | *Pft* | *(-) 41887/-* | |
| *6.* | *Refilling the excavated stuff & surplus Earth etc. complete.* | *9720* | *2760* | *%Cft* | *26827/-* | |
| *7.* | *Carriage of 100-Cft tons of all kind material like Cole brick i/c loading unloading 10 mile.* | *1080* | *1065.08* | *%Cft* | *11505/-* | |
| *8.* | *Manufacturing and supplying R.C.C main hole covers cast in situ 1:2:4 C.C. 3” inch deep in center reinforced with 3/8” dia M.S Bars welded on M.S. sheet i/c curing transportation.*  *21” dia.* | *41* | *913.63* | *Each* | *37459/-* | |
| *9.* | *Manufacturing and supplying of R.C.C Ring Slab of 21” inside 36” dia outside 75 wide and to thick i/c 3/8” dia tor steel bar two concentric rings with 3/8” dia Nos. cross links bars welded and two sunk type hook, lasted in 1:1-1/2:3 concrete with embedded 15kg C.I frame in per feet position i/c terms partition charges for an average lead of 20 km per trip from casting yard to town office (A minimum of 25 slabs per trip will be transported.)* | *25* | *1906.60* | *Each* | *47665/-* | |
| ***Total Estimated Cost*** | | | | | | ***9,93,503.00*** |

***PTO***

*Nomenclature, Quantities and Rates etc checked*

*and found correct.*

***ASSTT: EX-ENGINEER (B&R) EXECUTIVE ENGINEER (B&R)***

*BALDIA ZONE BALDIA ZONE*

*I/We hereby quoted Rates @ % above/below the S/R*

*The total amount is Rs: (Rupees:*

*(In Figure) (In Word)*

## *Contractor’s Signature:*

## 

## *Address:*