***SCHEDULE OF QUANTITIES***

***WORK No: 12***

# 

**DISTRICT MUNICIPAL CORPORATION (WEST)**

**KARACHI, BALDIA ZONE**

***Estimated Cost Rs: 9,98,868 Earnest Money Rs: 19,978/-***

***Time Limit: 45 Days Penalty Per Day Rs: 1,000/-***

**SUBJECT: *Improvement of R.C.C Drain Pipe Line & C.C Flooring at Baloch Muhallah near Hafeez***

***Baloch House to Kaka House in UC-35 Baldia Zone DMC (West).***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ***S.No:*** | ***DESCRIPTION OF WORK*** | ***QUANTITY*** | ***RATE*** | ***PER*** | ***AMOUNT*** |
| *1.* | *Dismantling cement concrete rain for Separating reinforced cement form concrete cleaning and straightening the same 1:2:4.* | *915* | *5445* | *%Cft* | *49822/-* |
| *2.* | *Earth work excavator in asher sand salt soil or slit clearance undressed lead upto 50Cft.* | *5490* | *1663.75* | *%0Cft* | *9134/-* |
| *3.* | *Fabrication of mild steel reinforced cement concrete i/c cutting butting laying in position making joints and fastening i/c cost of bedding wire also i/c removal rust from bars.* | *28.60* | *4820.20* | *CTW* | *137858/-* |
| *4.* | *P/L R.C.C Work cement concrete 1:2:4 i/c surface finishing and diving into panels etc complete.* | *915* | *337* | *Pft* | *308355/-* |
| *5.* | *Excavation for pipe line in trenches, and pits in all kind of soil of Murum Shape Leveling of beds of trenches to correct lever & grade, surplus earth within a one chain as directed by Eng incharge.* | *1687* | *4650* | *%Cft* | *7844/-* |
| *6.* | *P/L reinforced cement concrete pipes with rubber rings i/c cartage, loading unloading at site of work fixing in trenches cutting fitting, jointing with rubber rings etc complete KWSB Approved Rate, M/S Balochistan R.C.C Pipe Co. M/S Pakistan construction (Pvt.) Ltd. M/S Kamal R.C.C Pipe Co. 15”dia pipe* | *125* | *412* | *P/Rft* | *51500/-* |
| *7.* | *Construction of 4” dia manhole inside complete with 21”dia c c 1:2:4 pre cast C.I frame 15kg i/c the cost of M.S bars reinforcement and two handles 5” clear depth c c 1:2:4 cast in situ walls with 50% screened graded bajri of 9” thick i/c bending and channel i/c inside walls surface complete i/c cutting asphalt roads excavation in all kind of soil back filling and disposal of surplus stuff (KW&SB) approved rate.* | *05-Nos* | *14529.29* | *Each* | *72646/-* |
| *8.* | *Extra depth beyond 5” ft or less then 5 deducted at the same rate (KWSB) approved rate.* | *(-) 2.5* | *2538.60* | *Pft* | *6346/-* |
| *9.* | *Refilling the excavated stuff & surplus Earth etc. complete.* | *1631* | *2760* | *%Cft* | *4502/-* |
| *10.* | *Dismantling Cement concrete plain 1:4:8.* | *1706* | *1663.75* | *%0Cft* | *2838/-* |
| *11* | *P/L cement concrete brick or stone 6 ballast 1 ½” to 2” gauge 1:4:8.under floor.* | *1706* | *9416.28* | *%Cft* | *160642/-* |
| *12.* | *P/L 2” thick topping cement concrete 1:2:4 i/c surface finishing and diving into panels etc complete.* | *3412* | *3275.50* | *%Sft* | *111760/-* |
| *13.* | *Carriage of 100 cft tons of all kinds’ material like Cole bricks i/c loading unloading 10 miles.* | *8292* | *1065.04* | *%Cft* | *88313/-* |
| ***Total Estimated Cost*** | | | | | ***9,98,868.00*** |

***PTO***

*Nomenclature, Quantities and Rates etc checked*

*and found correct.*

***ASSTT: EX-ENGINEER (B&R) EXECUTIVE ENGINEER (B&R)***

*BALDIA ZONE BALDIA ZONE*

*I/We hereby quoted Rates @ % above/below the S/R*

*The total amount is Rs: (Rupees:*

*(In Figure) (In Word)*

## *Contractor’s Signature:*

## 

## *Address:*