SCHEDULE-B:- M/R TO SUPERINTENDENT BUNGALOW COMPOUND WALL @ CENTERAL JAIL KHAIRPUR

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| S# | NAME OF ITEM | NO:L.B.D | QTY: | RATE | UNIT | AMOUNT |

01/- Excavation in foundation of building bridges and other structures i/c dag balling dressing refilling around structure with excavated earth watering and ramming lead up-to 5ft. (b) in ordinary soil. (S.I.No.18 (b) P.No.4)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | |  |  |  |  |  |  |
|  | Total | **=** | **3600** | **Cft** | **3176.25** | **%Cft** | **11435/-** |

02/- Cement concrete stone of brick ballast 1½” to 2” gauge. Ratio (1:4:8). (S.I.No.4 (c) P.No.15)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | |  |  |  |  |  |  |
|  | Total | **=** | **600** | **Cft** | **9416.28** | **%Cft** | **11435/-** |

03/- Fabrication of mild steel reinforcement for cement concrete i/c cutting bending laying in position making joints and fastenings i/c cost of binding wire (also includes removal of rust from bars) (a) Using tor bars. (S.I.No.7 (a) P.No.20)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  |  | **=46.741** | **“** | **5001.70** | **P.cwt** | **233785/-** |

04/- R.C.C. work in roof slab beams columns rafts lintels and other structural members laid in situ or precast laid in position complete in all respects: (i) Ratio (1:2:4) 90 lbs cement 2 cft sand 4 cft shingle 1/8” to 1/4” gauge. (S.I NO: 6 P-19)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | **=** | **1613** | **“** | **337/-** | **P.Cft** | **543581/-** |

05/- Random Rubble masonry (Un-Coursed )including hammer dressing in cement /sand mortar Ratio (1:6).(S.NO: 1 (iv)P26

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | Total | **=** | **1200** | **Cft** | **17723/-** | **% Cft** | **212676/-** |
|  |  |  |  |  |  |  |  |

06/- Coursed Rubble Masonry including hammer dressing in cement sand mortar Ratio (1:6). (S.I NO: P.NO: )

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | Total | **=** | **1830** | **“** | **25321/-** | **% Cft** | **463374/-** |

07/- Pacca brick work in Other than Building in Cement Sand mortar 1:6 (S.I NO: 50 (d)P )

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | Total | **=** | **1785** | **“** | **12346.65** | **% Cft** | **220388/-** |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **08/-** | Cement Plaster 1:6 up to 20-0 height ½” thick (S.I NO: P.NO: ). | | | |  |  |  |  |
|  |  |  | **=** | **5600** | **Sft** | **2206.60** | **% Sft** | **123570/-** |

**10/-** Pointing flush on Stone work in cement mortar (S.I NO: P.NO: )

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | Total | **=** | **3000** | **“** | **1062.33** | **% Cft** | **31870/-** |

**11/-** Distempering 03 coats (S.I NO: P.NO:

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | Total | **=** | **6400** | **“** | **1079.65** | **% Cft** | **69098/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  | **================================================** | | | | |
|  |  |  |  | **Total** |  |  | **1966275/-** |
|  |  |  |  |  |  |  |  |

CONTRACTOR EXECUTIVE ENGINEER,

PROVINCIAL BUILDINGS DIVISION

SHAHEED BENAZIR ABAD