|  |  |
| --- | --- |
| **NAME OR WORK :-** | **M/R TO SINDH SECRETARIAT NO.III ( OLD K.D.A ) BUILDING KARACHI**  **( P/F GI SHADE FOR VENDOR REMAINING WORKS ).** |

**“ SCHEDULE ‘B’ “**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION OF ITEMS** | **QTY:** | **RATE** | **UNIT** | **AMOUNT** |
|  | **SCHEDULE ITEMS PART-“A” ( CIVIL WORK )** |  |  |  |  |
| 1 | Dismantling cement concrete plain 1:2:4(SI19-c/ P-10 ). | 841.99 Cft. | 3327/50 | %Cft. | 28017/- |
|  | Rupees. three thousand three hundred twenty seven. And fifty. Paisa | | | | |
| 2 | P/F cement paving blocks flooring having size 197x197x60 (mm) of city / quddra / cobble shape with pigmented having strength b/w 5000 psi to 8500 psi in/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete. (SI-73/P-49) | 1014.46 Sft. | 223/97 | P/Sft. | 227209/- |
|  | Rupees. two hundred twenty three. And. Ninety seven. Paisa | | | | |
| 3 | Cement concrete plain including placing compacting, finishing and curing, complete ( including screening and washing at stone aggregate without shuttering.(i). Ratio 1: 4: 8. ( SI.5-i / P-16 ). | 335.88 Cft | 11288/75 | %Cft | 37917/- |
|  | Rupees. eleven thousand two hundred eighty eight. And. Seventy five. Paisa | | | | |
|  |  |  | **Total Rs.** | | **294157/-** |
|  | Above / Below Rs. | | | |  |
|  | **(A). Total Rs.** | | | |  |
|  | **NON-SCHEDULE ITEMS PART-“B”** |  |  |  |  |
| 1 | P/F G.I. shade with G.I. sheet 18” gauge in/c necessary frame work of angle iron or GI pipe & fixing GI sheet with nut bolts / screws in proper design & shape as directed by the Engineer Incharge. | 1052.03 Sft. |  | P/Sft. |  |
| 2 | Providing and fixing cement concrete Kerb Blocks (Envicrete make) of size 36”x12” in grey colour having crushing strength not less than 5000 PSI laid over a bed of 3” thick cement sand mortar & laying kerbs properly compacted maintaining slop and filling joints with cement sand mortar etc the cost in/c dismantling old Cc kerbs or stone blocks excavation upto required depth & laying kerbs blocks also in/c all cartage labour & material as directed by the Engineer Incharge. | 150.29 Rft. |  | P/Rft. |  |
|  |  |  | **(B). Total Rs.** | |  |
|  |  |  | **(A). Total Rs.** | |  |
|  |  | **G. Total (A + B ) Total Rs:-** | | |  |
|  |  | **Say Rs.** | | |  |

**CONDITION.**

1). Typographical errors in the schedule-“B” are the subject to the correction with reference to the schedule of rate ( Gen: Vol: III, Part-II, inforced: 2012, as approved by the standing rates committee.

2). No Cartage will be paid on any items of works.

3). No premium shall be paid on Non-Schedule items.

4). Water shall be arranged by the Contractor.

|  |  |  |
| --- | --- | --- |
| **CONTRACTOR.** | **ASSISTANT ENGINEER**  **PROVINCIAL BUILDINGS SUB-DIVISION-V,**  **KARACHI.** | **EXECUTIVE ENGINEER**  **PROVINCIAL BUILDINGS DIVISION-II,**  **KARACHI.** |