|  |  |
| --- | --- |
| **NAME OF WORK** | **M/R TO SINDH SECRETARIAT BUILDING NO. VI (OLD STATE BANK) KARACHI**  **(GROUND FLOOR LAW DEPARTMENT ALUMINUM PARTITION FALSE CEILING& TILES.)** |

**“ SCHEDULE “B“**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION OF ITEMS** | **QTY:** | **RATE** | **UNIT** | **AMOUNT** |
|  | **PART “A” SCHEDULE ITEMS.** |  |  |  |  |
| 1 | Providing and fixing in position doors, windows and ventilators of 1st class deodar wood frames and 1-1/2” thick Teak wood ply shutters of 2nd class deodar wood skeleton ( solid ) styles and rails core of partal wood and commercial ply wood ( 3-Ply ) on both side in/c hold fasts, hinges, Iron tower bolts, handles and cleats with cord etc complete.  ( SI.58 / P-65 ) – ( SI.25-b / P-61 )  Rs.1077/06 ( - ) Rs.370/83 = **706/23** | 255.00 Sft | 706/23 | P.Sft | 180089/- |
|  | Rupees (Seven hundred six & Ps. Twenty three) only. | | | | |
| 2 | Providing and fixing approved quality mortice lock. ( SI.21 / P-60 ). | 20 Nos | 1786/13 | Each | 35723/- |
|  | Rupees (One thousand seven hundred eighty six & Ps. Thirteen ) only. | | | | |
| 3 | P/F with sunk iron screws wooden Architrave approved design/ shape having width not less than 2- 1/2 inches as directed by Engineer Incharge. ( SI.60/P-65 ) | 544.00 Rft | 49/97 | P.Rft | 27184/- |
|  | Rupees (Fourty nine & Ps. Ninety seven) only. | | | | |
| 4 | Scraping ( b) Ordinary distemper oil bound distemper or Pain on Walls. ( SI.54-(b) / P-13 ). | 2784.00  Sft | 226/88 | %Sft | 6316/- |
|  | Rupees (Two hundred twenty six & Ps. Eighty eight) only. | | | | |
| 5 | Preparing the surface & painting with matt finish paint of approved make to old matt finish surface (2nd & subsequent coat  (37-a+b / P-55) | 2784.00  Sft | 1772/38 | %Sft | 49343/- |
|  | Rupees (One thousand seven hundred seventy two & Ps. Thirty eight) only. | | | | |
| 6 | Painting old surface (c ) Painting doors and windows any type. (i) 1st coat (ii) second & subsequent coat ( SI.4( c ) ( i + ii )/P-68 ). | 923.00 Sft | 1160/06 | %Sft | 10707/- |
|  | Rupees (One thousand one hundred sixty & Ps. Six ) only. | | | | |
| 7 | Removing window and sky light with chowkats. ( 13-a P/12) | 25-Nos | 102/85 | P No. | 2571/- |
|  | Rupees (One hundred two & ps. Eighty five) only. | | | | |
|  | **Total Rs.** | | | | **311933/-** |
|  | Above / below on Rs. | | | |  |
|  | **(A). Total Rs.** | | | |  |
|  | **PART “ B” NON-SCHEDULE ITEM** |  |  |  |  |
| 1 | P/F Aluminum partition with fixed glass (frosted) 5mm thick using 4” lucky section in champion color as frame on floor or block masonry fixed with necessary fixtures rubber packings etc. The cost in/c tools & plants used in making and carriage from shop to site as directed by the Engineer Incharge. | 900.Sft |  | P.Sft |  |
| 2 | P/F false ceiling of Gypsum board panels of required design & size in/c frame work of aluminum T-Section hanged with nail wire to ceiling etc complete. | 3380.00 Sft |  | P.Sft |  |
| 3 | P/F wooden cabinet with shutter and back shelves by using laminated Lassani sheet 3/4" thick and frame work of 1st class partal wood 2”x1” with 18” deep box in/c providing & fixing wooden leaping or gola around Lassani shutter or making gola by router in approved design & shape & polishing it. The cost in/c necessary hinges, catchers, handles, sliding wheels in draws, nails, screws, draws locks etc. The cost also in/c necessary tools and plants to be used in making etc complete as directed by the Engineer Incharge. | 40.00 Sft |  | P.Sft |  |
| 4 | Supplying and fixing in position Aluminum channels framing 2-mm thick for sliding windows & ventilators of Lucky or equivalent made with 5mm thick tinted glass glazing (Belgium) and aluminum fly screen, handles, stoppers and locking arrangement etc complete. (b) Deluxe Model (Bronze of Champion color) | 252.00 Sft |  | P.Sft |  |
| 5 | P/L Porcelain tiles glazed or matt glazed Master or equivalent jointed in white cement and laid over 1:2 grey cement sand mortar ¾” thick in/c finishing & filling of joints with slurry of white cement or tile grout in desired shape in/c cutting of tiles to proper profile (on floor or facing) **size 24”x24””x1/4”.** | 926.00 -Sft |  | PSft |  |
|  |  |  | **Total Rs. (B).** | |  |
|  |  |  | **Total Rs. (A).** | |  |
|  |  |  | **G. Total (A + B )** | |  |
|  |  |  | **Say Rs.** | |  |

**CONDITION.**

1). Typographical errors in the schedule-“B” are the subject to the correction with reference to the schedule of rate ( Gen: Vol: III, Part-II, inforced: 2012, as approved by the standing rates committee.

2). No Cartage will be paid on any items of works.

3). No premium shall be paid on Non-Schedule items.

4). Water shall be arranged by the Contractor.

|  |  |  |
| --- | --- | --- |
| **CONTRACTOR.** | **ASSISTANT ENGINEER**  **PROVINCIAL BUILDINGS SUB-DIVISION-V,**  **KARACHI.** | **EXECUTIVE ENGINEER**  **PROVINCIAL BUILDINGS DIVISION-II,**  **KARACHI.** |