|  |  |
| --- | --- |
| **NAME OR WORK :-** | **M/R TO SINDH SECRETARIAT NO.III ( OLD K.D.A ) BUILDING KARACHI**  **( P/F TILES, FALSE CEILING WALL PANELING @ GROUND FLOOR & 1ST FLOOR CORRIDOR & ROOMS.) (Remaining Works)** |

**“ SCHEDULE “B “**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION OF ITEMS** | **QTY:** | **RATE** | **UNIT** | **AMOUNT** |
|  | **SCHEDULE ITEMS PART-“A” ( CIVIL WORK )** |  |  |  |  |
| 1 | Scraping ( b) Ordinary distemper oil bound distemper or Pain on Walls. ( SI.54-(b) / P-13 ). | 2376.00-Sft  Sft | 226/88 | %Sft | 5391/- |
|  | Rupees (Two hundred twenty six & Ps. Eighty eight) only. | | | | |
| 2 | Preparing the surface and painting with matt finish paint of approved make to old matt finish ( b ). 2nd & subsequent coat. ( SI.37(A+B) / P-55 ). | 2376.00-Sft  Sft | 1772/38 | %Sft | 42112/- |
|  | Rupees (One thousand seven hundred seventy two & Ps. Thirty eight) only. | | | | |
|  | **Total Rs.** | | | | **47503/-** |
|  | **Above / Below Rs:** | | | |  |
|  | **(A). Total Rs.** | | | |  |
|  | **SCHEDULE ITEMS PART-“B” (Electric Works)** |  |  |  |  |
| 1 | Wiring for light or fan point with 3/.029 PVC insulated wire in 20mm ( ¾” ) PVC conduit recessed in the wall or column as required.( SI.124 / P-15 ). | 49 Nos | 1130/- | P/Point | 55370/- |
|  | Rupees (One thousand one hundred thirty) only. | | | | |
| 2 | Wiring for plug point with 3/.029 PVC insulated wire in 20mm ( ¾” ) PVC conduit recessed in the wall or column as required.( SI.126 / P-15 ). | 08 Nos | 985/- | P.Point | 7880/- |
|  | Rupees (Nine hundred eighty five) only. | | | | |
|  |  | **Total Rs.** | | | **63250/-** |
|  |  | **Above / Blow Rs:** | | |  |
|  |  | **(B). Total Rs:** | | |  |
|  | **NON-SCHEDULE ITEMS PART-“C”** |  |  |  |  |
| 1 | P/L Porcelain tiles glazed or matt glazed Master or equivalent jointed in white cement and laid over 1:2 grey cement sand mortar ¾” thick in/c finishing & filling of joints with slurry of white cement or tile grout in desired shape in/c cutting of tiles to proper profile (on floor or facing) **size 24”x24”x1/4”** | 2506.00 Sft |  | PSft |  |
| 2 | P/F false ceiling of Gypsum board panels of required design & size in/c frame work of aluminum T-Section hanged with nail wire to ceiling etc complete. | 575.00 Sft. |  | P/Sft. |  |
| 3 | P/F Gypsum board pelmet to be hanged from ceiling in specified shape and design as approved by the consultant. This in/c cutting the existing Gypsum board false ceiling in proper shape, hanging the structure by aluminum angle 1’x1” @ 3’-0 apart drilled and screwed in RCC slab, making hanging frame by using Aluminum U-channel section 1-1/2” wide in 18”x18” rafters and fixing Gypsum board sheet with chips and screws. Then filling the joints & screws holes with plastic mesh and plaster of Paris and making surface smooth as directed by the Engineer Incharge. | 814.00 Sft |  | PSft |  |
| 4 | S/F LED spot light China make with 7 Nos lamps each 6 watts fitted on walls, ceiling of approved quality as directed by the Engineer Incharge. | 98-Nos |  | Each |  |
| 5 | P/F Switch 5-Amp Plug Socket with fancy type Sheet ( Imported make ) including Plastic Board with necessary electric connection etc complete (Clipsal or equivalent | 63 Nos |  | Each |  |
| 6 | P/F wall paneling with lassani sheet 3/4" thick and teak ply in/c frame work of partal wood 2”x1” & fixing lassani sheet & then teak ply in approved design and texture including all cost of labour making & cartage etc complete. | 207.00  Sft |  | P/Sft. |  |
|  |  |  | **(C). Total Rs.** | |  |
|  |  |  | **(B). Total Rs.** | |  |
|  |  |  | **(A). Total Rs.** | |  |
|  |  | **G. Total (A + B ) Total Rs:-** | | |  |
|  |  | **Say Rs.** | | |  |

**CONDITION.**

1). Typographical errors in the schedule-“B” are the subject to the correction with reference to the schedule of rate ( Gen: Vol: III, Part-II, inforced: 2012, as approved by the standing rates committee.

2). No Cartage will be paid on any items of works.

3). No premium shall be paid on Non-Schedule items.

4). Water shall be arranged by the Contractor.

|  |  |  |
| --- | --- | --- |
| **CONTRACTOR.** | **ASSISTANT ENGINEER**  **PROVINCIAL BUILDINGS SUB-DIVISION-V,**  **KARACHI.** | **EXECUTIVE ENGINEER**  **PROVINCIAL BUILDINGS DIVISION-II,**  **KARACHI.** |