**BILL OF QUANITITY (B.O.Q)**

**PART “B” WATER SUPPLY & S/FITTING**

**NAME OF WORK REPAIR / MAINTENANCE OF GOVT: BOYS PRIMARY SCHOOL PARO JO KHOOH (COMPOUND WALL & LAV BLOCK) TALUKA & DISTRICT DADU (2016-17) PROG:**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S#** | **ITEM OF WORK** | **QNTY** | **RATE** | **UNIT** | **AMOUNT** |
| 1 | P/F Squatting type white glazed earthen were w.c pan with including the cost of flushing cistern with internal fitting and flush pipe with bend & making requisite number of holes in walls plinth & floor for pipe connections & making good in cement concrete 1:2:4 (S.I.N:1(b)P/1) | 2.0 | 5044.60 | P.No | 10089 |
| 2 | Providing G.I pipe specials & clamps etc including fixing cutting and fitting complete with and i/c the cost of breaking rough wall and roof making good etc painting two coats after cleaning the pipe etc white zink point with pigment to match the colour of building (S.I.NO:1P/12) |  |  |  |  |
|  | 1/2” dia | 50.00 | 73.21 | p.rft | 3661 |
|  | 3/4” dia | 50.00 | 95.89 | p.rft | 4795 |
| 3 | Providing fixing handle valves (china) (S.I:No:5 | 2.00 | 271.92 | P.No | 544 |
| 4 | Construction of main hole or inspection diameter of circular sewer and 3”6” (1067mm)depth with wall of B.B in cement plastered 1:3.1/2”thick ,inside of wall and 1”(25 mm))thick over benching and channel i/c etc.complete | 4.00 | 14748 | P.NO | 58992 |
| 5 | S/Fixing long bib-cook of superior quality with c.p head ½” dia (S.I.N.O:13 P/10) | 2.00 | 1109.46 | P.NO | 2219 |
| 6 | S/Fixing concealed tee-stop cock of superior quality with c.p head ½”dia .(S.I.NO: 12(b) P/18) | 2.00 | 889.46 | P.NO | 1779 |
| 7 | Providing R.C.C pipe with collars class “B” and digging the to required depth & fixing in positing i/c cutting fitting & jointing with maxphalt composition cement to a head of 4” feet above the top of the heightest pipe & refilling excavated staff 6” pipe class “B” |  |  |  |  |
|  | 6” dia | 50.00 | 199.25 | P.rft | 9963 |
|  | 4’’ dia | 30.00 | 146.00 | P.Rft | 4380 |
|  | P/F Hand Pump with all accessories wooden shown i/c boring cutting etc. (R.A) |  |  |  |  |
| A | Filer | 10.0 | 76.05 | P.Rft | 761 |
| B | Boring | 80.0 | 38.50 | P.Rft | 3080 |
| C | Hand Pump | 01.0 | 1442.0 | Each | 1442 |
| 9 | Providing and fixing water pumping set ½ H.P Mono Blck single phase 220 bolts with 1”x1-1/4” suction and delivery 20 ft head including making c.c 1:3:6 platform of required size and fixing with nuts and bolts (local made). (R.A) | 01.0 | 14417.70 | Each | 14418.0 |
|  |  |  | Total: |  | 116095.0 |
|  |  |  | N.S.I |  | 19673.0 |
|  |  |  | S.I |  | 96422.0 |

**10 % Above /below 3 on the Rates of CSR Amount tobe added/aeduted on**

**Basis of premium quoted Total (b)**

**Total A+B Rs: (a)\_\_\_\_\_\_\_\_\_\_\_\_ Rs: (b)\_\_\_\_\_\_\_\_\_\_\_\_\_ Rs:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**R.CC (a) 10 & Rs:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Total Amount Rs:\_\_\_\_\_\_\_\_\_\_\_\_Fabrication (a) 10 % Above Rs:\_\_\_\_\_\_\_\_\_\_\_\_ Total Amount Rs: \_\_\_\_\_\_\_\_\_\_\_\_**

**Total (A) +b in works & Figure\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**NOTE:- Quantities/Rates can be changed after Technical sanctioned is received from competent authortity.**

**CONTRACTORT EXECUTIVE ENGINEER**

**EDUCATION WORKS DIVISION**

**DADU**

**BILL OF QUANITITY (B.O.Q)**

**PART “B” WATER SUPPLY & S/FITTING**

**NAME OF WORK REPAIR / MAINTENANCE OF GOVT: BOYS PRIMARY SCHOOL IBRAHIM CHANDIO (COMPOUND WALL & LAV BLOCK) TALUKA & DISTRICT DADU**

**(2016-17) PROG:**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S#** | **ITEM OF WORK** | **QNTY** | **RATE** | **UNIT** | **AMOUNT** |
| 1 | P/F Squatting type white glazed earthen were w.c pan with including the cost of flushing cistern with internal fitting and flush pipe with bend & making requisite number of holes in walls plinth & floor for pipe connections & making good in cement concrete 1:2:4 (S.I.N:1(b)P/1) | 2.0 | 5044.60 | P.No | 10089 |
| 2 | Providing G.I pipe specials & clamps etc including fixing cutting and fitting complete with and i/c the cost of breaking rough wall and roof making good etc painting two coats after cleaning the pipe etc white zink point with pigment to match the colour of building (S.I.NO:1P/12) |  |  |  |  |
|  | 1/2” dia | 50.00 | 73.21 | p.rft | 3661 |
|  | 3/4” dia | 50.00 | 95.89 | p.rft | 4795 |
| 3 | Providing fixing handle valves (china) (S.I:No:5 | 2.00 | 271.92 | P.No | 544 |
| 4 | Construction of main hole or inspection diameter of circular sewer and 3”6” (1067mm)depth with wall of B.B in cement plastered 1:3.1/2”thick ,inside of wall and 1”(25 mm))thick over benching and channel i/c etc.complete | 2.00 | 14748 | P.NO | 29496 |
| 5 | S/Fixing long bib-cook of superior quality with c.p head ½” dia (S.I.N.O:13 P/10) | 2.00 | 1109.46 | P.NO | 2219 |
| 6 | S/Fixing concealed tee-stop cock of superior quality with c.p head ½”dia .(S.I.NO: 12(b) P/18) | 2.00 | 889.46 | P.NO | 1779 |
| 7 | Providing R.C.C pipe with collars class “B” and digging the to required depth & fixing in positing i/c cutting fitting & jointing with maxphalt composition cement to a head of 4” feet above the top of the heightest pipe & refilling excavated staff 6” pipe class “B” |  |  |  |  |
|  | 6” dia | 50.00 | 199.25 | P.rft | 9963 |
|  | 4’’ dia | 30.00 | 146.00 | P.Rft | 4380 |
|  | P/F Hand Pump with all accessories wooden shown i/c boring cutting etc. (R.A) |  |  |  |  |
| A | Filer | 10.0 | 76.05 | P.Rft | 761 |
| B | Boring | 80.0 | 38.50 | P.Rft | 3080 |
| C | Hand Pump | 01.0 | 1442.0 | Each | 1442 |
| 9 | Providing and fixing water pumping set ½ H.P Mono Blck single phase 220 bolts with 1”x1-1/4” suction and delivery 20 ft head including making c.c 1:3:6 platform of required size and fixing with nuts and bolts (local made). (R.A) | 01.0 | 14417.70 | Each | 14418.0 |
|  |  |  | Total: |  | 86599.0 |
|  |  |  | N.S.I |  | 19673.0 |
|  |  |  | S.I |  | 66926.0 |

**10 % Above /below 3 on the Rates of CSR Amount tobe added/aeduted on**

**Basis of premium quoted Total (b)**

**Total A+B Rs: (a)\_\_\_\_\_\_\_\_\_\_\_\_ Rs: (b)\_\_\_\_\_\_\_\_\_\_\_\_\_ Rs:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**R.CC (a) 10 & Rs:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Total Amount Rs:\_\_\_\_\_\_\_\_\_\_\_\_Fabrication (a) 10 % Above Rs:\_\_\_\_\_\_\_\_\_\_\_\_ Total Amount Rs: \_\_\_\_\_\_\_\_\_\_\_\_**

**Total (A) +b in works & Figure\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**NOTE:- Quantities/Rates can be changed after Technical sanctioned is received from competent authortity.**

**CONTRACTORT EXECUTIVE ENGINEER**

**EDUCATION WORKS DIVISION**

**DADU**

**BILL OF QUANITITY (B.O.Q)**

**PART “B” WATER SUPPLY & S/FITTING**

**NAME OF WORK REPAIR / MAINTENANCE OF GOVT: GIRLS PRIMARY SCHOOL SHER MOHAMMAD DAWACH (COMPOUND WALL & LAV BLOCK) TALUKA & DISTRICT DADU (2016-17) PROG:**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S#** | **ITEM OF WORK** | **QNTY** | **RATE** | **UNIT** | **AMOUNT** |
| 1 | P/F Squatting type white glazed earthen were w.c pan with including the cost of flushing cistern with internal fitting and flush pipe with bend & making requisite number of holes in walls plinth & floor for pipe connections & making good in cement concrete 1:2:4 (S.I.N:1(b)P/1) | 1.0 | 5044.60 | P.No | 5044.60 |
| 2 | Providing G.I pipe specials & clamps etc including fixing cutting and fitting complete with and i/c the cost of breaking rough wall and roof making good etc painting two coats after cleaning the pipe etc white zink point with pigment to match the colour of building (S.I.NO:1P/12) |  |  |  |  |
|  | 3/4” dia | 50.00 | 95.89 | p.rft | 4795 |
| 3 | Providing fixing handle valves (china) (S.I:No:5 | 2.00 | 271.92 | P.No | 544 |
| 5 | S/Fixing long bib-cook of superior quality with c.p head ½” dia (S.I.N.O:13 P/10) | 1.00 | 1109.46 | P.NO | 1109.46 |
| 6 | S/Fixing concealed tee-stop cock of superior quality with c.p head ½”dia .(S.I.NO: 12(b) P/18) | 1.00 | 889.46 | P.NO | 889.46 |
| 7 | Providing R.C.C pipe with collars class “B” and digging the to required depth & fixing in positing i/c cutting fitting & jointing with maxphalt composition cement to a head of 4” feet above the top of the heightest pipe & refilling excavated staff 6” pipe class “B” |  |  |  |  |
|  | 4’’ dia | 30.00 | 146.00 | P.Rft | 4380 |
| 8 | P/F Hand Pump with all accessories wooden shown i/c boring cutting etc. (R.A) |  |  |  |  |
| A | Filer | 10.0 | 76.05 | P.Rft | 761 |
| B | Boring | 80.0 | 38.50 | P.Rft | 3052 |
| C | Hand Pump | 01.0 | 1442.0 | Each | 1442 |
| 9 | Providing and fixing water pumping set ½ H.P Mono Blck single phase 220 bolts with 1”x1-1/4” suction and delivery 20 ft head including making c.c 1:3:6 platform of required size and fixing with nuts and bolts (local made). (R.A) | 01.0 | 14417.70 | Each | 14418.0 |
|  |  |  | Total: |  | 36434.0 |
|  |  |  | N.S.I |  | 19673.0 |
|  |  |  | S.I |  | 16761.0 |

**10 % Above /below 3 on the Rates of CSR Amount tobe added/aeduted on**

**Basis of premium quoted Total (b)**

**Total A+B Rs: (a)\_\_\_\_\_\_\_\_\_\_\_\_ Rs: (b)\_\_\_\_\_\_\_\_\_\_\_\_\_ Rs:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**R.CC (a) 10 & Rs:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Total Amount Rs:\_\_\_\_\_\_\_\_\_\_\_\_Fabrication (a) 10 % Above Rs:\_\_\_\_\_\_\_\_\_\_\_\_ Total Amount Rs: \_\_\_\_\_\_\_\_\_\_\_\_**

**Total (A) +b in works & Figure\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**NOTE:- Quantities/Rates can be changed after Technical sanctioned is received from competent authortity.**

**CONTRACTORT EXECUTIVE ENGINEER**

**EDUCATION WORKS DIVISION**

**DADU**

**BILL OF QUANITITY (B.O.Q)**

**PART “B” WATER SUPPLY & S/FITTING**

**NAME OF WORK REPAIR / MAINTENANCE OF GOVT: BOYS PRIMARY SCHOOL NARI WALL LUND (COMPOUND WALL & LAV BLOCK) TALUKA & DISTRICT DADU (2016-17) PROG:**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S#** | **ITEM OF WORK** | **QNTY** | **RATE** | **UNIT** | **AMOUNT** |
| 1 | P/F Squatting type white glazed earthen were w.c pan with including the cost of flushing cistern with internal fitting and flush pipe with bend & making requisite number of holes in walls plinth & floor for pipe connections & making good in cement concrete 1:2:4 (S.I.N:1(b)P/1) | 1.0 | 5044.60 | P.No | 5044.60 |
| 2 | Providing G.I pipe specials & clamps etc including fixing cutting and fitting complete with and i/c the cost of breaking rough wall and roof making good etc painting two coats after cleaning the pipe etc white zink point with pigment to match the colour of building (S.I.NO:1P/12) |  |  |  |  |
|  | 3/4” dia | 50.00 | 95.89 | p.rft | 4795 |
| 3 | Providing fixing handle valves (china) (S.I:No:5 | 2.00 | 271.92 | P.No | 544 |
| 5 | S/Fixing long bib-cook of superior quality with c.p head ½” dia (S.I.N.O:13 P/10) | 1.00 | 1109.46 | P.NO | 1109.46 |
| 6 | S/Fixing concealed tee-stop cock of superior quality with c.p head ½”dia .(S.I.NO: 12(b) P/18) | 1.00 | 889.46 | P.NO | 889.46 |
| 7 | Providing R.C.C pipe with collars class “B” and digging the to required depth & fixing in positing i/c cutting fitting & jointing with maxphalt composition cement to a head of 4” feet above the top of the heightest pipe & refilling excavated staff 6” pipe class “B” |  |  |  |  |
|  | 4’’ dia | 30.00 | 146.00 | P.Rft | 4380 |
| 8 | P/F Hand Pump with all accessories wooden shown i/c boring cutting etc. (R.A) |  |  |  |  |
| A | Filer | 10.0 | 76.05 | P.Rft | 761 |
| B | Boring | 80.0 | 38.50 | P.Rft | 3052 |
| C | Hand Pump | 01.0 | 1442.0 | Each | 1442 |
| 9 | Providing and fixing water pumping set ½ H.P Mono Blck single phase 220 bolts with 1”x1-1/4” suction and delivery 20 ft head including making c.c 1:3:6 platform of required size and fixing with nuts and bolts (local made). (R.A) | 01.0 | 14417.70 | Each | 14418.0 |
|  |  |  | Total: |  | 36434.0 |
|  |  |  | N.S.I |  | 19673.0 |
|  |  |  | S.I |  | 16761.0 |

**10 % Above /below 3 on the Rates of CSR Amount tobe added/aeduted on**

**Basis of premium quoted Total (b)**

**Total A+B Rs: (a)\_\_\_\_\_\_\_\_\_\_\_\_ Rs: (b)\_\_\_\_\_\_\_\_\_\_\_\_\_ Rs:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**R.CC (a) 10 & Rs:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Total Amount Rs:\_\_\_\_\_\_\_\_\_\_\_\_Fabrication (a) 10 % Above Rs:\_\_\_\_\_\_\_\_\_\_\_\_ Total Amount Rs: \_\_\_\_\_\_\_\_\_\_\_\_**

**Total (A) +b in works & Figure\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**NOTE:- Quantities/Rates can be changed after Technical sanctioned is received from competent authortity.**

**CONTRACTORT EXECUTIVE ENGINEER**

**EDUCATION WORKS DIVISION**

**DADU**

**BILL OF QUANITITY (B.O.Q)**

**PART “B” WATER SUPPLY & S/FITTING**

**NAME OF WORK REPAIR / MAINTENANCE OF GOVT: GIRLS PRIMARY SCHOOL KUMBHAR MUHALLA (COMPOUND WALL & LAV BLOCK) TALUKA & DISTRICT DADU (2016-17) PROG:**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S#** | **ITEM OF WORK** | **QNTY** | **RATE** | **UNIT** | **AMOUNT** |
| 1 | P/F Squatting type white glazed earthen were w.c pan with including the cost of flushing cistern with internal fitting and flush pipe with bend & making requisite number of holes in walls plinth & floor for pipe connections & making good in cement concrete 1:2:4 (S.I.N:1(b)P/1) | 5.0 | 5044.60 | P.No | 25223 |
| 2 | Providing G.I pipe specials & clamps etc including fixing cutting and fitting complete with and i/c the cost of breaking rough wall and roof making good etc painting two coats after cleaning the pipe etc white zink point with pigment to match the colour of building (S.I.NO:1P/12) |  |  |  |  |
|  | 1/2” dia | 80.00 | 73.21 | p.rft | 5856 |
|  | 3/4” dia | 50.00 | 95.89 | p.rft | 4795 |
| 3 | Providing fixing handle valves (china) (S.I:No:5 | 4.00 | 271.92 | P.No | 1088 |
| 5 | S/Fixing long bib-cook of superior quality with c.p head ½” dia (S.I.N.O:13 P/10) | 5.00 | 1109.46 | P.NO | 5547 |
| 6 | S/Fixing concealed tee-stop cock of superior quality with c.p head ½”dia .(S.I.NO: 12(b) P/18) | 5.00 | 889.46 | P.NO | 4447 |
| 7 | Providing R.C.C pipe with collars class “B” and digging the to required depth & fixing in positing i/c cutting fitting & jointing with asphalt composition cement to a head of 4” feet above the top of the heights pipe & refilling excavated staff 6” pipe class “B” |  |  |  |  |
|  | 6” dia | 50.00 | 199.25 | P.rft | 9963 |
|  | 4’’ dia | 30.00 | 146.00 | P.Rft | 4380 |
| 8 | P/F Hand Pump with all accessories wooden shown i/c boring cutting etc. (R.A) |  |  |  |  |
| A | Filter | 10.0 | 76.05 | P.Rft | 761 |
| B | Boring | 80.0 | 38.50 | P.Rft | 3052 |
| C | Hand Pump | 01.0 | 1442.0 | Each | 1442 |
| 9 | Providing and fixing water pumping set ½ H.P Mono Block single phase 220 bolts with 1”x1-1/4” suction and delivery 20 ft head including making c.c 1:3:6 platform of required size and fixing with nuts and bolts (local made). (R.A) | 01.0 | 14417.70 | Each | 14418.0 |
|  |  |  | Total: |  | 80972.0 |
|  |  |  | N.S.I |  | 19673.0 |
|  |  |  | S.I |  | 61299.0 |

**10 % Above /below 3 on the Rates of CSR Amount tobe added/aeduted on**

**Basis of premium quoted Total (b)**

**Total A+B Rs: (a)\_\_\_\_\_\_\_\_\_\_\_\_ Rs: (b)\_\_\_\_\_\_\_\_\_\_\_\_\_ Rs:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**R.CC (a) 10 & Rs:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Total Amount Rs:\_\_\_\_\_\_\_\_\_\_\_\_Fabrication (a) 10 % Above Rs:\_\_\_\_\_\_\_\_\_\_\_\_ Total Amount Rs: \_\_\_\_\_\_\_\_\_\_\_\_**

**Total (A) +b in works & Figure\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**NOTE:- Quantities/Rates can be changed after Technical sanctioned is received from competent authortity.**

**CONTRACTORT EXECUTIVE ENGINEER**

**EDUCATION WORKS DIVISION**

**DADU**

**BILL OF QUANITITY (B.O.Q)**

**PART “B” WATER SUPPLY & S/FITTING**

**NAME OF WORK REPAIR / MAINTENANCE OF GOVT: GIRLS PRIMARY SCHOOL BUTH MUHALLA (COMPOUND WALL & LAV BLOCK) TALUKA & DISTRICT DADU (2016-17) PROG:**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S#** | **ITEM OF WORK** | **QNTY** | **RATE** | **UNIT** | **AMOUNT** |
| 1 | P/F Squatting type white glazed earthen ware w.c pan with including the cost of flushing cistern with internal fitting and flush pipe with bend & making requisite number of holes in walls plinth & floor for pipe connections & making good in cement concrete 1:2:4 (S.I.N:1(b)P/1) | 3.0 | 5044.60 | P.No | 15134 |
| 2 | Providing G.I pipe specials & clamps etc including fixing cutting and fitting complete with and i/c the cost of breaking rough wall and roof making good etc painting two coats after cleaning the pipe etc white zink point with pigment to match the colour of building (S.I.NO:1P/12) |  |  |  |  |
|  | 1/2” dia | 50.00 | 73.21 | p.rft | 3661 |
|  | 3/4” dia | 50.00 | 95.89 | p.rft | 4795 |
| 3 | Providing fixing handle valves (china) (S.I:No:5 | 3.00 | 271.92 | P.No | 815 |
| 4 | S/Fixing long bib-cook of superior quality with c.p head ½” dia (S.I.N.O:13 P/10) | 5.00 | 1109.46 | P.NO | 5547 |
| 5 | S/Fixing concealed tee-stop cock of superior quality with c.p head ½”dia .(S.I.NO: 12(b) P/18) | 3.00 | 889.46 | P.NO | 2668 |
| 6 | Providing R.C.C pipe with collars class “B” and digging the to required depth & fixing in positing i/c cutting fitting & jointing with maxphalt composition cement to a head of 4” feet above the top of the heightest pipe & refilling excavated staff 6” pipe class “B” |  |  |  |  |
|  | 6” dia | 50.00 | 199.25 | P.rft | 9963 |
|  | 4’’ dia | 30.00 | 146.00 | P.Rft | 4380 |
| 7 | P/F Hand Pump with all accessories wooden shown i/c boring cutting etc. (R.A) |  |  |  |  |
| A | Filter | 10.0 | 76.05 | P.Rft | 761 |
| B | Boring | 80.0 | 38.50 | P.Rft | 3052 |
| C | Hand Pump | 1.0 | 1442.0 | Each | 1442 |
| 8 | Providing and fixing water pumping set ½ H.P Mono Blck single phase 220 bolts with 1”x1-1/4” suction and delivery 20 ft head including making c.c 1:3:6 platform of required size and fixing with nuts and bolts (local made). (R.A) | 1.0 | 14417.70 | Each | 14418.0 |
|  |  |  | Total: |  | 66636.0 |
|  |  |  | N.S.I |  | 19673.0 |
|  |  |  | S.I |  | 46963.0 |

**10 % Above /below 3 on the Rates of CSR Amount tobe added/aeduted on**

**Basis of premium quoted Total (b)**

**Total A+B Rs: (a)\_\_\_\_\_\_\_\_\_\_\_\_ Rs: (b)\_\_\_\_\_\_\_\_\_\_\_\_\_ Rs:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**R.CC (a) 10 & Rs:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Total Amount Rs:\_\_\_\_\_\_\_\_\_\_\_\_Fabrication (a) 10 % Above Rs:\_\_\_\_\_\_\_\_\_\_\_\_ Total Amount Rs: \_\_\_\_\_\_\_\_\_\_\_\_**

**Total (A) +b in works & Figure\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**NOTE:- Quantities/Rates can be changed after Technical sanctioned is received from competent authortity.**

**CONTRACTORT EXECUTIVE ENGINEER**

**EDUCATION WORKS DIVISION**

**DADU**