**OFFICE OF THE DIRECTOR PARKS**

**Work 01**

**DISTRICT MUNICIPAL CORPORATION (WEST) KARACHI**

**SUBJECT: - REPAIR AND MAINTENANCE OF BOUNDARY WALL OF PARK KERB**

**STONE NEAR JAM-E-MASJID UC-43, KEAMARI ZONE, DMC (WEST)**

**E/Cost: 9,26,269/-+O/R E/Money 20,000/- T/Limit ­30 Days Penalty 500/- PD.**

**S.No Description of Work Quantity Rate Per%**

1. Excavation in Foundation of building, bridges and

other structures including dagbolling dressing re

ground structure with excavated earth watering and

ramming lead upto 5 feet in ordinary soil. 1904/Cft 3176.25%0Cft

2. Cartage of 100 Cft 5 tons all materials like stone

aggregate spwals lime surkhi BG rail fasting points

crossing bridge guders pipe sheet M/S Brass sheets

1000 trenches 10×5×3" 1000 tiles 12×6×2" 150 cft

timber 100 mould fuel wood by trenches owned by the

contractor withing 10 miles etc comp: 1904/Cft 902.20%Cft

3. P/F Precast edge block 3750 PSI industrial Made Size

6 inches thick X 18” long X 12” high including the

cost of cartage, excavation, from the work for hunching

lean concrete 2250 PSI Concrete for hunching 1:4

cement sand mortar 1904/Rft 297.01/P.Rft

4. Painting on Surface 1904/Sft 1489.68%Sft

5. P/F Fiber Glass 1-9” dust bin dia with M.S Pipe fitting

Moveable as per approved by Office Incharge 06 Nos Open Rate

6. Stucco Cement Plaster 1:2:4 (Cement stand and Shingle) 7400/Sft 4178.02%Sft

**DIRECTOR PARKS**

**DMC (WEST) KARACHI**

**I / we hereby quoted \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Above / Below the SR.**

**Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**OFFICE OF THE DIRECTOR PARKS**

**Work 02**

**DISTRICT MUNICIPAL CORPORATION (WEST) KARACHI**

**SUBJECT: - IMPROVEMENT OF PARK NEAR KPT QUARTER UC-43, KEAMARI**

**ZONE DMC (WEST)**

**E/Cost: 3,16,368/-+O/R E/Money 20,000/- T/Limit ­30 Days Penalty 500/- PD.**

**S.No Description of Work Quantity Rate Per%**

1. Filling watering and riming earth under floor new earth

(Excavated) from out side lead up to one chain and

lift up to 5ft. 14250/Cft Open Rate

2. ¾" thick cement plaster 1:4 upto 20' height. 7400/Sft 2283.93%Sft

3. Supplying stacking and spreading murrum from

app: quarries to required slop i/c consolidation by famig

and watering etc complete. 2657/Cft Open Rate

4. Making and fixing steel grated door complete with

1 / 16” thick sheeting including angle iron frames

2”×2”×3/8” and ¾” Square bar 1" center to center with

locking arrangement 192/Sft 726.72%Sft

5. Painting Doors & Windows any type 192/Sft 1160.06%Sft

6. P/F 4 Seated white or coloured light shade marble

mosaic benches (5½×3'×2') with back of app: design &

drawing in white cement i/c cartage loading and

unloading etc complete. 15Nos Open Rate

7. P/F piston pump in set 1 H.P single phase 220 volts

with 1¼×1¼ suction and delivery (Local made). 01 No Open Rate

8. P/L PVC Pipe 1”dia i/c cutting fitting fixing etc complete 200/Rft 28/P.Rft

9. Rubber Pipe best quality 1”dia 150/Rft Open Rate

10. Valve (local) China i/c cutting of pipr fitting in trench 08 Nos 365.42/Each

11. P/F mono Block Pumping set 1 H.P Single Phase 220

Volts with ¼ x 1-4” section and other delivery i/c other

fitting (local Made) 01 No Open Rate

**DIRECTOR PARKS**

**DMC (WEST) KARACHI**

**I / we hereby quoted \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Above / Below the SR.**

**Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**OFFICE OF THE DIRECTOR PARKS**

**Work 03**

**DISTRICT MUNICIPAL CORPORATION (WEST) KARACHI**

**SUBJECT: - S/ STACKING SWEET EARTH AND MANURE AT PARK ADJACENT**

**TO TOHEED MASJID IN UC-43 KEAMARI ZONE DMC (WEST)**

**E/Cost: Open Rate E/Money 20,000/- T/Limit ­30 Days Penalty 500/- PD.**

**S.No Description of Work Quantity Rate Per%**

1. Supplying stacking and spreading app: garden soil

(S/Earth) free from salt and grass roots etc i/c all lead

and lift. 13899/Cft Open Rate

2. Supplying stacking and spreading wall decayed cow

dung manure from app: source i/c all lead and lift. 4408/Cft Open Rate

3. Supply Line (Dacca) grass in slab with earth intact i/c

all lead and lift. 26568/Sft Open Rate

**DIRECTOR PARKS**

**DMC (WEST) KARACHI**

**I / we hereby quoted \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Above / Below the SR.**

**Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**OFFICE OF THE DIRECTOR PARKS**

**Work 04**

**DISTRICT MUNICIPAL CORPORATION (WEST) KARACHI**

**SUBJECT: - P/F PHYSICAL APPLIANCES AND BENCHES AND BEAUTIFICATION**

**OF LAWN OF PARK NEAR TO GOVT. SCHOOL KEAMARI ZONE**

**DMC (WEST)**

**E/Cost: 3,28,690/-+O/R E/Money 20,000/- T/Limit ­30 Days Penalty 500/- PD.**

**S.No Description of Work Quantity Rate Per%**

1. Excavation in Foundation of building, bridges and

other structures including dagbolling dressing re

ground structure with excavated earth watering and

ramming lead upto 5 feet in ordinary soil. 600/Cft 3176.25%0Cft

2. Cartage of 100 Cft 5 tons all materials like stone

aggregate spwals lime surkhi BG rail fasting points

crossing bridge guders pipe sheet M/S Brass sheets

1000 trenches 10×5×3" 1000 tiles 12×6×2" 150 cft

timber 100 mould fuel wood by trenches owned by the

contractor withing 10 miles etc comp: 600/Cft 902.20%Cft

3. P/L 1:4:8 plain i/c placing compacting finishing

curing etc comp: 396/Cft 9416.28%Cft

4. P/L Pavers Colored (Rockrete) Glazed on Floor Facing

in required colored and pattern of stile specification

jointed in white cement and pigment over a base of 1:2

grey cement mortars ¾ thick including washing and

filling of joints 1200/Sft 223.97/P.Sft

5. P/F Slide out fit covered with G.P sheet as per app:

drawing size 2” dia pipe 14g 25’ rft support 1 ¼ dia

pipe 14 g1’ Sft feet 1’ feet 1 ¼ dia pipe 14g 02 Nos Open Rate

6. P/F Seesaw as per app: drawing size pipe 3"dia 14g

7' long 2 seats. 02Nos Open Rate

7. P/F merry –go-round center pipe 4'' dia (100.mm)

angle iron and wooden plod covered with m-s sheet

etc as per app: drawing. 02Nos Open Rate

8. P/F Swing type as per app: drawing size pipe 2"dia

14g 50 cob 8' long 2 seat. 02 Nos Open Rate

9. Grass Cutting Machine Hand 01 No Open Rate

10. P/F Name Plate G.I Sheet 12’ 1.5’ with angle iron

frame necessary welding & Color embedded instruction

of Engineer Incharge 01 Job Open Rate

11. P/L 1:3:6 CC Solid black Masonry wall 6" & below in

thickness set in 1:6 comate motor in ground flour

complete. 45/Cft 15771.01%Cft

12. ¾" thick cement plaster 1:4 upto 20' height. 360/Sft 2283.93%Sft

13. Supply of Coconut Tree 35 Nos Open Rate

14. Supply of Mix Shrub Plants 200 Nos Open Rate

**DIRECTOR PARKS**

**DMC (WEST) KARACHI**

**I / we hereby quoted \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Above / Below the SR.**

**Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**OFFICE OF THE EXECUTIVE ENGINEER**

**Work 05**

**DMC WEST KARACHI**

**SUBJECT: - PROVIDING / FIXING OF LED LIGHTS & SON LIGHTS IN**

**IMPROVEMENTS & R/M WORK OF STREET LIGHTS SYSTEM**

**DMC (WEST)**

**E/Cost: 9,98,150/- E/Money 20,000/- T/Limit 45 Days Penalty 500/- PD.**

**S.No Description of Work Quantity Rate Per%**

1. Providing / Fixing of LED Light 30 W Best as required 140 Nos 2500/-

2. P/F of Rod 250W Son T Philips equivalent make as

required 110 Nos 2100/-

3. P/F of Choke 250 W Son T Philips equivalent make as

required 85 Nos 3990/-

4. P/F of Capacitor 250 35uf Philips / equivalent make as

required 60 Nos 600/-

5. P/F of Igniter SN-58 Philips equivalent make as required 70 Nos 600/-

**EXECUTIVE ENGINEER (M&E)**

**DMC (WEST)**

**I / we hereby quoted \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Above / Below the SR.**

**Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**OFFICE OF THE EXECUTIVE ENGINEER**

**Work 06**

**DMC WEST KARACHI**

**SUBJECT: - PROVIDING / FIXING OF LED LIGHTS & SON LIGHTS IN**

**IMPROVEMENTS & R/M WORK OF STREET LIGHTS SYSTEM**

**DMC (WEST)**

**E/Cost: 9,97,500/- E/Money 20,000/- T/Limit 45 Days Penalty 500/- PD.**

**S.No Description of Work Quantity Rate Per%**

1. Providing / Fixing of LED Light 30 W Best as required 192 Nos 2500/-

2. P/F of Rod 250W Son T Philips equivalent make as

required 50 Nos 1700/-

3. P/F of Choke 150 W Son T Philips equivalent make as

required 30 Nos 3150/-

4. P/F of Capacitor 250 35uf Philips / equivalent make as

required 90 Nos 600/-

5. P/F of Igniter SN-58 Philips equivalent make as required 60 Nos 600/-

6. Providing / Laying of 3/.029 Wire Single Core Million

Supreme as rquired 30 Coil 2400/-

7. Providing / Laying of 7/.029 Wire Single Core Million

Supreme as rquired 15 Coil 2800/-

8. Providing / Laying of 7/.036 Two Core for lighting

main connection 05 Coil 16500/-

9. P’/F of Porcelain thread holder 250w best quality

as required 85 Nos 200/-

10. P/F of Open Switch 10 Amp best quality as required 400 Nos 40/-

11. P/F of Acyrelic cover 250w make as required 20 Nos 700/-

12. P/F of PVC Nitto Tape Best Quality as required 100 Nos 45/-

**EXECUTIVE ENGINEER (M&E)**

**DMC (WEST)**

**I / we hereby quoted \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Above / Below the SR.**

**Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**