***SCHEDULE OF QUANTITIES***

***WORK No: 11***

# 

**DISTRICT MUNICIPAL CORPORATION (WEST)**

**KARACHI, BALDIA ZONE**

***Estimated Cost Rs: 9,90,847/- Earnest Money Rs: 19,817/-***

***Time Limit: 45 Days Penalty Per Day Rs: 1,000/-***

**SUBJECT: *Improvement of R.C.C Culvert at Mahboob Shah Chowk in UC-35 DMC (West)***

***Baldia Zone.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ***S.No:*** | ***DESCRIPTION OF WORK*** | ***QUANTITY*** | ***RATE*** | ***PER*** | ***AMOUNT*** |
| *1.* | *Dismantling cement rain for Separating reinforced cement form concrete cleaning and straightening 1ft same.* | *210* | *5445* | *%Cft* | *11434/-* |
| *2.* | *Stone Pitching for tep layer only (1:3 to 1:5) thick (b) in bed.* | *1050* | *1996.50* | *%Cft* | *20963/-* |
| *3.* | *P/L Cement concrete brick or Stone ballast 1 ½” to 2” gauge 1:4:8.* | *350* | *9416.28* | *%Cft* | *32957/-* |
| *4.* | *Erection of Removal shattering coat RCC or plain cement concrete work of portal wood vertical.* | *2200* | *3127.41* | *%Sft* | *68803/-* |
| *5.* | *Cement concrete plain including placing compacting finishing and curing complete including screening and washing at stone aggregate without 1:2:4.* | *1100* | *14429.25* | *%Cft* | *158722/-* |
| *6.* | *RCC Work in Roof slab beans columns raft lintels and other structured member laid in situ or precast laid in position complete in all respects. Ratio (1:2:4) go Ibs cement 2Cft Sand Cft Shingle 1/8” to ¼” gauge.* | *350* | *337* | *%Cft* | *117950/-* |
| *7.* | *Fabrication at mold steel reinforcement cement concrete i/c cutting binding laying in position making joints and fastening i/c cast of bending wire also i/c removal rust from bars,* | *10.93* | *5001.70* | *P/Cwt* | *150701/-* |
| *8.* | *Carriage of 100 Cft tons at all kind material like cole brikes i/c.* | *210* | *1065.08* | *%Cft* | *2237/-* |
| *9.* | *Hire charges of pumping set of upto 10 H.P (But not less than 5 H.P) Pumping out water from 20ft. deep trench.* | *05* | *1500* | *P-Day* | *7500/-* |
| *10.* | *Hiring of Private labour Per-Day.* | *330* | *900* | *Nos* | *297000/-* |
| *11.* | *Hiring of Machinery front Loader / Excavator P-Hour.* | *24* | *3088.13* | *P-Hour* | *74115/-* |
| *12.* | *Hiring of Machinery Dumper Per Hour.* | *72* | *2006.90* | *P-Hour* | *144497* |
| ***Total Estimated Cost*** | | | | | ***9,90,847.00*** |

*Nomenclature, Quantities and Rates etc checked*

*and found correct.*

***ASSTT: EX-ENGINEER (B&R) EXECUTIVE ENGINEER (B&R)***

*BALDIA ZONE BALDIA ZONE*

*I/We hereby quoted Rates @ % above/below the S/R*

*The total amount is Rs: (Rupees:*

*(In Figure) (In Word)*

## *Contractor’s Signature:*

## 

## *Address:*