***SCHEDULE “B”***

**NAME OF WORK: - ESTABLISHMENT OF JAM MUMTAZ HUSSAIN DAHAR GOVT: BOYS DEGREE COLLEGE UBAURO EXTERNAL DEVELOPMENT (CONSTRUCTION OF ROADS AND PATHS I/C RAISING OF C/WALL) TALUKA UBAURO.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S. No:** | **Item of Work** | **Qty:** | **Rate** | **Unit** | **Amount** |
|  |  |  |  |  |  |
| 1 | Excavation in foundation of Building Bridges and other structures including dagbelling dressing, refilling around structure with excavated earth Watering and ramming lead upto 5 ft In ordinary soil (S. I No: 18 (b) P. No: 4). | | | | |
|  |  | 10543 | @ 3176/25 | %0Cft | 33487/- |
| 2 | Cement concrete brick or stone ballast 1 1/2" to 2" gauge Ratio 1 : 5 : 10 (S. I 4 (c) P. No: 15). | | | | |
|  |  | 10140 | @ 8694/95 | %Cft | 881668/- |
| 3 | Pacca brick work in foundation and plinth in Cement sand mortar 1:6 (S. I No: 4 (e) P. No: 21). | | | | |
|  |  | 9000 | @ 11948/36 | %Cft | 1075352/- |
| 4 | Filling, watering and ramming earth under floor with new earth (Excavated from outside) lead upto one chain and lift upto 5 feet (S. I No: 22 P. No: 4). | | | | |
|  |  | 302530 | @ 3630/- | %0Cft | 1098184/- |
| 5 | Supplying and filling sand under floor and plugging in walls (S. I No: 29 P. No: 26). | | | | |
|  |  | 11116 | @ 1141/25 | %Cft | 126861/- |
| 6 | Add Extra lead 03 miles. | | | | |
|  |  | 313646 | @ 579/41 | %Cft | 181729/- |
| 7 | Dismantling brick work in lime or cement mortar (S. I No: 13 P. No: 10). | | | | |
|  |  | 746 | @ 1285/63 | %Cft | 9591/- |
| 8 | Removing cement or lime plaster (S. I No: 53 P. No: 13). | | | | |
|  |  | 2000 | @ 121/- | %Sft | 2420/- |
| 9 | Pacca brick work other than building including striking of joints upto 20 feet height in Cement sand mortar 1:6 (S. I No: 7 I (e) P. No: 22). | | | | |
|  |  | 5841 | @ 12346/65 | %Cft | 721168/- |
| 10 | Cement plaster 1:6 upto 12' height 1/2" thick (S.I No: 13 (b) P. No: 52). | | | | |
|  |  | 30598 | @ 2206/60 | %Sft | 675175/- |
| 11 | Cement plaster 1:4 upto 12' height 3/8" thick (S.I No: 11 (a) P. No: 52). | | | | |
|  |  | 30598 | @ 2197/52 | %Sft | 672397/- |
| 12 | Providing and laying 1" thick topping cement concrete (1:2:4 ) including Surface finishing and dividing into panels 3" thick (S. I No: 16 (d) P. No: 42). | | | | |
|  |  | 4671 | @ 4411/82 | %Sft | 206076/- |
| 13 | Providing & fixing cement paving blocks flooring having size of 197 x 97 x 60 (mm) of city / quddra / cobble shape with pigmented, having strength b/w 5000 psi to 8500 psi I/c filling the joints with hill sand and laying in specified manner/ pattern and design etc: complete (S. I No: 72 P. No: 49). | | | | |
|  |  | 19555 | @ 223/97 | P.Sft | 4379733/- |
| 14 | Cumb Stone | | | | |
|  |  | 1760 | @ 297/01 | P.Sft | 522738/- |
| 15 | Colour washing Two coats (S. I No: 25 (b) P. No: 54). | | | | |
|  |  | 68238 | @ 859/90 | %Sft | 586779/- |
| 16 | Two coats of bitumen laid hot using 34 Lbs for % Sft. Ober roof and blinded with sand at one Cft. Per % Sft. (S. I No: 13 P. No: 35). | | | | |
|  |  | 20613 | @ 1887/40 | %Sft | 389050/- |
| 17 | S/F steel stair railly | | | | |
|  |  | 129 | @ 1550/- | P.Rft | 199950/- |
|  |  |  |  |  |  |
|  |  |  |  | **Total** | **13397925/-** |

\_\_\_\_\_\_\_\_% above/below on the rates of CSR.

**CONTRACTOR**

### EXECUTIVE ENGINEER

**EDUCATION WORKS DIVISION**

**GHOTKI**