**GOVERNMENT OF SINDH  
DIRECTORATE OF SINDH ARCHIVES  
INFORMATION & ARCHIVES DEPARTMENT  
GOVERNMENT OF SINDH**

|  |  |
| --- | --- |
| 1. Tender No. | INF-KRY:No.0786/17 |
| 1. Name & Address of Bidder | **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_** |
| 1. Indenters Name and Address | **PROJECT DIRECTOR**  SINDH ARCHIVES KARACHI  INFORMATION & ARCHIVES DEPARTMENT  GOVERNMENT OF SINDH – KARACHI |
| 1. Tender Terms and Conditions | **The following documents should be submitted with the Bid.**  **Company Profile, Literature of the items,**  **Samples of the material and as per further terms and conditions of this tender, DIS-12-14, Sindh Purchase Manual & Other relevant laws in force** |
| 1. Particulars of the stores | As below: |

**6.** Particulars of the stores

|  |  |  |  |
| --- | --- | --- | --- |
| **SERIAL#** | **Description of Stores** | **Rate per item** | |
| **In Figure** | **In Words** |
|  | **CONSERVATION EQUIPMENTS , EQUIPMENT ACCESSORIES, HARDWARE & SOFTWARE** | | |
| **1** | **AIR CONTROLLED PAPER BLOWER Qty. 01** **Specifications:**   * Imported type * Digitally air controlled O to 500 BTI * Air Pressure and Temperature 0 to 150 C * Highly perception needed. | Each | Each |
| **2** | **ARCHIVAL PRECESSION CUTTER MACHINE Qty. 01**  **Specifications:**   * Imported type * 432mm loprat knife * 535mm Height with 220V | Each | Each |
| **3** | **ARCHIVAL STUIVER Qty. 04 Specifications:**   * Thermo controlled * Imported Brand | Each | Each |
| **4** | **ARCHIVAL STORIO Qty.06**  **Specifications:**   * + - * 110mm x 125mm       * Made of Archival Metal | Each | Each |
| **5** | **ARCHIVAL COBOLLO Qty. 05** **Specifications:**   * + - * Made of special Archival Plastic * Imported type | Each | Each |
| **6** | **ARCHIVAL JAPANESE SET OF SKRAMUSHES Qty. 01**  **Specifications:**   * + - * Made of Special Wood * Imported Brand * Lengths of 10cm, 12cm, 14cm | Each | Each |
| **7** | **ARCHIVAL DECRATIVE TOOLS AND SET OF WORD**  **Qty. 01**  **Specifications:**   * + - * Made of Special Archival Metal * Length 125cm x width 135cm * Neutralized in Melkatoze * Hard in 550 Bar Pressure * Processed in Auto Catrologe Machine | Each | Each |
| **8** | **ARCHIVAL BARCODE CONTROLLER Qty. 01**  **Specifications:**   * + - * Install Software EP-1245-PDT/X-10 * Auto Eltrofil Device | Each | Each |
| **9** | **a.c sPLIT UNITS Qty. 08**  **Specifications:**   * 18000 Btu/H (British Thermal Unit/Hour) – Cooling Capacity * Rated Frequency 50 Hz * Rated Voltage 220-240 Volts * Air Flow Rate 850 M3/H * Sound Pressure Level 44db(A) * Climate Type T1 * Refrigerant R22 * Cooling Power Input 1900w * Wireless Remote Control | Each | Each |
| **10** | **BRANDED SYSTEM CORE i7 Qty. 06**  **Specifications:**   * + - * Branded * Latest generation * HP * Tower | Each | Each |
| **11** | **CALIFO PLEXA Qty. 01**  **Specifications:**   * + - * Imported type * 220V * Base Made of Special Archival Material * Temperature Changeable | Each | Each |
| **12** | **COMPUTER (CORE i3) Qty. 03**  **Specifications:**   * + - * Brand Hp       * Core-I3 | Each | Each |
| **13** | **cuteau atemt Qty. 01**  **Specifications:**   * + - * Made of Imported type * Made of Archival Rubber * Length 254 x Width 381MM | Each | Each |
| **14** | **DIGITAL ACCESS SYSTEM Qty. Lump Sum**  **Specifications:**   * + - * Imported Brand | Each | Each |
| **15** | **dacoretifs leaux Qty. 01**  **Specifications:**   * + - * Made of Imported * Archival Grade Metal * Handle 325MM x Base 425MM | Each | Each |
| **16** | **fumigatiion chamber Qty. 01**  **Specifications:**   * + - * Size Overall dimensions 54” x 60” x 102”       * Chamber Size: Outer 34” x 46” x 102”       * Inner 30” x 42” x 98”       * Carrying Trolleys: 3 Trolleys each consisting of a size 30” x 31” x 36” basket mounted.       * On carriage frame, basket made of Non Reactive Meter wire. Caring frame shall be plastic coated.       * Trolley caring capacity is 200 Kg.       * Fittings: * Vertical is fitted for outlet of the poisonous gasses. * Vacuum pump is install to create vacuum in the chamber. * Gas making chamber is dual control system by chemical reaction and also by electronically heating system. * Vacuum gage is use to cheek the vacuum inside the chamber during operation. * Light is installed inside the chamber to see the vision during operation. * Panel board for controlling all electrically operated fittings. | Each | Each |
| **17** | **fire extinguisher with wall bracket Qty. 08**  **Specifications:**   * 5 Kg * Working Temperature -10 Degree Celsius To * - / + 55 Degree Celsius * Fire Rating 5-B : C * Built-In Pressure Gauge * Pressure Gauge For Added Reassurance * Co2 Type * FDA / CE Approved * Wall-Bracket * Is 9001 Standard * EU Approved Brand | Each | Each |
| **18** | **humidifier Qty. 01**  **Specifications:**   * + - * Imported * Temp Maintained: 15C | Each | Each |
| **19** | **hygrometer Qty. 02**  **Specifications:**   * + - * Imported type       * Precession 0.002 to 5.900 | Each | Each |
| **20** | **hand scanner Qty. 01**  **Specifications:**   * + - * Imported type       * Resolution 660dpm | Each | Each |
| **21** | **liquets prase Qty. 01**  **Specifications:**   * + - * Made of Iron       * Pressure Maintain 50-KG-70KG       * Motorized | Each | Each |
| **22** | **lagano resa ratura Qty. 01**  **Specifications:**   * + - * Made of Archival Wood       * Spiral Handle | Each | Each |

|  |  |  |  |
| --- | --- | --- | --- |
| **23** | **livre ablet prase Qty. 01**  **Specifications:**   * + - * Made of Iron Casting       * Pressure of 30-40Kg       * Manual Operate | Each | Each |
| **24** | **legator pasle Qty. 01**  **Specifications:**   * + - * L 23MM X W 45MM X H 34MM       * Imported type | Each | Each |
| **25** | **mono color lesser printer Qty. 09**  **Specifications:**   * + - * Imported type * HP | Each | Each |
| **26** | **motorized hard bed press Qty. 01**  **Specifications:**   * + - * Made of Iron Cast       * 220V       * 25hp Imported Lamter Motor | Each | Each |
| **27** | **mertolo saporto Qty. 01**  **Specifications:**   * + - * Imported type       * Handle 355mm       * Base 155mm | Each | Each |
| **28** | **nas (iscsi) fabric s-controllers asic sdn**  **Qty. Lump Sum**  **Specifications:**   * + - * Imported Branded | Each | Each |
| **29** | **Oupe ApTIS Qty. 01**  **Specifications:**   * + - * L 658mm x W 588mm       * Sap Made       * Imported type | Each | Each |
| **30** | **PH ANALYSIS GRAFE Qty. 03**  **Specifications:**   * + - * Imported type       * Data Maintain of 14-days | Each | Each |
| **31** | **PAPER FRESA Qty. 01**  **Specifications:**   * + - * Imported type       * Stainless Steel Sharp Blade       * 658mm x 168mm | Each | Each |
| **32** | **SET OF ASFE VIRE Qty. 01**  **Specifications:**   * + - * Imported type       * Made of S.S       * 5mm thin | Each | Each |
| **33** | **SET OF RAGEL FLESIBLE Qty. 01**  **Specifications:**   * + - * Imported type       * Length 304mm       * Plastic Made | Each | Each |
| **34** | **TOOLS KIT Qty. 01**  **Specifications:**   * + - * Imported type       * Archival Misc Tools | Each | Each |
| **35** | **VARPUMATE DEVICE Qty. 01**  **Specifications:**   * + - * Imported type       * Sensor Control Handle       * Precession 0.01 to 0.10 | Each | Each |
| **36** | **U.P.S Qty. 03**  **Specifications:**   * Imported type * BACKUP 30 MINUTES | Each | Each |
| **37** | **WATER DISPENSER Qty. 08**  **Specifications:**   * Imported type | Each | Each |
| **38** | **DONGLE Qty. 06**  **Specifications:**   * Imported type | Each | Each |
| **39** | **ROUTER Qty. 01**  **Specifications:**   * Imported type | Each | Each |
| **40** | **FLASH DRIVE Qty. 06**  **Specifications:**   * Imported type | Each | Each |
| **41** | **UPS Qty. 03**  **Specifications:**   * Imported type | Each | Each |
| **42** | **PASSPORT DRIVE Qty. 01**  **Specifications:**   * Imported type | Each | Each |

Delivery Time: a) 04 weeks for local articles  
 b) 12-14 weeks for import products

1. Place of Delivery: Sindh Archives Complex,  
    ST. No. 26-A, Block-5, Main Clifton – Karachi
2. Dispatch Instructions: Stores should be delivered free of  
    transportation charges to the consignee at  
    place mentioned above.
3. Inspection Authority: The Procurement Committee constituted by the  
    Secretary, Information & Archives Dept.
4. Place at which stores to be inspected: Sindh Archives Complex,  
    ST. No. 26-A, Block-5, Main Clifton – Karachi
5. Payment: i. Part payment against part supply is  
    allowed.

ii. 100% payment to be made on the proof  
of inspection & consignee’s receipt  
certificate by Accountant General – Sindh, Karachi, during the fiscal   
year 2017-18.

iii. Less 0.25% as service charges and 0.20% stamp duty of the value of the contract by Accountant General Sindh – Karachi, while making payment to the contractor.

**DEPUTY DIRECTOR   
 SINDH ARCHIVES - KARACHI**