SCHEDULE-B **GRADATION OF SINDH GOVERNENT PRINTING PRESS @ KHAIRPUR ((Managers Bungalow)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO | ITEM OF WORK | |  | QTY |  | RATE | UNIT | AMOUNT |
|  |  |  |  |  |  |  |  |  |
| 01/- | Dismantling brick work in lime or cement mortar.(S.I NO: 13 P.NO:4 ) | | | | | |  |  |
|  |  |  | = | 2115 | “ | 1285.63 | % Cft | 27191/- |
|  |  |  |  |  |  |  |  |  |
| 02/- | Excavation in foundation of Building Bridges and other structures including dag belling dressing, refilling around structure with excavated earth Watering and ramming lead upto 5 ft.(S.I NO: 18 P.NO: 4) | | | | | |  |  |
|  |  |  | = | 1937 | “ | 3176.25 | %0Cft | 6152/- |
|  |  |  |  |  |  |  |  |  |
| 03/- | Cement concrete stone of brick ballast 1½” to 2” gauge. Ratio (1:5:10). (S.I.No.4 (b) P.No.17) | | | | |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 388 | “ | 8694.95 | % Cft | 33736/- |
|  |  |  |  |  |  |  |  |  |
| 04/- | Random, rubble masonry (un-coursed )Ratio 1:6 (S.I NO: 1 (iv)P.NO: 27) | | | | | |  |  |
|  |  |  | = | 1258 | “ | 17723/- | % Cft | 222955/- |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 05/- | Pacca brick work in foundation and plinth in:(e) Cement sand mortar 1:6(S.I NO: 4 (e)P: NO: 20) | | | | | | | | | | | | |  |  |
|  |  | |  | | = | | 1195 | | | “ | | 11948.36 | | % Cft | 142783/- |
|  |  | |  | |  | |  | | |  | |  | |  |  |
| 06/- | Fabrication of mild steel reinforcement for cement concrete including cutting, bending, laying in position, making joints and fastenings including cost of binding wire (also includes removal of rust from bars.)(S.I NO: 8 P.NO: 17) | | | | | | | | | | | | |  |  |
|  |  | | Net: Qty: 3326.486/112 | | = | | 29.70 | | | cwt | | 5001.70 | | P.cwt | 148550/- |
|  |  | |  | |  | |  | | |  | |  | |  |  |
| 07/- | | R.C.C work in roof slab, beams columns rafts, lintels and other structural members laid in situ or precast laid in position complete in all respects. Ratio (1 : 2: 4 ) 90 Lbs. cement 2 Cft. Sand 4 Cft. Shingle 1/8" to 1/4" gauge.(S.I NO: 6 (a)P-16) | | | | | | | | |  | |  | |  |
|  | |  | |  | | = | | 733 | “ | | 337/- | | P.Cft | | 247021/- |
|  | |  | |  | |  | |  |  | |  | |  | |  |
| 08/- | | Supplying & Filling Sand under floor plugging into walls (S.I NO: P.NO: ) | | | | | | | | | | |  | |  |
|  | |  | |  | | = | | 4102 | “ | | 1913.21 | | % Cft | | 78480/- |
|  | |  | |  | |  | |  |  | |  | |  | |  |
| 09/- | | Cement concrete stone of brick ballast 1½” to 2” gauge. Ratio (1:5:10). (S.I.No.4 (b) P.No.17) | | | | | | | | | | |  | |  |
|  | |  | |  | | = | | 451 | Cft | | 8122.95 | | % Cft | | 36635/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO | ITEM OF WORK |  | QTY |  | RATE | UNIT | AMOUNT |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 10 | Pacca Brick work in Ground Floor in cement sand mortar (S.I NO: P.NO: ) | | | | | |  |  |
|  |  |  | = | 2535 | Cft | 12674.36 | % Cft | 321295/- |
|  |  |  |  |  |  |  |  |  |
| 11/- | Providing and fixing G.I frames /Choukhats of size 7" x 2" or 4 1/2" x 3" for door using 20 gauge G.I sheet I/c welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage , tools and plants used in making and fixing.(CSI NO: 29 P-93) | | | | | |  |  |
|  |  |  | = | 169 | “ | 228.90 | P.Rft | 38684/- |
|  |  |  |  |  |  |  |  |  |
| 12/- | Providing and fixing G.I frames /Choukhats of size 7" x 2" or 4 1/2" x 3" for windows using 20 gauge G.I sheet I/c welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage , tools and plants used in making and fixing.(CSI NO: 28 P-93) | | | | | |  |  |
|  |  |  | = | 70 | Rft | 240.5 | P.Rft | 16835/- |
| 13/- | First class deodar wood wrought, joinery in doors and windows etc, fixxed in position including chowkats hold fasts hinges, iron tower bolts, chocks cleats, handles and cords with hooks, etc.(1 3/4" thick)(S.I NO: 7 P-58) | | | | | |  |  |
|  |  |  | = | 203 | “ | 902.93 | P.Sft | 183295/- |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 14/- | Supplying & Fixing R.S Girder (Material Schedule) | | | | | | | | | | |  | |  |
|  |  |  | | = | | 45.214 | | cwt | | 3850/- | | P.cwt | | 174074/- |
| 15/- | Supplying & Fixing R.S T-Iron (Material Schedule) | | | | | | | | | | |  | |  |
|  |  |  | | = | | 24.169 | | cwt | | 3575/- | | P.cwt | | 86404/- |
|  |  |  | |  | |  | |  | |  | |  | |  |
| 16/- | Second class tile roofing consisting of 4" earth and 1" mud plaster with Gobri leeping over 1/2"thick cement plaster 1:6 with 34 Lbs. Of hot bitumen coating sand blinded, provided over one layer of 12" x 6"x2" tiles laid in 1:6 cement mortar including 1:2 cement pointing under neath of tiles complete including curing etc.(S.I NO: 2 P-33) | | | | | | | | | | | | |  |
|  |  |  | | = | | 1148 | | “ | | 7607.25 | | % Sft | | 87331/- |
| 17/- | Supplying & fixing in position iron/steel grill of 3/4" x 1/4" size flat iron of approved design including painting 3 coats etc. complete (weight not to be less than 3.7 Lbs./Sq . Foot of finished grill).(S.I NO: 26 P-93) | | | | | | | | | | | | |  |
|  |  |  | |  | |  | |  | |  | |  | |  |
|  |  |  | | = | | 80 | | “ | | 180.50 | | P.Sft | | 14440/- |
| 18/- | Cement plaster 1:6 upto 12' height.(b) 1/2" thick. (S.I NO: 13 P-52) | | | | | | | | | | | | |  |
|  |  |  | = | | 6166 | | Sft | | 2206.60 | | % Sft | | 136059/- | |
|  |  |  |  | |  | |  | |  | |  | |  | |
| 19/- | Cement plaster 1:4 upto 12' height. 3/4 thick. (S.I NO: 13 P-52) | | | | | | | | | | | |  | |
|  |  |  | = | | 6166 | | “ | | 2197.52 | | % SFt | | 135499/- | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO | | ITEM OF WORK | |  | | QTY | |  | | RATE | | | UNIT | | | AMOUNT | |
| 20/- | Cement concrete plain including placing compacting, finishing and curing, complete (including screening and washing at stone aggregate without shuttering. (S.I NO: 5 (i)P-16) Ratio 1:2:4 | | | | | | | | | | | | | | |  | |
|  |  | |  | |  | |  | |  | |  | | |  | |  | |
|  |  | |  | | = | | 223 | | “ | | 14429.25 | | | % Cft | | 32177/- | |
|  |  | |  | |  | |  | |  | |  | | |  | |  | |
| 21/- | Providing and laying tiles glazed 6" x 6" x 1/4" on floor or wall facing in required colour and a pattern of STILE specification jointed in white cement and pigment over a base of 1:2 grey cement mortar 3/4" thick including washing and filling of joints with slurry of white cement and pigment in desired shape with finishing, clearing and cost of wax polish etc. complete including cutting tiles to proper profile.(S.I NO: 60 P-47) | | | | | | | | | | | | | | |  | |
|  |  | |  | | = | | 954 | | “ | | 30509.77 | | | % Sft | | 291063/- | |
|  |  | |  | |  | |  | |  | |  | | |  | |  | |
| 22/- | Laying floor of approved with glazed tile 1/4" thick in white cement 1:2 over 3/4" thick cement mortar 1:2 complete.(S.I NO: 24 P.NO: 43) | | | | | | | | | | | | | | | |  |
|  |  | |  | |  | |  | |  | | |  | | |  | |  |
|  |  | |  | | = | | 232 | | “ | | | 27678.86 | | | % Sft | | 64215/- |
|  |  | |  | |  | |  | |  | | |  | | |  | |  |
| 23/- | White glazed tiles 1/4" thick dado jointed in white cement and laid over 1:2 cement sand mortar 3/4" thick including finishing.(S.I NO: 37 P.NO: 45) | | | | | | | | | | | | | | | |  |
|  |  | |  | | = | | 487 | | sft | | | 28253.61 | | | % Sft | | 137595/- |
|  |  | |  | |  | |  | |  | | |  | | |  | |  |
| 24/- | Laying white marble flooring fine dressed on the surface without winding set in lime mortar 1:2 including rubbing and polishing of the joints.(S.I NO: 28 P.NO: 43) | | | | | | | | | | | | | |  | |  |
|  |  | |  | | = | | 240 | | “ | | | 567.48 | | | P.Sft | | 136188/- |
|  |  | |  | |  | |  | |  | | |  | | |  | |  |
| 25/- | Reinforced cement concrete spout including fixing in position with top and bottom khuras(S.I NO: 27 P-19) | | | | | | | | | | | | | |  | |  |
|  |  | |  | | = | | 05 | | “ | | | 524.95 | | | each | | 2625/- |
| 26/- | Making & fixing steel grated doors complete with locking arrangement angle iron frame 2" x 2" 3/8"and 3/4" sq: bars 4" centre to centr.(S.I NO: 23 P-92) | | | | | | | | | | | | | |  | |  |
|  |  | |  | | = | | 28 | | “ | | | 594.57 | | | P.Sft | | 16648/- |
|  |  | |  | |  | |  | |  | | |  | | |  | |  |
| 27/- | Supplying and fixing false cailing of plaster of paris, in pannels including making frame , work of Deodar wood including painting with Soligia paint. (S.I NO: 52 P-64) | | | | | | | | | | | | | |  | |  |
|  |  | |  | | = | | 672 | | “ | | | 25293.42 | | | % Sft | | 169972/- |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 28/- | Providing & fixing plaster of Paris ceiling border of 8" -10 " with of specified design & thickness I/c fixing besides ceiling with nails/ screws with jetties.(S.I NO: 44 P-39) | | | | | |  |  |
|  |  |  | = | 208 | “ | 104.22 | P.Rft | 21678/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO | ITEM OF WORK |  | QTY |  | RATE | UNIT | AMOUNT |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 29/- | Galvanized wire gauze fixed to chowkats with 3/4" deodar stips and screws.(S.I NO: 14 (d) P.NO: 60) | | | | | |  |  |
|  | windows | 5x4.0x4.0 | = | 80 | Sft |  |  |  |
|  |  |  | = | 80 | “ | 190.72 | P.Sft | 15258/- |
| 30/- | White washing. 03 three coats (S.I NO: 26 ©P.NO: 54). | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 1072 | “ | 829.95 | % Sft | 8897/- |
| 31/- | Distempering. three 03 Coats (S.I NO: 24 P-54) | | | | | |  |  |
|  |  |  | = | 4146 | “ | 1079.65 | % Sft | 44762/- |
|  |  |  |  |  |  |  |  |  |
| 32/- | Painting doors and windows any type (S.I NO: P.NO: ) | | | | | |  |  |
|  |  |  | = | 587 | “ | 2116.41 | % Sft | 12423/- |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 33/- | Preparing the surface and painting with weather coat of approved make to old weather coat surface.(S.I NO: 39(b) A P-56) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 1632 | “ | 1948.50 | % Sft | 31800/- |
|  |  |  |  | ===================================== | | | | |
|  |  |  | **Total** | |  |  |  | **3122718/-** |
|  |  |  |  | |  |  |  |  |
|  |  |  |  | |  |  |  |  |

CONTRACTOR EXECUTIVE ENGINEER

PROVINCIAL BUILDINGS DIVISON

SHAHEED BENAZIR ABAD