***SCHEDULE OF QUANTITIES***

***WORK No: 03***

# 

**DISTRICT MUNICIPAL CORPORATION (WEST)**

**KARACHI, BALDIA ZONE**

***Estimated Cost Rs: 7,27,229/-+O/R Earnest Money Rs: 14,544-+O/R***

***Time Limit: 45 Days Penalty Per Day Rs: 1,000/-***

**SUBJECT: *Maintenance of Park Cum Play Ground Baldia # 7,UC-32 Baldia Zone, DMC (West).***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ***S.No:*** | ***DESCRIPTION OF WORK*** | ***QUANTITY*** | ***RATE*** | ***PER*** | ***AMOUNT*** |
| *1.* | *Excavation for foundation of building bridges and other structure i/c dog bolling dressing refilling ground structure with excavated earth watering & ramming lead upto 5 Feet in ordinary soil.* | *1117* | *3176.25* | *%0Cft* | *3548/-* |
| *2.* | *Excavation ton (and reserves in soft soil i/c trimming and dressing sides to tale pigment design section / profile and shape leveling i/c laying at earth in 6” layer for construction of bars and dicing and deposal of surplus earth excavated earth within one chain as directed by engineer in charge ilc providing fence guide lights flogs and temporary crossings for noon vehicular traffic where war relish lift upto 5 ft.* | *600* | *3000* | *%Cft* | *1800/-* |
| *3.* | *Erection and removal centering for R.C.C or Plain cement concrete wore of portion wood (2nd class) vertical).* | *1567* | *3127.41* | *%Sft* | *49006.51/-* |
| *4.* | *Fabrication of mild steel reinforcement for cement concrete including cutting, bending, laying in position making joints and fastenings including cost of binding wire (also includes removal of rust from bars) using tor* | *54.09* | *4820.20* | *Pcwt* | *260725/-* |
| *5.* | *Providing & Laying 1:3:6 cement concrete solid block masonry wall above 6 in thickness set in 1:6 cement mortar in GF ground floor Super structure including ranking out joints and crying etc Complete.* | *1031* | *14621.44* | %Cft | *150747/-* |
| *6.* | *Cement concrete plain including play compacting finishing (1:4:8)* | *33* | *11288.75* | %Cft | *3725/-* |
| *7.* | *Cement concrete plain including play compacting finishing and curing complete (including screening and washing at stone aggregate without shuttering (1:2:4)* | *488.20* | *14429.25* | *%Cft* | *70444/-* |
| *8.* | *Cement Plaster 1:4 12” Height.* | *4619* | *2496.72* | *%Sft* | *115323/-* |
| *9.* | *Cement née plaster 1:2 cement and sand ¼” three* | *340* | *1176.83* | *%Sft* | *4001/-* |
| *10.* | *Water supply pump sel.* | *01-Nos* | *O/R* | *Each* | *O/R* |
| *11.* | *Distempering three coat.* | *4764* | *1079.65* | *%Sft* | *51434.52* |
| *12.* | *Painting with enamel paint on masonry wall.* | *746* | *837.10* | *%Sft* | *6244.76/-* |
| *13.* | *Providing & Laying up VC-1 Dia Pipe.* | *750* | *O/R* | *P/Rft* | *O/R* |
| *14.* | *Tee 1” Dia* | *12-Nos* | *O/R* | *Each* | *O/R* |
| *15.* | *ELBO 1” Dia* | *12-Nos* | *O/R* | *Each* | *O/R* |
| *16.* | *Socket 1” Dia* | *35-Nos* | *O/R* | *Each* | *O/R* |
| *17.* | *Valves 1” Dia* | *6-Nos* | *O/R* | *Each* | *O/R* |
| *18.* | *Tumbler Plantation.* | *700-Nos* | *O/R* | *Each* | *O/R* |
| *19.* | *Carriage of Material of 100 Cft 5 tons all material like stone aggregate sprawl, lod, line, B-4 Rail fastening points and crossing bridge cards points shut Rails M.S Bars. Etc 100 other man own by the Contractors.* | *1717* | *595.80* | *%Cft* | *10230/-* |
| ***Total Estimated Cost*** | | | | | ***7,27,229/-+O/R*** |

*Nomenclature, Quantities and Rates etc checked*

*and found correct.*

***SUB-ENGINEER (PARK) Dy. DIRECTOR (PARK & RECREATION)***

*BALDIA ZONE BALDIA ZONE*

*I/We hereby quoted Rates @ % above/below the S/R*

*The total amount is Rs: (Rupees:*

*(In Figure) (In Word)*

## *Contractor’s Signature:*

## 

## *Address:*