**OFFICE OF THE EXECUTIVE ENGINEER (B&R) SITE ZONE DMC WEST KARACHI**

**Work 01**

**SUBJECT: - HIRING OF MACHINERY I/C EXCAVATOR, LOADER, DUMPER**

**AND LABOUR FOR DEASALTING AND CLEANING OF NALLAH**

**REGARDING UPLIFTING OF AREA SITE ZONE DMC (WEST)**

**E/Cost: 9,85,406/- E/Money 20,000/- T/Limit 45 Days Penalty 500/- PD.**

**S.No Description of Work Quantity Rate Per%**

1. **Hiring of Machinery**

Machiner with POL

1. Front Loader / Excavator 85 Hours 3088.13/P.Hour
2. Dumper (Hino) 350 Hours 2006.90/P.Hour

2. Hiring of Skilled Labour for Cleaning of Nallah for 8 Hour 23 Nos 750/Each

3. Over Time of Private Labour after 8 hours 26 Hours 125/P.Hour

**EXECUTIVE ENGINEER (B&R)**

**SITE ZONE DMC (WEST)**

**I / we hereby quoted \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Above / Below the SR.**

**Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**OFFICE OF THE EXECUTIVE ENGINEER (B&R) SITE ZONE DMC WEST KARACHI**

**Work 02**

**SUBJECT: - HIRING OF TRACTOR BLADE AND OTHER MACHINERY FOR**

**REPAIR & REHABILITATION OF ROAD MEVASHAH GRAVEYARD**

**ROAD AND JOHAR COLONY UC-05 SITE ZONE DMC (WEST)**

**E/Cost: 9,97,354/- E/Money 20,000/- T/Limit 45 Days Penalty 500/- PD.**

**S.No Description of Work Quantity Rate Per%**

1. **Hiring of Machinery**

Machiner with POL

1. Front Loader / Excavator 56 Hours 3088.13/P.Hour
2. Dumper (Hino) 336 Hours 2006.90/P.Hour

2. Hiring of Tractor Blade for Cleaning of Road & Street

with P.O.L 158 Hours 950/P.Hour

**EXECUTIVE ENGINEER (B&R)**

**SITE ZONE DMC (WEST)**

**I / we hereby quoted \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Above / Below the SR.**

**Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**OFFICE OF THE EXECUTIVE ENGINEER (B&R) SITE ZONE DMC WEST KARACHI**

**Work 03**

**SUBJECT: - REHABILITATION OF SEWERAGE SYSTEM FROM JOHAR COLONY**

**WARD NO. 02 PARDHA PARK IN UC-05 SITE ZONE**

**E/Cost: 8,71,282/- E/Money 20,000/- T/Limit 45 Days Penalty 500/- PD.**

**S.No Description of Work Quantity Rate Per%**

1. Dismantling of CC Work 1:2:4 875/Cft 3327.50%Cft

2. Excavation of pipe line trenches pipe all kind of soil

murum i/c trimming dressing leveling beds trenches

correct level and graded cutting joints holes disposal

of surplus earth with in 1 chains as directed by the

Engg: Inch: P. fence guard lights flags temporary

crossing non vehicler traffic where ever req: a lift up

to 5 ft & lead up to 1 chain. 8313/Cft 4650 %0 Cft

3. P. Rcc pipe ASTM class class ‘C’ 76-62 T/C 76-70

class II wall ‘B’ and fixing in trenches i/c cutting

fitting jointing with rubber ring i/c testing with water

to specified pressure 9″ & 12″dia pipe. 700/Rft 412/P.Rft

4. Const of Main Holes 4 inside with Rcc covers 21″dia

3×¾ with flat iron frame 5ft depth 1:2:4 in laying CC

cost in situ 9″ thick wall and disposal of surplus stuff

etc comp: 30/Nos. 13028 / Each

5. Add or deduct for depth of man holes above or beyond

5 ft (RA). 7.5/Rft 2245.55/P.Rft

6. Refilling the excavated stuff in trenches 6″ thick layer i/c

watering ramming to full compaction etc comp: 8269/Cft 2760.0/%0Cft

7. M/S 21”dia Rcc Manhole covers cost is 1:2:4 concrete

ratio 3" depth at i/c reinforced with 3/8"dia tor steel bars

4" C.C welded to 1/8" thick 2.5" depth M.S plat i/c curing

stacking and transportation with in 10 Miles 30 Nos 913.63/Each

8. M/S of Rcc Ring Slab of 21"dia inside 36"dia out side

75" width and 6" thick i/c dia tor steel bars two concrete

ring with 3/8"dia 8 No cross liaked bars welded and two

sunk type hooks cost in a 1:1 1/2 3 concrete with embaded

15kg C.I from in prefund position i/c transportation

cage etc 30 Nos 1906.60/Each

**EXECUTIVE ENGINEER (B&R)**

**SITE ZONE DMC (WEST)**

**I / we hereby quoted \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Above / Below the SR.**

**Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**OFFICE OF THE EXECUTIVE ENGINEER (B&R) SITE ZONE DMC WEST KARACHI**

**Work 04**

**SUBJECT: - WINCTHING OF CHOCKED EXISTING SEWERAGE SYSTEM IN**

**NOORANI MASJID TO WARSI MASJID AND BHITTAI LIBRARY TO**

**SHAHNAWAZ CHOWK UC-06 SITE ZONE DMC (WEST)**

**E/Cost: 9,92,150/- E/Money 20,000/- T/Limit 45 Days Penalty 500/- PD.**

**S.No Description of Work Quantity Rate Per%**

1. Cleaning inside sewerage Line completely restoring

original silt free space / diameter of pipe lines by labour

and equipment (Mechanically / electrically driven)

including accessories like pulleys steel rope bucket

and draggers sizing from 6” to 18”dia. Their to and from

“Pulling action (No of Passes Shall be as many as required)

would be taken in two phases (as free flow) and in second

phase from up to stream to down stream of entier length

ensuring no silt is observed in buckets (6”dia to 18”dia)

except only sewage water and finally passing a steel ball

of dia 12” lesser that the diameter of pipe but nott

exceeding 48”dia ball even for larger dia pipe to ensure

perfect cleaning. The job includes all the hiew / cost of

equipment and accessories of above winching machine /

devices curing desalting and clearance of site etc

complete as per full satisfaction of site Engineer

12”dia 5000/Rft 80.50/P.Rft

15”dia 1000/Rft 96.60/P.Rft

18”dia 1000/Rft 128.80/P.Rft

2. M/S 21”dia Rcc Manhole covers cost is 1:2:4 concrete

ratio 3" depth at i/c reinforced with 3/8"dia tor steel bars

4" C.C welded to 1/8" thick 2.5" depth M.S plat i/c curing

stacking and transportation with in 10 Miles 190 Nos 913.63/Each

3. M/S of Rcc Ring Slab of 21"dia inside 36"dia out side

75" width and 6" thick i/c dia tor steel bars two concrete

ring with 3/8"dia 8 No cross liaked bars welded and two

sunk type hooks cost in a 1:1 1/2 3 concrete with embaded

15kg C.I from in prefund position i/c transportation

cage etc 100 Nos 1906.60/Each

**EXECUTIVE ENGINEER (B&R)**

**SITE ZONE DMC (WEST)**

**I / we hereby quoted \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Above / Below the SR.**

**Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**OFFICE OF THE EXECUTIVE ENGINEER (B&R) SITE ZONE DMC WEST KARACHI**

**Work 05**

**SUBJECT: - HIRING OF MACHINERY LOADER, DUMPER & LABOUR FOR**

**REMOVAL OF DEBRIS & CLEANING OF NALLAH IN UC-05 &**

**UC-06 SITE ZONE DMC (WEST)**

**E/Cost: 9,98,684/- E/Money 20,000/- T/Limit 45 Days Penalty 500/- PD.**

**S.No Description of Work Quantity Rate Per%**

1. **Hiring of Machinery**

Machiner with POL

1. Front Loader / Excavator 88 Hours 3088.13/P.Hour
2. Dumper (Hino) 352 Hours 2006.90/P.Hour

2. Hiring of Skilled Labour for Cleaning of Nallah for 8 Hour 22 Nos 750/Each

3. Over Time of Private Labour after 8 hours 32 Hours 125/P.Hour

**EXECUTIVE ENGINEER (B&R)**

**SITE ZONE DMC (WEST)**

**I / we hereby quoted \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Above / Below the SR.**

**Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**OFFICE OF THE EXECUTIVE ENGINEER (B&R) SITE ZONE DMC WEST KARACHI**

**Work 06**

**SUBJECT: - HIRING OF MACHINERY LOADER, DUMPER & LABOUR FOR**

**REMOVAL OF DEBRIS & CLEANING OF NALLAH IN UC-14 &**

**UC-15 SITE ZONE DMC (WEST)**

**E/Cost: 9,99,082/- E/Money 20,000/- T/Limit 45 Days Penalty 500/- PD.**

**S.No Description of Work Quantity Rate Per%**

1. **Hiring of Machinery**

Machiner with POL

1. Front Loader / Excavator 87 Hours 3088.13/P.Hour
2. Dumper (Hino) 350 Hours 2006.90/P.Hour

2. Hiring of Skilled Labour for Cleaning of Nallah for 8 Hour 32 Nos 750/Each

3. Over Time of Private Labour after 8 hours 32 Hours 125/P.Hour

**EXECUTIVE ENGINEER (B&R)**

**SITE ZONE DMC (WEST)**

**I / we hereby quoted \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Above / Below the SR.**

**Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**OFFICE OF THE EXECUTIVE ENGINEER (B&R) SITE ZONE DMC WEST KARACHI**

**Work 07**

**SUBJECT: - IMP OF CULVERT MAIN KATTI PAHARI ROAD INFRONT OF**

**BISMILLAH MASJID SITE ZONE DMC (WEST)**

**E/Cost: 7,38,378/- E/Money 20,000/- T/Limit 45 Days Penalty 500/- PD.**

**S.No Description of Work Quantity Rate Per%**

1. P/L 1:2:4 cc situ i/c placing compacting finishing curing

i/c screening washing stone aggregate without shuttering

etc. 96/Cft 14429.25%Cft

2. Erection or removal centering for Rcc or Plain CC plain

work deador wood 2nd class. 192/Sft 3588.48%Sft

3. P/L Rcc work i/c all labour materials the cost of reinf:

its labour bending which will be a paid separately i/c all

kind form moulds lifting shuttering washing finishing

single Rcc work roof slab beams lintel columns other

structural members laid in situ or pre cost in position

in all respect. 240/Cft 337/P.Cft

4. Fabrication of mild steel reinforcement cement concrete

i/c cutting binding laying in position making joints and

fastening i/c cost of bending wire also i.c removal rust

from bars. 12.29/Cwt 5001.70/P.Cwt

5. Dismantling CC reinf: separating reinforcement from

concrete cleaning the straightening the same. 384/Cft 5445%Cft

6. Cartage of 100 Cft 5 tons all materials like stone aggregate

spwals lime surkhi BG rail fasting points crossing bridge

guders pipe sheet M/S Brass sheets 1000 trenches 10×5×3"  
1000 tiles 12×6×2" 150 cft timber 100 mould fuel wood

by trenches owned by the contractor withing 10 miles

etc comp: 308/Cft 902.20%Cft

7. **Hiring of Machinery**

Machiner with POL

1. Front Loader / Excavator 62 Hours 3088.13/P.Hour
2. Dumper (Hino) 128 Hours 2006.90/P.Hour

8. Hiring of Skilled Labour for Cleaning of Nallah for 8 Hour 118 Nos 750/Each

9. Over Time of Private Labour after 8 hours 118 Hours 125/P.Hour

**EXECUTIVE ENGINEER (B&R)**

**SITE ZONE DMC (WEST)**

**I / we hereby quoted \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Above / Below the SR.**

**Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**