***“SHEDULE B”***

**NAME OF WORK:- CONSTRUCTION OF C/WALL GOVT. GIRLS DEGREE COLLEGE DAHARKI TALUKA DAHARKI.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S. No:** | **Item of Work** | **Qty:** | **Rate** | **Unit** | **Amount** |
|  |  |  |  |  |  |
| 1 | Excavation in foundation of Building Bridges and other structures including dagbelling dressing, refilling around structure with excavated earth Watering and ramming lead upto 5 ft In ordinary soil (S. I No: 18 (b) P. No: 4). | | | | |
|  |  | 4043 | @ 3176/25 | %0Cft | 12842/- |
|  |  |  |  |  |  |
| 2 | Cement concrete brick or stone ballast 1 1/2" to 2" gauge Ratio 1 : 5 : 10 (S. I 4 (c) P. No: 15). | | | | |
|  |  | 643 | @ 8694/95 | %Cft | 55909/- |
| 3 | Reinforced cement concrete work including all labour and material except the cost of steel reinforcement and its labour for bending and binding which will be paid separately. This rate also includes all kinds of forms moulds lifting shuttering curing rendering and finishing the exposed surface (including screening and washing of shingle) (S. I No: 6 a i P. No: 17) | | | | |
|  |  | 1272 | @ 337/- | P.Cft | 428664/- |
|  |  |  |  |  |  |
| 4 | Fabrication of mild steel reinforcement for cement concrete including cutting, bending, laying in position, making joints and fastenings including cost of binding wire (also includes removal of mild steel (S. I No: 8 (b) P. No: 17) | | | | |
|  | Tor Bar | 56.785 | @ 5001/70 | P.Cwt | 284025/- |
|  | Mild Steel | 11.357 | @ 4820/20 | P.Cwt | 54744/- |
|  |  |  |  |  |  |
| 5 | Pacca brick work in foundation and plinth in Cement sand mortar 1:6 (S. I No: 4 (e) P. No: 21). | | | | |
|  |  | 969 | @ 11948/36 | %Cft | 115780/- |
|  |  |  |  |  |  |
| 6 | Pacca brick work other then building including striking of joints upto 20 feet height in Cement sand mortar 1:6 (S. I No: 7 I (e) P. No: 22). | | | | |
|  |  | 1903 | @ 12346/65 | %Cft | 234857/- |
|  |  |  |  |  |  |
| 7 | Cement plaster 1:6 upto 12' height 1/2" thick (S.I No: 13 (b) P. No: 52). | | | | |
|  |  | 7658 | @ 2206/60 | %Sft | 168981/- |
|  |  |  |  |  |  |
| 8 | Cement plaster 1:4 upto 12' height 3/8" thick (S.I No: 11 (a) P. No: 52). | | | | |
|  |  | 7658 | @ 2197/52 | %Sft | 168286/- |
|  |  |  |  |  |  |
| 9 | Colour washing 03 coats (S. I No: 25 (b) P. No: 54) | | | | |
|  |  |  |  |  |  |
|  |  | 7658 | @ 859/90 | %Sft | 65851/- |
|  |  |  |  |  |  |
| 10 | Providing & fixing angle iron vertical plats barbed wire fencing of size 2”x2 ½” embedded in RCC / Masonry pillars i/c making cuts / holders @ 12” i/c fixing in pillars by chiseling and filling the with cement sand mortar, spraining & finishing the surface (R.A). | | | | |
|  |  | 685 | @ 628/- | P.Rft | 430180/- |
|  |  |  |  |  |  |
|  |  |  |  | **Total** | **2020219/-** |

\_\_\_\_\_\_\_\_% above/below on the rates of CSR.

**CONTRACTOR**

### EXECUTIVE ENGINEER

**EDUCATION WORKS DIVISION**

**GHOTKI**