***“SHEDULE B”***

**NAME OF WORK:- CONSTRUCTION OF C/WALL GOVT. GIRLS DEGREE COLLEGE GHOTKI TALUKA GHOTKI.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S. No:** | **Item of Work** | **Qty:** | **Rate** | **Unit** | **Amount** |
|  |  |  |  |  |  |
| 1 | Dismantling brick work in lime or cement mortar (S.I No: 13 P. No: 10) | | | | |
|  |  |  |  |  |  |
|  |  | 88 | @ 1285/63 | %Cft | 1131/- |
|  |  |  |  |  |  |
| 2 | Cement concrete plain placing compacting finishing and complete i/c screening and washing stone aggregate without shuttering Ratio: 1:2:4 (SI No: 5 P-16) | | | | |
|  |  |  |  |  |  |
|  |  | 88 | @ 14429/25 | %Cft | 12698/- |
|  |  |  |  |  |  |
| 3 | Erection and removal of centering for R.C.C of plain cement concrete works of deodar wood (2nd Class) (S. I No: 19 b ii P. No: 18) | | | | |
|  |  |  |  |  |  |
|  |  | 234 | @ 3127/41 | %Sft | 7318/- |
|  |  |  |  |  |  |
| 4 | Reinforced cement concrete work including all labour and material except the cost of steel reinforcement and its labour for bending and binding which will be paid separately. This rate also includes all kinds of forms moulds lifting shuttering curing rendering and finishing the exposed surface (including screening and washing of shingle) (S. I No: 6 a i P. No: 17) | | | | |
|  |  |  |  |  |  |
|  |  | 469 | @ 337/- | P.Cft | 158053/- |
|  |  |  |  |  |  |
| 5 | Fabrication of mild steel reinforcement for cement concrete including cutting, bending, laying in position, making joints and fastenings including cost of binding wire (also includes removal of mild steel (S. I No: 8 (b) P. No: 17) | | | | |
|  |  |  |  |  |  |
|  |  | 20.937 | @ 5001/70 | P.Cwt | 104721/- |
|  |  |  |  |  |  |
| 6 | Removing cement or lime plaster (S. I No: 53 P. No: 13) | | | | |
|  |  |  |  |  |  |
|  |  | 7110 | @ 121 | %Sft | 8603/- |
|  |  |  |  |  |  |
| 7 | Applying floating coat of cement 1/32” thick (S. I No: 14 P. No: 53) | | | | |
|  |  |  |  |  |  |
|  |  | 7110 | @ 660/- | %Sft | 46926/- |
|  |  |  |  |  |  |
| 8 | Cement plaster 1:4 upto 12’ height ¾ “ thick (S. I No: 11 (c) P. No: 52) | | | | |
|  |  |  |  |  |  |
|  |  | 7110 | @ 3015/76 | %Sft | 214421/- |
|  |  |  |  |  |  |
| 9 | Providing & fixing angle iron vertical plats barbed wire fencing of size 2”x2” ½” embedded in RCC / Masonry pillars i/c making cuts / holders @ 12” i/c fixing in pillars by chiseling and filling the with cement sand mortar, spraining & finishing the surface (S. I No: 8 P. No: 95). | | | | |
|  |  |  |  |  |  |
|  |  | 468 | @ 169/18 | P.Rft | 79176/- |
|  |  |  |  |  |  |
| 10 | Providing & fixing barbed wire fencing with 12 gauge-4 points @ 6” apart barbed wire i/c straightening & fixing in angle iron vertical posts (S. I No: 9 P. No: 96) | | | | |
|  |  |  |  |  |  |
|  |  | 7110 | @ 8/38 | P.Rft | 59582/- |
|  |  |  |  |  |  |
| 11 | Colour washing 03 coats (S. I No: 25 (b) P. No: 54) | | | | |
|  |  |  |  |  |  |
|  |  | 24174 | @ 859/90 | %Sft | 207873/- |
|  |  |  |  |  |  |
|  |  |  |  | **Total** | **900502/-** |

\_\_\_\_\_\_\_\_% above/below on the rates of CSR.

**CONTRACTOR**

### EXECUTIVE ENGINEER

**EDUCATION WORKS DIVISION**

**GHOTKI**