**SCHEDULE “B” FOR PROVIDING INSTALLING OF HYPO CHLORINATOR @ VARIOUS OPERATION AND MAINTENANCE OF RURAL WATER SUPPLY SCHEMES TALUKA SANGHAR & SINJHORO DISTRICT SANGHAR.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.# | Description | Qty | Rate | Unit | Amount |

1. Pultron (USA) series “A” Plus model LBBS3SB-VTC-XX Hypo Chlorinator (Electronic Metering pump) flow rate 33 GPD Max, pressure 150 PSL/10-Bar Solenoid protection y Thermal Over load with Auto Rest Manual Control, Dosage Adjustable 0-100% Highly reliable water resistant made for indoor and outdoor installation guided ball check valve circuit protection against voltage and circuit upset Material non corrosive made to inject sodium Hypochlorite solution in water supply delivery main line following slandered accessories with each unit as per attached light bulletin # EMP 025 B-5 (Non Schedule Item)

1. Clear Flexible solution Tubing.
2. Stiff white Discharge tubing
3. Foot valve / Strainer Assembly
4. Back pressure injection valve
5. Bleed valve assembly
6. Strainer weight
7. Installation Operation Maintenance manual.

1.0 No @Rs. Each Rs.

Total Rs.

**Rs. x 10 = Rs.**

**CONDITIONS.**

1. Any error omission in the specification quantity and unit will be governed by the relevant schedule items.
2. The rates should be inclusive of all taxes i.e sales tax octori tax etc.
3. No separate carriage will be paid to the contractor
4. No premium will be allowed for no-schedule items.
5. The decision of the Superintending Engineer, Public health Engineering Circle Mirpurkhas will be final and binding the parties if in any dispute.

EXECUTIVE ENGINEER

PUBLIC HEALTH ENGG: DIVISION

SANGHAR