|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **SCHEDULE-B**  **ESTABLISHMENT OF DISTRICT ARCHIVES KHAIRPUR.**  **Part-A** | | | | | | | | | | | | |
| 1 | Excavation in foundation of Building Bridges and other structures including dabbling dressing, refilling around structure with excavated earth Watering and ramming lead up to 5 ft.(S.I NO: 18 P.NO: 4) | | | | | | | |  |  |  |  |
|  |  |  |  |  |  |  |  |  | 8183 Cft | 3176.25 | %0Cft | 25993 |
| 2 | Cement concrete brick or stone ballast 1 1/2" to 2" gauge.(S.I NO: 4 (b)P.NO: 15) | | | | | | | |  |  |  |  |
|  |  |  |  |  |  |  |  |  | 866 Cft | 11948.36 | % Cft | 103497 |
| 4 | R.C.C work in roof slab, beams columns rafts, lintels and other structural members laid in situ or precast laid in position complete in all respects. Ratio (1 : 2: 4 ) 90 Lbs. cement 2 Cft. Sand 4 Cft. Shingle 1/8" to 1/4" gauge.(S.I NO: 6 (a)P-16) | | | | | | | |
|  |  |  |  |  |  |  |  |  | 4562 Cft | 337 | P.Cft | 1537259 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
| 5 | Fabrication of mild steel reinforcement for cement concrete including cutting, bending, laying in position, making joints and fastenings including cost of binding wire (also includes removal of rust from bars.)(S.I NO: 8 P.NO: 17) | | | | | | | |  |  |  |  |
|  |  |  |  |  |  |  |  |  | 264.76 Cwt | 5001.7 | P.cwt | 1324245 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
| 6 | Filling, watering and ramming earth in floors with surplus earth from foundation lead upto one chain and lift jupto 5 feet.(S.I NO: 21 P-4). | | | | | | | |  |  |  |  |
|  |  |  |  |  |  |  |  |  | 5455 Cft | 1512.5 | % Cft | 8251 |
| 7 | Supplying and filling sand under floor and plugging in walls.(S.I NO: 29 P-26) | | | | | | | |  |  |  |  |
|  |  |  |  |  |  |  |  | = | 3654 Cft | 1141.25 | % Cft | 41701 |
| 8 | Pacca Brick work in Ground Floor in cement sand mortar 1:6 ( S.I NO: 5 P-21) | | | | | | | |  |  |  |  |
|  | Net: Qty: 2368 - 431 = | | | | | | |  | 1937 Cft | 12674.36 | % Cft | 245502 |
| 9 | Cement plaster 1:6 upto 12' height.(b) 1/2" thick. (S.I NO: 13 P-52) | | | | | | | | |  |  |  |
|  |  | | | | | | |  | 5939 Sft | 2206.6 | % Sft | 131050 |
| 10 | Cement plaster 1:4 upto 12' height.(b) 3/8" thick. (S.I NO: 13 P-52) | | | | | | | |  |  |  |  |
|  |  |  |  |  |  |  |  |  | 5939 Sft | 2197.52 | % Sft | 130511 |
| 11 | Providing and fixing G.I frames /Choukhats of size 7" x 2" or 4 1/2" x 3" for door using 20 gauge G.I sheet I/c welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage , tools and plants used in making and fixing.(CSI NO: 29 P-93) | | | | | | | |  |  |  |  |
|  |  |  |  |  |  |  |  |  | 342 Rft | 228.9 | P.Rft | 78284 |
| 12 | First class deodar wood wrought, joinery in doors and windows etc, fixed in position including chowkats hold fasts hinges, iron tower bolts, chocks cleats, handles and cords with hooks, etc.(1 3/4" thick)(S.I NO: 7 P-58) | | | | | | | |  |  |  |  |
|  |  |  |  |  |  |  |  |  | 269 Sft | 902.93 | P.Sft | 242888 |
| 13 | Laying white marble flooring fine dressed on the surface without winding set in lime mortar 1:2 including rubbing and polishing of the joints.(S.I NO: 28 P.NO: 43) | | | | | | | |  |  |  |  |
|  |  |  |  |  |  |  |  |  | 1427 Sft | 567.48 | P.Sft | 809794 |
| 14 | Providing and fixing 3/8" thick marble tiles of approved quality and colour and shade size 8" x 4" /6" x 4" in dado skirting anf facing removal /tucking of existing plaster surface ete. Over 1/2" thick base of cement mortar 1:3 setting of tiles in slurry of white cement over mortar base including filling the joints and washing the tiles with white cement slurry , currint finishing, cleaning and ploishing etc. complete.(S.I NO: 68 P.NO: 49) | | | | | | | | |  |  |  |
|  |  |  |  |  |  |  |  |  | 449 Sft | 186.04 | P.Sft | 83532 |
| 15 | Laying floor of approved with glazed tile 1/4" thick in white cement 1:2 over 3/4" thick cement mortar 1:2 complete.(S.I NO: 24 P.NO: 43) | | | | | | | |  |  |  |  |
|  |  |  |  |  |  |  |  |  | 372 Sft | 27678.86 | % Sft | 102965 |
| 16 | White glazed tiles 1/4" thick dado jointed in white cement and laid over 1:2 cement sand mortar 3/4" thick including finishing.(S.I NO: 37 P.NO: 45) | | | | | | | |  |  |  |  |
|  |  |  |  |  |  |  |  |  | 341 Sft | 28253.61 | % Sft | 96345 |
| 17 | Providing & fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with pigmented having strength b/w 5000 psi to 8500 psi I/c filling the joints with hill sand and laying in specified manner / patter and design etc: complete.( S.I NO: 74 P-50) | | | | | | | |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  | 210 Sft | 248.17 | P.Sft | 52116 |
| 18 | Supplying and fixing false ceiling of plaster of Paris, in panels including making frame , work of Deodar wood including painting with Soligia paint. (S.I NO: 52 P-64) | | | | | | | |  |  |  |  |
|  |  |  |  |  |  |  |  |  | 605 Sft | 25293.42 | % Sft | 153025 |
| 19 | Providing & fixing plaster of Paris ceiling border of 8" -10 " with of specified design & thickness I/c fixing besides ceiling with nails/ screws with jetties.(S.I NO: 44 P-39) | | | | | | | |  |  |  |  |
|  |  |  |  |  |  |  |  |  | 198 Sft | 104.22 | P.Sft | 20636 |
| 20 | Supplying & fixing in position iron/steel grill of 3/4" x 1/4" size flat iron of approved design including painting 3 coats etc. complete (weight not to be less than 3.7 Lbs./Sq . Foot of finished grill).(S.I NO: 26 P-93) | | | | | | | |  |  |  |  |
|  |  |  |  |  |  |  |  |  | 84 Sft | 180.5 | P.Sft | 15162 |
| 21 | Preparing the surface and painting with matt finish I/c rubbing the surface with Bathy (silicon carbide rubbing brick) filling the voids with zink /chalk / plaster of paris mixture, applying first coat premix, making the surface smooth and then painting 3 coats with matt finish of approved make etc: complete .(new surface).(S.I NO: 36(A) P-55) | | | | | | | |  |  |  |  |
|  | Net: Qty: | 5409 (-) 260 | | | | | | | 5149 Sft | 3444.38 | % Sft | 177351 |
|  |  |  | | | | | | |  |  |  |  |
| 22 | Two coats of bitumen laid hot using 34 Lbs for % Sft. Ober roof and blinded with sand at one Cft. Per % Sft.(S.I 13 P.NO; 35) | | | | | | | |  |  |  |  |
|  |  |  |  |  |  |  |  |  | 2523 Sft | 1887.4 | % Sft | 47619 |
| 23 | Supplying & fixing in position iron/steel grill of 3/4" x 1/4" size flat iron of approved design including painting 3 coats etc. complete (weight not to be less than 3.7 Lbs./Sq . Foot of finished grill).(S.I NO: 26 P-93) | | | | | | | |  |  |  |  |
|  |  |  |  |  |  |  |  |  | 156 Sft | 180.5 | P.Sft | 28158 |
| 24 | RCC Spouts including fixing in position with top & Bottom khurras ( S.I NO: 68 P-107) | | | | | | | |  |  |  |  |
|  |  |  |  |  |  |  |  |  | 15 Nos | 604.17 | each | 9063 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
| 25 | PNS, Painting Doors and Windows any type including edges three coats ( S.I NO: 4 P-76) | | | | | | | |  |  |  |  |
|  |  |  |  |  |  |  |  |  | 552 Sft | 2116.41 | % Sft | 11683 |
| 26 | Painting guard bars, gates iron bars gratings , railings including standard braces (etc.) and similar open work.(S.I NO: 1 P.NO: 69) | | | | | | | |  |  |  |  |
|  |  |  |  |  |  |  |  |  | 156 Sft | 1270.83 | % Sft | 1982 |
|  | ==================================== | | | | | | | | | | | |
|  |  |  |  |  |  |  |  |  | **Total** |  |  | **4865202** |
|  |  | | | | | | | | |  |  |  |

**PART-B FIRST FLOOR**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 01 | | | Pacca Brick work in Ground Floor in cement sand mortar 1:6 ( S.I NO: 5 P-21) | | | | | | | | | | | | | | | | | |  | | | |  | | | |  | | | |  | | | |
|  | | |  | | | | | | | | | | | | | | |  | | | 2842 Cft | | | | 12674.36 | | | | % Cft | | | | 360205/- | | | |
| 2 | Add: Extra Labour for First Floor. | | | | | | | | | | | | | | | | | | |  | | | |  | | | |  | | | | | |  | |
|  | Same Qty: of item NO: 1 | | | | | | | | | | | | |  | | | | | | 2842 Cft | | | | 438.63 | | | | % Cft | | | | | | 12466 | |
|  |  | | | | | | | | | | | | |  | | | | | |  | | | |  | | | |  | | | | | |  | |
| 3 | | R.C.C work in roof slab, beams columns rafts, lintels and other structural members laid in situ or precast laid in position complete in all respects. Ratio (1 : 2: 4 ) 90 Lbs. cement 2 Cft. Sand 4 Cft. Shingle 1/8" to 1/4" gauge.(S.I NO: 6 (a)P-16) | | | | | | | | | | | | | | | | | | | |
|  | |  | |  | |  | |  | |  | |  | | |  | |  | | | | | 2284 Cft | | | | 337 | | | | P.Cft | | 769731/- | | |
| 04 | | Add: Extra labour for First Floor RCC work | | | | | | | | | | | | | | | | | | | | | | | |  | | | |  | |  | | |
|  | | Same Qty: of item NO: 3 | | | | | | | |  | |  | | |  | |  | | | | | 2284 Cft | | | |  | | | |  | |  | | |
|  | |  | |  | |  | |  | |  | |  | | |  | |  | | | | | 2284 Cft | | | | 12.10 | | | | P,Cft | | 27636/- | | |
| 5 | | Fabrication of mild steel reinforcement for cement concrete including cutting, bending, laying in position, making joints and fastenings including cost of binding wire (also includes removal of rust from bars.)(S.I NO: 8 P.NO: 17) | | | | | | | | | | | | | | | | | | | |  | | | |  | | | |  | |  | | |
|  | |  | | | | | | | | | | | | | | | | | | | | 132.55 cwt | | | | 5001.70 | | | | P.cwt | | 662975/- | | |
| 06 | | Add: Extra labour for First Floor Fabrication work | | | | | | | | | | | | | | | | | | | | | | | |  | | | |  | |  | | |
|  | |  | |  | |  | |  | |  | |  | | |  | |  | | | | | 132.55 cwt | | | | 151.25 | | | | P,Cft | | 20048/- | | |
| 07 | | Providing and fixing G.I frames /Choukhats of size 7" x 2" or 4 1/2" x 3" for door using 20 gauge G.I sheet I/c welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage , tools and plants used in making and fixing.(CSI NO: 29 P-93) | | | | | | | | | | | | | | | | |  | | | |  | | | |  | | | |  | | | |
|  | |  | |  | |  | |  | |  | |  | | |  | |  | | 243 Rft | | | | 228.9 | | | | P.Rft | | | | 55623/- | | | |
| 08 | | First class deodar wood wrought, joinery in doors and windows etc, fixed in position including chowkats hold fasts hinges, iron tower bolts, chocks cleats, handles and cords with hooks, etc.(1 3/4" thick)(SN: 7 P-58) | | | | | | | | | | | | | | | | |  | | | |  | | | |  | | | |  | | | |
|  | |  | |  | |  | |  | |  | |  | | |  | |  | | 276 Sft | | | | 902.93 | | | | P.Sft | | | | 249209/- | | | |
|  | |  | |  | |  | |  | |  | |  | | |  | |  | |  | | | |  | | | |  | | | |  | | | |
| 09 | | Supplying & fixing in position Aluminum channels framing for hinged doors or Alcop made with 5 mm thick tinted glass glazing (Belgium) and Alpha (Japan) locks I/c handles, stoppers etc.(S.I NO: 83 (bP-NO: 108) | | | | | | | | | | | | | | | | | | | | |  | | | |  | | | |  | | | |
|  | |  | |  | |  | |  | |  | |  | | |  | |  | | 158 Sft | | | | 1507.66 | | | | P.Sft | | | | 238210/- | | | |
| 10 | | Supplying & fixing in position Aluminum channels framing for slidding windows & ventilators of Alcop made with 5 mm thick tinted glass glazing (Belgium) & Aluminums fly screen I/c handles stoppers & locking arrangement etc. complete.(S.I NO: 84 (b)P-108) | | | | | | | | | | | | | | | | | | | | |  | | | |  | | | |  | | | |
|  | |  | |  | |  | |  | |  | |  | | |  | |  | | 120 Sft | | | | 1647.69 | | | | P.Sft | | | | 197723/- | | | |
| 11 | | Cement plaster 1:6 upto 12' height.(b) 1/2" thick. (S.I NO: 13 P-52) | | | | | | | | | | | | | | | | | | | | |  | | | |  | | | |  | | | |
|  | |  | | Net: Qty: 8707 (-) 553 | | | | | | | | | | | | |  | | **8154** | | | | 2206.60 | | | | % Sft | | | | 179926/- | | | |
| 12 | | Add Extra labour for 1st Floor Cement Plaster 1:6 | | | | | | | | | | | | | | | | | | | | |  | | | |  | | | |  | | | |
|  | |  | |  | |  | |  | |  | |  | | |  | |  | | 8154 Sft | | | | 286.85 | | | | % Sft | | | | 23390/- | | | |
|  | |  | |  | |  | |  | |  | |  | | |  | |  | |  | | | |  | | | |  | | | |  | | | |
| 13 | | Cement plaster 1:4 upto 12' height.(b) 3/8" thick. (S.I NO: 13 P-52) | | | | | | | | | | | | | | | | | | | | |  | | | |  | | | |  | | | |
|  | |  | |  | | | | | | | | | | | | | | |  | | | |  | | | |  | | | |  | | | |
|  | |  | |  | |  | |  | |  | |  | | |  | |  | | 8154 Sft | | | | 2197.52 | | | | % Sft | | | | 179186/- | | | |
| 14 | | Add Extra labour for 1st Floor Cement Plaster 1:4 | | | | | | | | | | | | | | | | | | | | |  | | | |  | | | |  | | | |
|  | |  | |  | | | | | | | | | | | | | | |  | | | |  | | | |  | | | |  | | | |
|  | |  | |  | |  | |  | |  | |  | | |  | |  | | 8154 Sft | | | | 285.67 | | | | % Sft | | | | 23294/- | | | |
| 15 | | Laying white marble flooring fine dressed on the surface without winding set in lime mortar 1:2 including rubbing and polishing of the joints.(S.I NO: 28 P.NO: 43) | | | | | | | | | | | | | | | | | | | | |  | | | |  | | | |  | | | |
|  | |  | |  | |  | |  | |  | |  | | |  | |  | | 1524 Sft | | | | 567.48 | | | | P.Sft | | | | 864840/- | | | |
| 16 | | Providing and fixing 3/8" thick marble tiles of approved quality and colour and shade size 8" x 4" /6" x 4" in dado skirting anf facing removal /tucking of existing plaster surface ete. Over 1/2" thick base of cement mortar 1:3 setting of tiles in slurry of white cement over mortar base including filling the joints and washing the tiles with white cement slurry , currint finishing, cleaning and ploishing etc. complete.(S.I NO: 68 P.NO: 49)0 | | | | | | | | | | | | | | | | | | | | |  | | | |  | | | |  | | | |
|  | |  | |  | | | | | | | | | | | | | | | 405 Sft | | | | 186.09 | | | | P.Sft | | | | 75366/- | | | |
| 17 | | Laying floor of approved with glazed tile 1/4" thick in white cement 1:2 over 3/4" thick cement mortar 1:2 complete.(S.I NO: 24 P.NO: 43) | | | | | | | | | | | | | | | | | | | | |  | | | |  | | | |  | | | |
|  | |  | |  | |  | |  | |  | |  | | |  | |  | |  | | | |  | | | |  | | | |  | | | |
|  | |  | |  | |  | |  | |  | |  | | |  | |  | | 135 Sft | | | | 27678.86 | | | | % Sft | | | | 37366/- | | | |
| 18 | | White glazed tiles 1/4" thick dado jointed in white cement and laid over 1:2 cement sand mortar 3/4" thick including finishing.(S.I NO: 37 P.NO: 45) | | | | | | | | | | | | | | | | | | | | |  | | | |  | | | |  | | | |
|  | |  | |  | | | | | | | | | | | | |  | | 352 Sft | | | | 28253.61 | | | | % Sft | | | | 99453/- | | | |
|  | |  | |  | |  | |  | |  | |  | | |  | |  | |  | | | |  | | | |  | | | |  | | | |
| 19 | | Supplying and fixing false cailing of plaster of paris, in pannels including making frame , work of Deodar wood including painting with Soligia paint. (S.I NO: 52 P-64) | | | | | | | | | | | | | | | | | | | | |  | | | |  | | | |  | | | |
|  | |  | |  | |  | |  | |  | |  | | |  | |  | | 1198 Sft | | | | 25293.42 | | | | % Sft | | | | 303015/- | | | |
| 20 | | | Providing & fixing plaster of Paris ceiling border of 8" -10 " with of specified design & thickness I/c fixing besides ceiling with nails/ screws with jetties.(S.I NO: 44 P-39) | | | | | | | | | | | | | | | | | | | | | |  | | | |  | | | |  | | | |
|  | | |  | |  | |  | |  | |  | |  | | |  | |  | | | 394 Sft | | | | 104.22 | | | | P.Rft | | | | 41063/- | | | |
|  | | |  | |  | |  | |  | |  | |  | | |  | |  | | |  | | | |  | | | |  | | | |  | | | |
| 21 | | | Preparing the surface and painting with matt finish I/c rubbing the surface with Bathy (silicon carbide rubbing brick) filling the voids with zink /chalk / plaster of paris mixture, applying first coat premix, making the surface smooth and then painting 3 coats with matt finish of approved make etc: complete .(new surface).(S.I NO: 36(A) P-55) | | | | | | | | | | | | | | | | | | | | | |  | | | |  | | | |  | | | |
|  | | |  | |  | | | | | | | | | | |  | |  | | | 4116 Sft | | | | 3444.38 | | | | % Sft | | | | 141771/- | | | |
|  | | |  | |  | | | | | | | | | | |  | |  | | |  | | | |  | | | |  | | | |  | | | |
| 22 | | | PrePreparing the surface and painting with weather coat I/c rubbing the surface with rubbing brick / sand Paper, filling the voids with chalk/ plaster of Paris and then painting with weather coat of approved make.(S.I NO: 38 P.NO: 56)paring the surface and painting with weather coat I/c rubbing the surface with rubbing brick / sand Paper, filling the voids with chalk/ plaster of Paris and then painting with weather coat of approved make.(S.I NO: 38 P.NO: 56) | | | | | | | | | | | | | | | | | | | | | |  | | | |  | | | |  | | | |
|  | | |  | |  | | | | | | | | | | | | | | | | 4734 Sft | | | | 2567.95 | | | | % Sft | | | | 121567/- | | | |
| 23 | | | Providing and laying 1" thick topping cement concrete (1:2:4 ) including Surface finishing and dividing into panels:(S.I NO" 16 (c)P-42) 2" thick | | | | | | | | | | | | | | | | | | | | | |  | | | |  | | | |  | | | |
|  | | |  | |  | |  | |  | |  | |  | | |  | |  | | |  | | | |  | | | |  | | | |  | | | |
|  | | |  | |  | |  | |  | |  | |  | | |  | |  | | | 2523 Sft | | | | 3275.50 | | | | % Sft | | | | 82635/- | | | |
| 24 | | | Preparing the surface and painting with weather coat I/c rubbing the surface with rubbing brick / sand Paper, filling the voids with chalk/ plaster of Paris and then painting with weather coat of approved make.(S.I NO: 38 P.NO: 56) | | | | | | | | | | | | | | | | | | | | | |  | | | |  | | | |  | | | |
|  | | |  | |  | |  | |  | |  | |  | | |  | |  | | |  | | | |  | | | |  | | | |  | | | |
|  | | |  | |  | | | | | | | | | | | | | | | | 2346 Sft | | | | 2567.95 | | | | % Sft | | | | 60244/- | | | |
| 25 | | | PNS, Painting Doors and Windows any type including edges three coats ( S.I NO: 4 P-76) | | | | | | | | | | | | | | | | | | | | | |  | | | |  | | | |  | | | |
|  | | |  | |  | | | | | | | | | | | | |  | | |  | | | |  | | | |  | | | |  | | | |
|  | | |  | |  | |  | |  | |  | |  | | |  | |  | | | 538 Sft | | | | 2116.41 | | | | % Sft | | | | 11386/- | | | |
| 26 | | | Painting guard bars, gates iron bars gratings , railings including standard braces (etc.) and similar open work.(S.I NO: 1 P.NO: 69) | | | | | | | | | | | | | | | | | | | | | |  | | | |  | | | |  | | | |
|  | | |  | |  | |  | |  | |  | |  | | |  | |  | | |  | | | |  | | | |  | | | |  | | | |
|  | | |  | |  | |  | |  | |  | |  | | |  | |  | | | 84 Sft | | | | 1270.83 | | | | % Sft | | | | 1067/- | | | |
| 27 | | | Supplying & fixing in position Aluminum channels framing for hinged doors or Alcop made with 5 mm thick tinted glass glazing (Belgium) and Alpha (Japan) locks I/c handles, stoppers etc.(S.I NO: 83 (bP-NO: 108) | | | | | | | | | | | | | | | | | | | | | |  | | | |  | | | |  | | | |
|  | | |  | |  | |  | |  | |  | |  | | |  | |  | | |  | | | |  | | | |  | | | |  | | | |
|  | | |  | |  | |  | |  | |  | |  | | |  | |  | | | 126 Sft | | | | 1507.66 | | | | P.Sft | | | | 189965/- | | | |
| 28 | | | Supplying & fixing in position Aluminum channels framing for sliding windows & ventilators of Alcop made with 5 mm thick tinted glass glazing (Belgium) & Aluminum fly screen I/c handles stoppers & locking arrangement etc. complete.(S.I NO: 84 (b)P-108) | | | | | | | | | | | | | | | | | | | | | |  | | | |  | | | |  | | | |
|  | | |  | |  | |  | |  | |  | |  | | |  | |  | | |  | | | |  | | | |  | | | |  | | | |
|  | | |  | |  | |  | |  | |  | |  | | |  | |  | | | 72 Sft | | | | 1647.69 | | | | P.Sft | | | | 118634/- | | | |
|  | | |  | |  | |  | |  | |  | |  | | |  | |  | | |  | | | | ======================== | | | | | | | | | | | |
|  | | |  | |  | |  | |  | |  | |  | | |  | |  | | | **Total** | | | |  | | | |  | | | | **5898638/-** | | | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | NAME OF WORK  **ESTABLISHMENT OF ARCHIVES OFFICE KHAIRPUR.** | | | | | | | | | | | | | |
|  | **W/S & S/F** | | | | | | | |  |  | |  |  | |
| 1 | Providing and fixing orisa type white or colour glazed earthen ware w.c pan with cost of low level plastic flush tank of 3 gallons capacity of approved quality i8/c making requisite number of holes in wall, plainth & floor and making good in cement concrete 1: 2: 4.With 4" dia earthen ware trap and plastic thumble. | | | | | | | |  |  | |  |  | |
|  |  |  |  |  |  |  |  |  | 6 Nos | 6166.6 | | each | 37000 | |
| 2 | Providing & fixing steel sinks stainless local make complete with cast iron or wraught iron brackets 6 inches built in wall, 1-1/2" c.p bubber plug chrome plated brass chain, 1-1/2" c.p brass waste, with 1-1/2" P.V.C. waste pipe & making requisite number of holes in wall & plinth & floor for pipe connection & making good in cement concrete 1 : 2: 4.Steel sink stainless sized 33" x 18" local make (Standard Pattern.) | | | | | | | |  |  | |  |  | |
|  |  |  |  |  |  |  |  |  | 02 Nos | 5712.3 | | each | 11425 | |
|  |  |  |  |  |  |  |  |  |  |  | |  |  | |
| 3 | Supplying & Fixnig in position brass bib cock 1/2" dia ( S.I NO: 1 (b) P.NO: 16) | | | | | | | |  |  | |  |  | |
|  |  |  |  |  |  |  |  |  | 20 Nos | 348.92 | | each | 6978 | |
| 4 | Supplying & Fixnig in position brass bib cocks 1/2" dia Standard pattern ( S.I NO: 1 (b) P-15) | | | | | | | |  |  | |  |  | |
|  |  |  |  |  |  |  |  |  | 08 Nos | 337.92 | | each | 2703 | |
| 5 | Providing & Fixing 4" Dia C.I soil & vent Pipe including cutting and fitting and extra painting to match the colour of building ( S.I NO: 1 P-8) | | | | | | | |  |  | |  |  | |
|  |  |  |  |  |  |  |  |  | 72 Rft | 333.29 | | P.Rft | 23997 | |
| 6 | Supplying & Fixing Bath Room accessories set (7pics) including towel rod, brush holder, soap tray, shelf of approved quality design etc complete ( S.I NO: 22 P-19) | | | | | | | |  |  | |  |  | |
|  |  |  |  |  |  |  |  |  | 06 Nos | 10322.4 | | each | 61934 | |
| 7 | Providing G.I Pipes, specials, and clamps etc, including fixing cutting & fitting complete with and I/c the cost of breaking thorugh walls and roof, making good etc. painting two coats after cleaning the Pipe etc. with white zink paint with pigment to match the colour5 of the building and testing with water to a pressure head of 200 feet and handling. | | | | | | | |  |  | |  |  | |
|  | 1" Dia |  |  |  |  |  |  |  | 500 Rft | 128.55 | | P.Rft | 64275 | |
|  | 3/4" Dia |  |  |  |  |  |  |  | 500 Rft | 95.79 | | P.Rft | 47895 | |
|  | 1" Dia |  |  |  |  |  |  |  | 140 Rft | 73.21 | | P.Rft | 10249 | |
| 8 | Providing & fixing in position nyloon connections complete with 1/2" dia, brass stop cock with pair of brass nuts and lining joints to nyloon connection. | | | | | | | |  |  | |  |  | |
|  |  |  |  |  |  |  |  |  | 16 Nos | 447.15 | | each | 7154 | |
| 10 | Providing and Fixing handle valves (China) ( S.I NO: 5P-16 | | | | | | | |  |  | |  |  | |
|  | 1" Dia |  |  |  |  |  |  |  | 08 NOs | 365.42 | | each | 2923 | |
|  | 3/4" Dia |  |  |  |  |  |  |  | 14 Nos | 271.92 | | each | 3807 | |
|  | 1" Dia |  |  |  |  |  |  |  | 12 Nos | 200.42 | | each | 2405 | |
|  |  |  |  |  |  |  |  |  |  |  | |  |  | |
| 11 | Providing & fixing 24" x 18" lavatory basin in white glazed earthen ware complete with & I/c the cost of W.I or C.I cantilever brackets 6 inches built into wall, painted white in two coast after a primary coat of red lead paint, a pair of 1/2" dia rubber plug & chrome plate brass chain 1-1/4" dia malloable iron or c.P brass traps malloable iron or brass unions and making requisite number of holes in walls, plinth & floor for pipe connection and making good in cement concrete 1: 2: 4 (Standard pattern). | | | | | | | | |  |  | | |
|  |  |  |  |  |  |  |  |  | 06 Nos | 4253.9 | | each | 25523 | |
| 12 | Add extra for labour for providing & fixing of earthen ware pedestal white or coloured glazed (Foreign or Equivalent..) | | | | | | | |  |  | |  |  | |
|  |  |  |  |  |  |  |  |  | 06 Nos | 938.47 | | each | 5631 | |
|  | Providing & fixing 6" x 2" or 6" x 3" C.I floor trap of the approved selt cleaning design with a C.I screwed down grating with or without a vent arm complete with & I/c making requisite number of holes in walls, plinth & floor for Pipe connections & making good cement concrete 1:2:4. | | | | | | | | |  | |  |  | |
|  |  |  |  |  |  |  |  |  | 14 Nos | 2042.43 | | each | 28594 | |
| 14 | Providing & fixing 4" dia. C.I plain bend of the required degree including extra painting to match the colour of the building. | | | | | | | |  |  | |  |  | |
|  |  |  |  |  |  |  |  |  | 12 NOs | 566.7 | | each | 6800 | |
| 15 | Construction of manhole or inspection chamber for the required dia of circular sewer and 3’-6’ (1067 mm ) depth with walls of B.B in cement mortar 1:3 cement plaster 1:3 ½” thick in side 1” (25 mm ) thick over beching and channel i/c fixing C.I main hole cover with frame of clear opening 1 ½”x 1 ½”” 457x457 mm) of 1.75 cwt . (88.9 kg) embedded in plain c.c 1:2:4) & fixing (25 mm) dia M.S steps 6” 150 mm) white projecting 4” (102 mm) from the face of walls at 12” (305 mm) c/c duly painted etc complete as per standard specification & drawing.(S.I No- P-46). | | | | | | | | |  | |  |  | |
|  |  |  |  |  |  |  |  |  | 03 Nos | 14748 | | each | 44244 | |
| 16 | Providing Laying RCC pipes & Collars of Class "B" and fixing in trench including cutting, fitting, & jointing with maxphalt composition and cement mortar (1:1) including testing with water to head of 22.5 meter or 75 ft: ( S.I NO: 2 P-16). | | | | | | | | |  | |  |  | |
|  |  |  |  |  |  |  |  |  | 250 Rft | 534.8 | | P.Rft | 133700 | |
| 17 | Providing & fixing M.S clamps of the approved design to 4" dia C.I Pipe sockets including the cost of cutting and making good to wall or M.S bolts and nuts, 4" into wall including Pipe distance Pieces extra painting to match the colour of the building. | | | | | | | |  |  | |  |  | |
|  |  |  |  |  |  |  |  |  | 12 Nos | 72.16 | | each | 866 | |
| 18 | Providing & fixing 4" x 4" x4" dia. C.I branched of the required degree with access doors, rubber washer 1/8" thick and bolts and nuts and extra painting to match colour of the building. | | | | | | | |  |  | |  |  | |
|  |  |  |  |  |  |  |  |  | 12 Nos | 72.16 | | each | 866 | |
| 19 | S/F Fiber glass tank of approved quality and design and wall thickness as specified i/c cost bolts and fixing in plate form of cement concrete (1:3:6) and making connection for in-let & out let & over flow pipes etc complete. (a)250 gallons wall thickness 3.5 mm. | | | | | | | |  |  | |  |  | |
|  |  |  |  |  |  |  |  |  | 03 Nos | 37505 | | each | 112515 | |
|  |  |  |  |  |  |  |  |  | ==================================== | | | | | |
|  |  |  |  |  |  |  |  |  | Total |  | |  | 707484/- | |
|  |  |  |  |  |  |  |  |  |  |  | |  |  | |
|  |  |  |  |  |  |  |  |  |  |  | |  |  | |
|  |  |  |  |  |  |  |  |  |  |  | |  |  | |
|  |  |  |  |  |  |  |  |  |  |  | |  |  | |

CONTRACTOR EXECUTIVE ENGINEER

PROVINCIAL BUILDINGSDIVISION

. SHAHEED BENAZIR ABAD