**SCHEDULE-B M/R TO CENTRAL JAIL KHAIRPUR (Repair of suptdd: b’low**).

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **S.NO** | **NAME OF WORK** | **NO:L.B.D** | **QTY:** | **RATE** | **UNIT** | **AMOUNT** |

01/- laying floors of approved coloured glazed tiles 1/4" thick laid in white cement and pigment on a bed of 3/4" thick cement mortar 1:2. (S.I NO: 25 P.NO: 4)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | Total | = | 462 | Sft | 27678.86 | % Sft | 127876/- |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 02 | Laying white marble flooring fine dressed on the surface without winding set in lime mortar 1:2 including rubbing and polishing of the joints.(S.I NO: 28 P.NO: 43) | | | | |  | |  | |  |  | |
|  |  |  | = | 800 | “ | | 567.48 | | P.Sft | | | 453984/- |
|  |  |  |  |  |  | |  | |  | | |  |
| 03 | Supplying and fixing false ceiling of plaster of Paris, in panels including making frame , work of Deodar wood including painting with Soligia paint. (S.I NO: 52 P-64) | | | |  | |  | |  | | |  |
|  |  |  | = | 580 | “ | | 25293.42 | | % Sft | | | 146702/- |
| 04 | Providing & fixing plaster of Paris ceiling border of 8" -10 " with of specified design & thickness I/c fixing besides ceiling with nails/ screws with jetties.(S.I NO: 44 P-39) | | | |  | |  | |  | | |  |
|  |  |  | = | 193 | “ | | 104.22 | | P.Rft | | | 20114/- |
|  |  |  |  |  |  | |  | |  | | |  |
| 05 | Preparing the surface and painting with matt finish I/c rubbing the surface with Bathy (silicon carbide rubbing brick) filling the voids with zink /chalk / plaster of paris mixture, applying first coat premix, making the surface smooth and then painting 3 coats with matt finish of approved make etc: complete .(new surface).(S.I NO: 36) | | | |  | |  | |  | | |  |
|  |  |  |  |  |  | |  | |  | | |  |
|  |  |  | = | 5011 | Sft | | 2717/- | | % Sft | | | 136149/- |
|  |  |  |  |  |  | |  | |  | | |  |
| 06 | Distempering 02 coats (S.I NO: P.NO: ) | | |  |  | |  | |  | | |  |
|  |  |  | = | 2860 | Sft | | 1043.90 | | % Sft | | | 29856/- |
| 07/- | Panting New Surface Painting Doors & Windows any type 03 coats (S.I NO: P.NO: ). | | | |  | |  | |  | | |  |
|  |  |  | = | 563 | “ | | 1489.68 | | % Sft | | | 8387/- |
|  |  |  |  |  |  | |  | |  | | |  |
| 08/- | Removing Cement or lime plaster (S.I NO: P.NO: ) | | | |  | |  | |  | | |  |
|  |  |  | = | 2080 | Sft | | 121/- | | % Sft | | | 2517/- |
|  |  |  |  |  |  | |  | |  | | |  |
| 09/- | Pacca brick work in ground floor in:(e) Cement sand mortar. 1:6(S.I NO: 5 P-21) | | | | | |  | |  | | |  |
|  |  |  | = | 305 | “ | | 12674.36 | | % Cft | | | 38657/- |
|  |  |  |  |  |  | |  | |  | | |  |
| 10/- | Applying floating coat of Cement 1/32" thick.(S.I NO: 14 P-53) | | | | | |  | |  | | |  |
|  |  |  |  |  |  | |  | |  | | |  |
|  |  |  | = | 2080 | Sft | | 660/- | | % Sft | | | 13728/- |
|  |  |  |  |  |  | |  | |  | | |  |
| 11/- | Cement plaster 1:6 upto 12' height.(b) 1/2" thick. (S.I NO: 13 P-52) | | | |  | |  | |  | | |  |
|  |  |  |  |  |  | |  | |  | | |  |
|  |  |  | = | 2080 | Sft | | 2206.60 | | % Sft | | | 45897/- |
| 12 | Cement plaster 1:4 upto 12' height.(b) 3/8" thick. (S.I NO: 13 P-52) | | | |  | |  | |  | | |  |
|  |  |  |  |  |  | |  | |  | | |  |
|  |  | = | =================================== | | | | | | | | | |
|  |  |  |  | **Total** | | |  | |  | | | **1069575** |
|  |  |  |  |  |  | |  | |  | | |  |

**PART-C- NON SHEDULE ITEM**

01/- P/F UPVC pipe ¾” dia PAK-ARAB) SCH-40 surface by using clip /saddler/socket/reducer/bush/tee / elbow etc .or recessed in masonry C.C or R.C.C upto 20’ ft. height and making good with c.c i/c curing finishing etc complete as per instruction of the Engineer In charge ,.Specification of the material should meet the requirement of class 12454-Bin accordance with the ASTM-D-1784 type 1 Grade 1. rate include all costs of labor ,material, cartage scaffolding ladders .etc complete (R.A Sanction).

¾” Dia

4” Dia

Qty: 100 rft @Rs: 290/- P.rft RS: 29000/-

============================

Total RS: 29000/-

CONTRACTOR EXECUTIVE ENGINEER

PROVINCIAL BUILDINGSDIVISION

. SHAHEED BENAZIR ABAD