SCHEDULE-B **CONSTRUCTION OF COMPOUND WALL FOR MANDER & DARBAR BASAR FAKER U/C RAHEEM BUX WASSAN TALUKA KOT DIJI DISTRICT KHAIRPUR.**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO | ITEM OF WORK | NO:L.B.D |  | QTY |  | RATE | UNIT | AMOUNT |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 01 | Excavation in foundation of Building Bridges and other structures including dag belling dressing, refilling around structure with excavated earth Watering and ramming lead upto 5 ft.(S.I NO: 18 P.NO: 4) | | | | | |  |  |
|  |  |  | = | 1000 | “ | 3176.25 | %0Cft | 3176/- |
|  |  |  | Thirty one hundreds seventy six rups twenty five ps: | | | | |  |
| 02 | Cement concrete brick or stone ballast 1 1/2" to 2" gauge.1:5:10 (S.I NO: 4 (e)P.NO: 15) | | | | | |  |  |
|  |  |  | = | 250 | “ | 8694.95 | %Cft | 21737/- |
|  |  |  |  | Eighty six hundreds ninety four rups ninety five ps: | | | |  |
| 03 | Random, rubble masonry (uncaused )Ratio 1:6 (S.I NO: 1 (iv)P.NO: 27) | | | | | |  |  |
|  |  |  | = | 563 | Cft | 17723/- | % Cft | 99780/- |
|  |  |  |  | Seventeen thousands seven hundreds twenty three rupees. | | | |  |
| 04 | Coursed Ruble masonry including hammer dressing.Ratio 1:6 (S.I NO: 2 P-NO: 27) | | | | | |  |  |
|  |  |  | = | 424 | Cft | 25321/- | % CFt | 107361/- |
|  |  |  |  | Twenty five thousands three hundreds twenty one rupes: | | | |  |
| 05 | R.C.C work in roof slab, beams columns rafts, lintels and other structural members laid in situ or precast laid in position complete in all respects. Ratio (1 : 2: 4 ) 90 Lbs. cement 2 Cft. Sand 4 Cft. Shingle 1/8" to 1/4" gauge.(S.I NO: 6 (a)P-16) | | | | | |  |  |
|  |  |  | = | 141 | Cft | 337/- | P.Cft | 47517/- |
|  |  |  |  | Three hundred thirty seven rupes | | | |  |
| 06 | Fabrication of mild steel reinforcement for cement concrete including cutting, bending, lying in position, making joints and fastenings including cost of binding wire (also includes removal of rust from bars.)(S.I NO: 8 P.NO: 17 | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 6.294 | cwt | 5001.70 | P.cwt | 31480/- |
|  |  |  |  | Five thousands one rupees seventy ps: | | | |  |
| 07 | Pacca brick work in Other than Building 1:6 in Cement sand mortar 1:6(S.I NO: 4 ( )P: NO: 20) | | | | | |  |  |
|  |  |  | = | 826 | Cft | 12346.65 | % Cft | 101983/- |
|  |  |  | Twelve thousands three hundreds fourty six rups: sixty five ps: | | | | |  |
| 08 | Cement plaster 1:6 upto 12' height.(b) 1/2" thick. (S.I NO: 13 P-52) | | | | | | |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 1402 | Sft | 2206.60 | % SFt | 16991/- |
|  |  |  | Twenty two hundreds six rupees sixty ps: | | | | |  |
| 09 | Cement plaster 1:4 upto 12' height.(b) 3/8” thick. (S.I NO: 13 P-52) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 1402 | Sft | 2197.52 | % Sft | 30809/- |
|  |  |  | Twenty one hundreds ninty seven rupees fifty two ps: | | | | |  |
| 10 | Cement pointing struck joints on walls 1:2.(S.I NO: 19 (a) P-53) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 937 | Sft | 1213.58 | % Sft | 11371/- |
|  |  |  |  | Twelve hundreds thirteen rupees fifty eight ps: | | | |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO | ITEM OF WORK | NO:L.B.D |  | QTY |  | RATE | UNIT | AMOUNT |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 11 | Colour washing two coats (S.I NO: 25 P-54) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 2339 | Sft | 859.90 | % Sft | 20113/- |
|  |  |  |  | Eight hundred fifty nine rupees ninty ps: | | | |  |
|  |  |  |  |  |  | ======================== | | |
|  |  |  |  | **Total** |  |  |  | **506264/-** |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR

**PART-B (Darbar Basar Fakir Main Building)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO | ITEM OF WORK | NO:L.B.D |  | QTY |  | RATE | UNIT | AMOUNT |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 01 | Excavation in foundation of Building Bridges and other structures including dag belling dressing, refilling around structure with excavated earth Watering and ramming lead upto 5 ft.(S.I NO: 18 P.NO: 4) | | | | | |  |  |
|  |  |  | = | 646 | “ | 3176.25 | %0Cft | 2052/- |
|  |  |  | Thirty one hundreds seventy six rups twenty five ps: | | | | |  |
| 02 | Cement concrete brick or stone ballast 1 1/2" to 2" gauge.1:6:12 (S.I NO: 4 (e)P.NO: 15) | | | | | |  |  |
|  |  |  | = | 192 | “ | 8122.95 | %Cft | 15596/- |
|  |  |  |  | Eighty six hundreds ninety four rups ninety five ps: | | | |  |
| 03 | R.C.C work in roof slab, beams columns rafts, lintels and other structural members laid in situ or precast laid in position complete in all respects. Ratio (1 : 2: 4 ) 90 Lbs. cement 2 Cft. Sand 4 Cft. Shingle 1/8" to 1/4" gauge.(S.I NO: 6 (a)P-16) | | | | | |  |  |
|  |  |  | = | 843 | Cft | 337/- | P.Cft | 284091/- |
|  |  |  |  | Three hundred thirty seven rupes | | | |  |
| 04 | Fabrication of mild steel reinforcement for cement concrete including cutting, bending, lying in position, making joints and fastenings including cost of binding wire (also includes removal of rust from bars.)(S.I NO: 8 P.NO: 17 | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 37.633 | cwt | 5001.70 | P.cwt | 188229/- |
|  |  |  |  | Five thousands one rupees seventy ps: | | | |  |
| 05 | Random, rubble masonry (uncaused )Ratio 1:6 (S.I NO: 1 (iv)P.NO: 27) | | | | | |  |  |
|  |  |  | = | 76 | Cft | 17723/- | % Cft | 13469/- |
|  |  |  |  | Seventeen thousands seven hundreds twenty three rupees. | | | |  |
| 06 | Pacca brick work in Ground Floor 1:6 in Cement sand mortar 1:6(S.I NO: 4 ( )P: NO: 20) | | | | | |  |  |
|  |  |  | = | 676 | Cft | 12674.36 | % Cft | 85679/- |
|  |  |  | Twelve thousands Six hundreds seventy six rupees thirty six s: | | | | |  |
| 07 | Providing and fixing G.I frames /Choukhats of size 7" x 2" or 4 1/2" x 3" for Door using 20 gauge G.I sheet I/c welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage , tools and plants used in making and fixing.(CSI NO: 28 P-93) | | | | | |  |  |
|  |  |  | = | 18 | Rft | 228.90 | P.Rft | 4120/- |
|  |  |  |  | Two hundred twenty eight rupees ninty ps: | | | |  |
| 08 | Providing and fixing G.I frames /Choukhats of size 7" x 2" or 4 1/2" x 3" for windows using 20 gauge G.I sheet I/c welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage , tools and plants used in making and fixing.(CSI NO: 28 P-93) | | | | | |  |  |
|  |  |  | = | 74 | Rft | 240.50 | P.Rft | 17797/- |
|  |  |  |  | Two hundreds forty rupees fifty ps: | | | |  |
| 09 | First class deodar wood wrought, joinery in doors and windows etc, fixxed in position including chowkats hold fasts hinges, iron tower bolts, chocks cleats, handles and cords with hooks, etc.(1 3/4" thick)(S.I NO: 7 P-58) | | | | | |  |  |
|  |  |  | = | 71 | Sft | 902.93 | P.Sft | 64108/- |
|  |  |  |  | Nine hundreds two rupes ninty three ps: | | | |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO | ITEM OF WORK | NO:L.B.D |  | QTY |  | RATE | UNIT | AMOUNT |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 10 | Cement plaster 1:6 upto 12' height.(b) 1/2" thick. (S.I NO: 13 P-52) | | | | | | |  |
|  |  |  | = | 2043 | Sft | 2206.60 | % SFt | 45081/- |
|  |  |  | Twenty two hundreds six rupees sixty ps: | | | | |  |
| 11 | Cement plaster 1:4 upto 12' height.(b) 3/8” thick. (S.I NO: 13 P-52) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 2043 | Sft | 2197.52 | % Sft | 44895/- |
|  |  |  | Twenty one hundreds ninty seven rupees fifty two ps: | | | | |  |
| 12 | Supplying and filling sand under floor and plugging in walls.(S.I NO: 29 P-26) | | | | | |  |  |
|  |  |  | = | 338 | Cft | 1141.25 | % CFt | 3857/- |
|  |  |  | Eleven hundreds forty one rupes twenty five ps: | | | | |  |
| 13 | Cement concrete plain including placing compacting, finishing and curing, complete (including screening and washing at stone aggregate without shuttering. (S.I NO: 5 (i)P-16) Ratio 1:3:6 | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 27 | Cft | 12695/- | % Cft | 3428/- |
|  |  |  |  | Fourteen thousands four hundreds twenty nine | | | |  |
| 14 | Laying white marble flooring fine dressed on the surface without winding set in lime mortar 1:2 including rubbing and polishing of the joints.(S.I NO: 28 P.NO: 43) | | | | | |  |  |
|  |  |  | = | 174 | Sft | 567.48 | P.Sft | 298742/- |
|  |  |  | Five hundred sixty seven rupees fourty eight ps: | | | | |  |
| 15 | Providing and fixing 3/8" thick marble tiles of approved quality and colour and shade size 8" x 4" /6" x 4" in dado skirting anf facing removal /tucking of existing plaster surface ete. Over 1/2" thick base of cement mortar 1:3 setting of tiles in slurry of white cement over mortar base including filling the joints and washing the tiles with white cement slurry , currint finishing, cleaning and ploishing etc. complete.(S.I NO: 68 P.NO: 49) | | | | | |  |  |
|  |  |  | = | 79 | Sft | 186.04 | P.Sft | 14697/- |
|  |  |  | One hundred eighty six rupees four ps: | | | | |  |
| 16 | Priming coat of chalk distemper.(S.I NO: 23 P.NO: 54) | | | | | |  |  |
|  |  |  | = | 2043 | Sft | 442.75 | P.Sft | 9045/- |
|  |  |  | four hundred fourty two rupees seventy five ps: | | | | |  |
| 17 | Distempering 02 two coats | | | | | |  |  |
|  |  |  | = | 2043 | Sft | 1043.90 | % Sft | 21327/- |
|  |  |  | One thousand fourty three rupees ninty ps: | | | | |  |
| 18 | Painting Door & Windows any type 02 coats (S.I NO: P.NO: ) | | | | | |  |  |
|  |  |  | = | 142 | Sft | 2116.41 | % Sft | 3005/- |
|  |  |  | Twenty one hundred sixteen rupees fourty one ps: | | | | |  |
|  |  |  |  |  |  | ======================== | | |
|  |  |  |  | **Total** |  |  |  | **919218/-** |

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO | ITEM OF WORK |  |  | QTY |  | RATE | UNIT | AMOUNT |

**PART-A (ii) Catt:**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 01 | Supplying and filling sand under floor and plugging in walls.(S.I NO: 29 P-26) | | | | | |  |  |
|  |  |  | = | 2957 | Cft | 1141.25 | % CFt | 33747/- |
|  |  |  |  | Eleven hundreds forty one rupes twenty five ps: | | | |  |
| 02 | Add: Extra for Lead 3-0 Miles | | | | | |  |  |
|  |  |  | = | 2957 | Cft | 579.41 | % Cft | 17148/- |
|  |  |  |  | Five hundreds seventy nine rupees fourty one ps: | | | |  |
| 03 | Cement concrete brick or stone ballast 1 1/2" to 2" gauge.1:6:12 (S.I NO: 4 (e)P.NO: 15) | | | | | |  |  |
|  |  |  | = | 976 | Cft | 8122.95 | % Cft | 79280/- |
|  |  |  | Eighty one hundred twenty two rupees ninty five ps: | | | | |  |
| 04 | Cement concrete plain including placing compacting, finishing and curing, complete (including screening and washing at stone aggregate without shuttering. (S.I NO: 5 (i)P-16) Ratio 1:2:4 | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 503 | Cft | 14429.25 | % Cft | 72579/- |
|  |  |  |  | Fourteen thousands four hundreds twenty nine rups: twenty five ps: | | | |  |
|  |  |  |  |  |  | ======================== | | |
|  |  |  |  | **Total** |  |  |  | **202754/-** |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G. Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities and rates may be changed as per/according to the Technical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR

PART:- wash room

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO | ITEM OF WORK | NO:L.B.D |  | QTY |  | RATE | UNIT | AMOUNT |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 01 | Excavation in foundation of Building Bridges and other structures including dag belling dressing, refilling around structure with excavated earth Watering and ramming lead upto 5 ft.(S.I NO: 18 P.NO: 4) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 214 | “ | 3176.25 | %0Cft | 680/- |
|  |  |  | Thirty one hundreds seventy six rups twenty five ps: | | | | |  |
| 02 | Cement concrete brick or stone ballast 1 1/2" to 2" gauge.1:5:10 (S.I NO: 4 (e)P.NO: 15) | | | | | |  |  |
|  |  |  | = | 54 | “ | 8694.95 | %Cft | 4695/- |
|  |  |  | Eighty six hundreds ninety four rups ninety five ps: | | | | |  |
| 03 | Random, rubble masonry (uncaused )Ratio 1:6 (S.I NO: 1 (iv)P.NO: 27) | | | | | |  |  |
|  |  |  | = | 122 | Cft | 17723/- | % Cft | 21622/- |
|  |  |  |  | Seventeen thousands seven hundreds twenty three rupees. | | | |  |
| 04 | Coursed Ruble masonry including hammer dressing.Ratio 1:6 (S.I NO: 2 P-NO: 27) | | | | | |  |  |
|  |  |  | = | 93 | Cft | 25321/- | % CFt | 23549/- |
|  |  |  |  | Twenty five thousands three hundreds twenty one rupes: | | | |  |
| 05 | R.C.C work in roof slab, beams columns rafts, lintels and other structural members laid in situ or precast laid in position complete in all respects. Ratio (1 : 2: 4 ) 90 Lbs. cement 2 Cft. Sand 4 Cft. Shingle 1/8" to 1/4" gauge.(S.I NO: 6 (a)P-16) | | | | | |  |  |
|  |  |  | = | 41 | Cft | 337/- | P.Cft | 13817/- |
|  |  |  | Three hundred thirty seven rupes | | | | |  |
| 06 | Fabrication of mild steel reinforcement for cement concrete including cutting, bending, lying in position, making joints and fastenings including cost of binding wire (also includes removal of rust from bars.)(S.I NO: 8 P.NO: 17 | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 1.83 | cwt | 5001.70 | P.cwt | 9153/- |
|  |  |  | Five thousands one rupees seventy ps: | | | | |  |
| 07 | Pacca Brick work in Ground Floor and plinth in Ratio 1:6 (S.I NO: 4 P-24) | | | | | |  |  |
|  |  |  | = | 376 | Cft | 12674.36 | % Cft | 47656/- |
|  |  |  | Twelve thousands Six hundreds seventy four rups: thirty six ps: | | | | |  |
| 08 | Supplying & Fixing R.S Girder (Material Schedule) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 1.928 | cwt | 3850/- | P.cwt | 7423/- |
|  |  |  |  | Thirty eight hundred fifty rupees. | | | |  |
| 09 | Supplying & Fixing R.S T-Iron (Material Schedule) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 1.571 | cwt | 3575/- | P.cwt | 5616/- |
|  |  |  |  | Thirty five hundreds seventy five ps: | | | |  |
| 10 | Second class tile roofing consisting of 4" earth and 1" mud plaster with Gobri leaping over 1/2"thick cement plaster 1:6 with 34 Lbs. Of hot bitumen coating sand blinded, provided over one layer of 12" x 6"x2" tiles laid in 1:6 cement mortar including 1:2 cement pointing under neath of tiles complete including curing etc.(S.I NO: 2 P-33) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 117 | Sft | 7607.25 | % Sft | 8900/- |
|  |  |  |  | Seventy six hundreds seven rupees twenty five ps: | | | |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO | ITEM OF WORK |  |  | QTY |  | RATE | UNIT | AMOUNT |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 11 | Supplying and filling sand under floor and plugging in walls.(S.I NO: 29 P-26) | | | | | |  |  |
|  |  |  | = | 112 | Cft | 1141.25 | % CFt | 1278/- |
|  |  |  |  | Eleven hundreds forty one rupes twenty five ps: | | | |  |
| 12 | Cement concrete brick or stone ballast 1 1/2" to 2" gauge.1:6:12 (S.I NO: 4 (e)P.NO: 15) | | | | | |  |  |
|  |  |  | = | 25 | Cft | 8122.95 | % Cft | 2031/- |
|  |  |  | Eighty one hundred twenty two rupees ninty five ps: | | | | |  |
| 13 | Cement plaster 1:6 upto 12' height.(b) 1/2" thick. (S.I NO: 13 P-52) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 1032 | Sft | 2206.60 | % Sft | 22772/- |
|  |  |  | Twenty two hundreds six rupes sixty ps: | | | | |  |
| 14 | Cement plaster 1:4 upto 12' height.(b) 3/8” thick. (S.I NO: 13 P-52) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 1032 | Sft | 2197.52 | % Sft | 22678/- |
|  |  |  | Twenty One hundreds ninety seven rupes fifty two ps: | | | | |  |
| 15 | Cement concrete plain including placing compacting, finishing and curing, complete (including screening and washing at stone aggregate without shuttering. (S.I NO: 5 (i)P-16) Ratio 1:3:6 | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 13 | Cft | 12695/- | % Cft | 1650/- |
|  |  |  |  | Twelve thousand six hundred ninty five rupees | | | |  |
| 16 | laying floors of approved colored glazed tiles 1/4" thick laid in white cement and pigment on a bed of 3/4" thick cement mortar 1:2. (S.I NO: 25 P.NO: 4) | | | | | |  |  |
|  |  |  | = | 68 | Sft | 27747.06 | % Sft | 18868/- |
|  |  |  | Twenty seven thousands seven hundred forty seven rups: six ps: | | | | |  |
| 17 | Glazed tile dado 1/4" thick laid in pigment over 1:2 cement sand mortar 3/4" thick including finishing.(S.I NO: 38 P-45) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 157 | SFt | 28299.30 | % Sft | 44430/- |
|  |  |  |  | Twenty eight thousands two hundreds ninty nine rupees thirty ps: | | | |  |
| 18 | Priming coat of chalk distemper.(S.I NO: 23 P.NO: 54) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 1032 | Sft | 442.75 | % Sft | 4569/- |
|  |  |  | Four hundred fourty two rupes seventy five ps: | | | | |  |
| 19 | Distempering. Two 02 Coats (S.I NO: 24 P-54) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 1032 | Sft | 1043.21 | % Sft | 10730/- |
|  |  |  | One thousand fourty three rupees twenty one ps: | | | | |  |
| 20 | Providing and fixing G.I frames /Choukhats of size 7" x 2" or 4 1/2" x 3" for door using 20 gauge G.I sheet I/c welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage , tools and plants used in making and fixing.(CSI NO: 29 P-93) | | | | | |  |  |
|  |  |  | = | 65 | Rft | 228.90 | P.Rft | 14879/- |
|  |  |  | Two hundred twenty eight rupees ninety ps: | | | | |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO | ITEM OF WORK |  |  | QTY |  | RATE | UNIT | AMOUNT |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 21 | First class deodar wood wrought, joinery in doors and windows etc, fixed in position including chowkats hold fasts hinges, iron tower bolts, chocks cleats, handles and cords with hooks, etc.(1 3/4" thick)(S.I NO: 7 P-58) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 48 | Sft | 902.93 | P.Sft | 43341/- |
|  |  |  | Nine hundreds two rupes ninty three ps: | | | | |  |
| 22 | Painting Door & Windows any type 02 coats (S.I NO: P.NO: ) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 96 | Sft | 2116.41 | % Sft | 2032/- |
|  |  |  |  | Twenty one hundreds sixteen rupees fourty one ps: | | | |  |
|  |  |  |  |  |  | ======================== | | |
|  |  |  |  | **Total** |  |  |  | **332369/-** |

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

**PART- WATER SUPPLY**

1/- P/F squatting type white glazed of flushing cistern with internal fitting and flush pipe with band and making requisite Nos. of holes in wall plinth & floor for pipe connections and making good in Cement concrete 1:2:4. (A) W.C pan of not less than 23” clear opening between flashing rims and 3 gallons flushing tank. With 4” dia C.I. tape. (S.I.NO.1(A) P.No.1)

Qty: 03 No @RS: 5044.60 each RS: 15134/-

2/- Providing G.I pipes special & clamps etc i/c fixing cutting and fitting complete with and i/c the cost of breaking through walls and roof making good etc painting two coats after cleaning the pipe etc with white zink paint with pigment to match the colour of the building and testing with water to a pressure head of 200 feet and handling. **(Internal)** (i) ½ dia G.I pipe. (S.I.NO.1 (i) P. No.11)

“ “ 1/2” dia Qty: 45 Rft @RS: 73.21 P.Rft RS: 3294/-

“ “ ¾” dia Qty: 60 Rft @RS: 95.79 P.Rft RS: 5717/-

03/- Supplying & fixing Fiber Glass Tank of approved quality and design and wall thickness as specified i/c cost of nuts bolts and fixing in plate form of cement concrete 1:3:6 and making connection for in-let outlet & over flow in-let outlet flow pipes etc. complete. (S.I.No.3 P.No.18) (Rate per gallon Rs: 33/60 for tanks upto capacity of 250 gallons) 200 Gallons

Qty: 01 NO @RS: 21989.16 each RS: 21990/-

04/- Providing R.C.C pipe with collars slass "B" and digging the trenches to required depth & fixing in position including cutting , fitting & jointing with maxphalt composition & cement mortor 1: 1 and testing with water pressure jto a head of 4 feet a bove the top of the heghest pipe & refilling with excavated staff.

Qty: 40 Rft @RS: 113.97 P.Rft RS: 4559/-

05/- Supplying and fixing in position brass bib cocks (b) 1/2" dia brass

bib cock , Standard

Qty: 06 Nos @RS: 337.92 each RS: 2028/-

06/- Construction of manhole or inspection chamber for the required dia of circular sewer and 3’-6’ (1067 mm ) depth with walls of B.B in cement mortar 1:3 cement plaster 1:3 ½” thick in side 1” (25 mm ) thick over benching and channel i/c fixing C.I main hole cover with frame of clear opening 1 ½”x 1 ½”” 457x457 mm) of 1.75 cwt . (88.9 kg) embedded in plain c.c 1:2:4) & fixing (25 mm) dia M.S steps 6” 150 mm) white projecting 4” (102 mm) from the face of walls at 12” (305 mm) c/c duly painted etc complete as per standard specification & drawing.(S.I No- P-46).

Qty:01 Nos @Rs:14748/- each RS: 14748/-

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

7/- P/F 6”x2” or 6”x3” C.I floor trap of the approved self cleaning design with a C.I screwed down gritting with or without a vent arm complete with and i/c making requisite number or holes in walls plinth and floor for pipe connections & making good in CC 1:2:4. (S.I. No. 20 P. No.5)

Qty: 03 NOs @RS: 2024.43 each RS: 6073/-

8/- Supplying and fixing concealed stopcock of superior quality with c.p head ½” dia.(S.I.NO.13 (a) P. No.15)

Qty: 01 No @RS: 889.46 each RS: 889/-

9/- Providing & Fixing Handle valve China

Qty: 02 NOs @RS: 271.92 each RS: 544/-

10/- Providing & fixing 6" x 4" C.C gully trap with 4" outlet complete with 4" thick 1: 2: 4 C.C. for bed & 1/2" thick cement plaster (1:3) to the karb, C.I grating 6" x 6" & C.I cover and frame 12" x 12" (inside) etc. complete.

Qty: 03 NOs @RS: 1193.17 each RS: 3580/-

========================================

Total RS: 18556/-

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR