**SCHEDULE B**

**EARTH FILLINFG OF GRAVE YARD AT VILLAGE AGRA TALUKA GAMBAT DISTRICKHAIRPUR.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **SR#** | **ITEM OF WORKS** | **QTY:** | **RATE** | **UNIT** | **AMOUNT** |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **01.** | Supplying and filling sand under floor plugging inwalls, i/c add extra lead 3miles. (S\_29P-26) | |  |  |  |  |
|  |  |  | **81000** | **1720/66** | **%Cft** | **Rs:1393735/-** |
| **02.** | Dressing and levelling of earth work to designed section , etc complete.(S-11 P-3). | |  |  |  |  |
|  |  |  | **81000** | **187/55** | **%0Cft** | **Rs:13504/-** |
|  |  |  |  |  |  |  |
| **03.** | Making and fixing steel grated doors complete with locking arrangement angle iron frame 2”x2” 3/8”and ¾”sq:bars 4”centre to centre.(S-23 P-91). | |  |  |  |  |
|  |  |  | **1 No:** | **47500/-** | **Each** | **Rs:47500/-** |
|  |  |  |  |  |  |  |
| **04.** | Providing and laying HALA or pattern tiles glazed 6”x6”x1/4” on floor or wall facing in required colour and pattern of STILE specification jointed in white cement and pigment over a base of 1:2 grey cemnt mortar ¾ “thick including washing and filling of joints with slurry of white cement and pigment in desired shape with finishing cleaning and cost of wax polish etc. complete including cutting tiles to proper profile.(S-61P-47) | |  |  |  |  |
|  |  |  | **84.0** | **47651/56** | **%Sft** | **Rs:40027/-** |
|  |  |  |  |  |  |  |
|  |  |  |  |  | **Total** | **Rs:1497766/-** |
|  |  |  |  |  |  |  |

% Above/Below (Amount to be added/deducted).Rs\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Grand Total** Rs.

**Note:-** Quantities and rates may be changed as per/according to the Technical Sanction by the competent authority.

|  |  |
| --- | --- |
| **CONTRACTOR** | EXECUTIVE ENGINEER  (BUILDINGS) WORKS & SERVICES  DEPARTMENT KHAIRPUR |