SCHEDULE-B **CONSTRUCTION OF EID GAH AT VILLAGE MALNGA ABAD U/C MUHBAT WAH TALUKA KOT DIJI U/C RAHEEM BUX WASSAN DISTRICT KHAIRPUR**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO | ITEM OF WORK | NO:L.B.D |  | QTY |  | RATE | UNIT | AMOUNT |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 01 | Excavation in foundation of Building Bridges and other structures including dag belling dressing, refilling around structure with excavated earth Watering and ramming lead upto 5 ft.(S.I NO: 18 P.NO: 4) | | | | | |  |  |
|  |  |  | = | 335 | “ | 3176.25 | %0Cft | 1064/- |
|  |  |  | Thirty one hundred seventy six rupees twenty five ps: | | | | |  |
| 02 | Cement concrete brick or stone ballast 1 1/2" to 2" gauge.1:5:10 (S.I NO: 4 (e)P.NO: 15) | | | | | |  |  |
|  |  |  | = | 84 | “ | 8694.95 | %Cft | 7304/- |
|  |  |  | Eighty six hundred ninty four rupees ninty five ps: | | | | |  |
| 03 | Random, rubble masonry (uncaused )Ratio 1:6 (S.I NO: 1 (iv)P.NO: 27) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 175 | Cft | 17723/- | % Cft | 31015/- |
|  |  |  | Seventeen thousand seven hundred twenty three rupees | | | | |  |
| 04 | Coursed Ruble masonry including hammer dressing.Ratio 1:6 (S.I NO: 2 P-NO: 27) | | | | | |  |  |
|  |  |  | = | 126 | Cft | 25321/- | % CFt | 31904/- |
|  |  |  | Twenty five thousand three hundred twenty one ps: | | | | |  |
| 05 | R.C.C work in roof slab, beams columns rafts, lintels and other structural members laid in situ or precast laid in position complete in all respects. Ratio (1 : 2: 4 ) 90 Lbs. cement 2 Cft. Sand 4 Cft. Shingle 1/8" to 1/4" gauge.(S.I NO: 6 (a)P-16) | | | | | |  |  |
|  |  |  | = | 91 | Cft | 337/- | P.Cft | 30667/- |
|  |  |  | Three hundred thirty seven rupees. | | | | |  |
| 06 | Fabrication of mild steel reinforcement for cement concrete including cutting, bending, lying in position, making joints and fastenings including cost of binding wire (also includes removal of rust from bars.)(S.I NO: 8 P.NO: 17 | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 4.468 | cwt | 5001.70 | P.cwt | 22348/- |
|  |  |  | Five thousand one rupee seventy ps: | | | | |  |
| 07 | Pacca brick work in Ground Floor 1:6 in Cement sand mortar 1:6(S.I NO: 4 ( )P: NO: 20) | | | | | |  |  |
|  |  |  | = | 566 | Cft | 12346.65 | % Cft | 57035/- |
|  |  |  | Twelve thousand three hundred fourty six rupees sixty five ps: | | | | |  |
| 07 | Providing and fixing G.I frames /Choukhats of size 7" x 2" or 4 1/2" x 3" for windows using 20 gauge G.I sheet I/c welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage , tools and plants used in making and fixing.(CSI NO: 28 P-93) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 38 | Rft | 240.50 | P.Rft | 9139/- |
|  |  |  | Two hundred fourty rupees fifty ps; | | | | |  |
| 08 | First class deodar wood wrought, joinery in doors and windows etc, fixxed in position including chowkats hold fasts hinges, iron tower bolts, chocks cleats, handles and cords with hooks, etc.(1 3/4" thick)(S.I NO: 7 P-58) | | | | | |  |  |
|  |  |  | = | 25 | Sft | 902.93 | P.Sft | 22573/- |
|  |  |  | Nine hundred two rupees ninty three ps: | | | | |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO | ITEM OF WORK | NO:L.B.D |  | QTY |  | RATE | UNIT | AMOUNT |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 09 | Supplying and filling sand under floor and plugging in walls.(S.I NO: 29 P-26) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 360 | Cft | 1141.25 | % CFt | 4109/- |
|  |  |  | Eleven hundred fourty one rupees twenty five ps: | | | | |  |
| 10 | Add: Extra for Lead 3-0 Miles | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 360 | Cft | 579.41 | % Cft | 2086/- |
|  |  |  | Five hundred seventy nine rupees fourty one ps: | | | | |  |
| 11 | Cement concrete brick or stone ballast 1 1/2" to 2" gauge.1:6:12 (S.I NO: 4 (e)P.NO: 15) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 79 | Cft | 8122.95 | % Cft | 6417/- |
|  |  |  | Eighty one hundred twenty two rupees ninty five ps: | | | | |  |
| 12 | Cement plaster 1:6 upto 12' height.(b) 1/2" thick. (S.I NO: 13 P-52) | | | | | | |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 770 | Sft | 2206.60 | % SFt | 16991/- |
|  |  |  | Twenty two hundred six rupees sixty ps: | | | | |  |
| 13 | Cement plaster 1:4 upto 12' height.(b) 3/8” thick. (S.I NO: 13 P-52) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 770 | Sft | 2197.52 | % Sft | 16921/- |
|  |  |  | Twenty one hundred ninty seven rupees fifty two ps: | | | | |  |
| 14 | Cement concrete plain including placing compacting, finishing and curing, complete (including screening and washing at stone aggregate without shuttering. (S.I NO: 5 (i)P-16) Ratio 1:2:4 | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 60 | Cft | 14429.25 | % Cft | 8658/- |
|  |  |  | Fourteen thousand four hundred twenty nine rupees twenty five ps: | | | | |  |
| 15 | Supplying & Fixing R.S Girder (Material Schedule) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 5.785 | cwt | 3850/- | P.cwt | 28935/- |
|  |  |  | Thirty eight hundred fifty ups: | | | | |  |
| 16 | Supplying & Fixing R.S T-Iron (Material Schedule) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 4.642 | cwt | 3575/- | P.cwt | 16595/- |
|  |  |  | Thirty five hundred seventy five rupees | | | | |  |
| 17 | Second class tile roofing consisting of 4" earth and 1" mud plaster with Gobri leaping over 1/2"thick cement plaster 1:6 with 34 Lbs. Of hot bitumen coating sand blinded, provided over one layer of 12" x 6"x2" tiles laid in 1:6 cement mortar including 1:2 cement pointing under neath of tiles complete including curing etc.(S.I NO: 2 P-33) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 258 | Sft | 7607.25 | % Sft | 19627/- |
|  |  |  | Seventy six hundred seven rupees twenty five ps: | | | | |  |
| 18 | Cement concrete plain including placing compacting, finishing and curing, complete (including screening and washing at stone aggregate without shuttering. (S.I NO: 5 (i)P-16) Ratio 1:2:4 | | | | | |  |  |
|  |  |  | = | 60 | Cft | 14429.25 | % Cft | 8658/- |
|  |  |  | Fourteen thousand four hundred twenty nine rupees twenty five ps | | | | |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO | ITEM OF WORK | NO:L.B.D |  | QTY |  | RATE | UNIT | AMOUNT |
|  |  |  |  |  |  |  |  |  |
| 19 | Cement pointing struck joints on walls 1:2.(S.I NO: 19 (a) P-53) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 509 | Sft | 1213.58 | % Sft | 6177/- |
|  |  |  | Twelve hundred thirteen rupees fifty eight ps: | | | | |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 20 | Colour washing two coats (S.I NO: 25 P-54) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 1279 | Sft | 859.90 | % Sft | 10998 |
|  |  |  | Eight hundred fifty nine rupees ninty ps: | | | | |  |
| 21 | Providing & Fixing RCC Spouts etc | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 03 | Nos | 261.25 | each | 784/- |
|  |  |  | Two hundred sixty one rupees twenty five ps: | | | | |  |
| 22 | Painting Door & Windows any type 02 coats (S.I NO: P.NO: ) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 50 | Sft | 2116.41 | % Sft | 1058/- |
|  |  |  | Twenty one hundred sixteen rupees fourty one ps: | | | | |  |
| 23 | Providing and laying HALA or pattern tiles glazed 6" x 6" x 1/4" on floor or wall facing in required colour and pattern of STILE specification jointed in white cement and pigment over a base of 1:2 grey cement mortar 3/4" thick including washing and filling of joints with slurry of white cement and pigment in desired shape with finishing, cleaning and cost of wax polish etc. complete including cutting tiles to proper profile.(S.I NO: 61P-48) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 91 | Sft | 47651.56 | % Sft | 43363/- |
|  |  |  | Fourty seven thousand six hundred fifty one rupees fifty six ps: | | | | |  |
|  |  |  |  |  |  | ======================== | | |
|  |  |  |  | **Total** |  |  |  | **400561/-** |

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO | ITEM OF WORK | NO:L.B.D |  | QTY |  | RATE | UNIT | AMOUNT |

PART-B Compound wall

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 01 | Excavation in foundation of Building Bridges and other structures including dag belling dressing, refilling around structure with excavated earth Watering and ramming lead upto 5 ft.(S.I NO: 18 P.NO: 4) | | | | | |  |  |
|  |  |  | = | 1200 | “ | 3176.25 | %0Cft | 3812/- |
|  |  |  | thirty one hundred seventy six rupees twenty five ps: | | | | |  |
| 02 | Cement concrete brick or stone ballast 1 1/2" to 2" gauge.1:5:10 (S.I NO: 4 (e)P.NO: 15) | | | | | |  |  |
|  |  |  | = | 300 | “ | 8694.95 | %Cft | 26085/- |
|  |  |  | eighty six hundred ninty four rupees ninty five ps: | | | | |  |
| 03 | Random, rubble masonry (uncaused )Ratio 1:6 (S.I NO: 1 (iv)P.NO: 27) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 675 | Cft | 17723/- | % Cft | 119630/- |
|  |  |  | Seventeen thousand seven hundred twenty three rupe | | | | |  |
| 04 | Coursed Ruble masonry including hammer dressing. Ratio 1:6 (S.I NO: 2 P-NO: 27) | | | | | |  |  |
|  |  |  | = | 509 | Cft | 25321/- | % CFt | 128884/- |
|  |  |  | Twenty five thousand three hundred twenty one rupees | | | | |  |
|  |  |  |  | | | | |  |
| 05 | R.C.C work in roof slab, beams columns rafts, lintels and other structural members laid in situ or precast laid in position complete in all respects. Ratio (1 : 2: 4 ) 90 Lbs. cement 2 Cft. Sand 4 Cft. Shingle 1/8" to 1/4" gauge.(S.I NO: 6 (a)P-16) | | | | | |  |  |
|  |  |  | = | 170 | Cft | 337/- | P.Cft | 57290/- |
|  |  |  | Three hundred thirty seven rupees | | | | |  |
|  |  |  |  | | | | |  |
| 06 | Fabrication of mild steel reinforcement for cement concrete including cutting, bending, lying in position, making joints and fastenings including cost of binding wire (also includes removal of rust from bars.)(S.I NO: 8 P.NO: 17 | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 8.348 | cwt | 5001.70 | P.cwt | 41754/- |
|  |  |  | Five thousand one rupee seventy ps: | | | | |  |
|  |  |  |  | | | | |  |
| 07 | Pacca brick work in Other than building in Cement sand mortar 1:6(S.I NO: 4 ( )P: NO: 20) | | | | | |  |  |
|  |  |  | = | 984 | Cft | 12346.65 | % Cft | 121491/- |
|  |  |  | Tweleve thousand three hundred fourty six rupees sixty five ps: | | | | |  |
|  |  |  |  | | | | |  |
| 07 | Cement plaster 1:6 upto 12' height.(b) 1/2" thick. (S.I NO: 13 P-52) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 1669 | Sft | 2206.60 | % SFt | 36828/- |
|  |  |  | Twenty two hundred six rupees sixty ps: | | | | |  |
|  |  |  |  | | | | |  |
| 08 | Cement plaster 1:4 upto 12' height.(b) 3/8” thick. (S.I NO: 13 P-52) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 1669 | Sft | 2197.52 | % Sft | 36677/- |
|  |  |  | Tweny one hundred ninty seven rupees fifty two ps: | | | | |  |
|  |  |  |  | | | | |  |
| 09 | Cement pointing struck joints on walls 1:3.(S.I NO: 19 (a) P-53) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 1125 | Sft | 1213.58 | % Sft | 13653/- |
|  |  |  | Twelve hundred thirteen rupees fifty eight ps: | | | | |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO | ITEM OF WORK | NO:L.B.D |  | QTY |  | RATE | UNIT | AMOUNT |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 10 | Colour washing two coats (S.I NO: 25 P-54) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 2794 | Sft | 859.90 | % Sft | 24026/- |
|  |  |  | Eight hundred fifty nine rupees ninty ps: | | | | |  |
|  |  |  |  |  |  | ======================== | | |
|  |  |  |  | **Total** |  |  |  | **610130/-** |

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO | ITEM OF WORK | NO:L.B.D |  | QTY |  | RATE | UNIT | AMOUNT |

PART-B Main Gate

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 01 | Excavation in foundation of Building Bridges and other structures including dag belling dressing, refilling around structure with excavated earth Watering and ramming lead upto 5 ft.(S.I NO: 18 P.NO: 4) | | | | | |  |  |
|  |  |  | = | 54 | “ | 3176.25 | %0Cft | 172/- |
|  |  |  | Thirty one hundred seventy six rupees twenty five ps: | | | | |  |
| 02 | Cement concrete brick or stone ballast 1 1/2" to 2" gauge.1:5:10 (S.I NO: 4 (e)P.NO: 15) | | | | | |  |  |
|  |  |  | = | 18 | “ | 8694.95 | %Cft | 1565/- |
|  |  |  | Eighty six hundred ninty foue rupees ninty five ps: | | | | |  |
|  | R.C.C work in roof slab, beams columns rafts, lintels and other structural members laid in situ or precast laid in position complete in all respects. Ratio (1 : 2: 4 ) 90 Lbs. cement 2 Cft. Sand 4 Cft. Shingle 1/8" to 1/4" gauge.(S.I NO: 6 (a)P-16) | | | | | |  |  |
|  |  |  | = | 65 | Cft | 337/- | P.Cft | 21905/- |
|  |  |  | Three hundred thirty seven rupees | | | | |  |
|  | Fabrication of mild steel reinforcement for cement concrete including cutting, bending, lying in position, making joints and fastenings including cost of binding wire (also includes removal of rust from bars.)(S.I NO: 8 P.NO: 17 | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 3.191 | cwt | 5001.70 | P.cwt | 15960/- |
|  |  |  | Five thousand one rupee seventy ps: | | | | |  |
|  | Making & fixing steel grated door with 1/16" thick sheeting including angle iron frame 2" x 2" 3/8"and 3/4" square bars 4" centre to centre with locking arrangement. (S.I NO: 24 P-92) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 70 | Sft | 726.72 | P.Sft | 50870/- |
|  |  |  | Seven hundred twenty six rupees seventy two ps: | | | | |  |
|  | Painting guard bars, gates iron bars gratings , railings including standard braces (etc.) and similar open work.(S.I NO: 1 P.NO: 69) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 140 | Sft | 908.40 | % Sft | 1272/- |
|  |  |  | Nine hundred eight rupees fourty ps: | | | | |  |
|  |  |  |  |  |  | ======================== | | |
|  |  |  |  | **Total** |  |  |  | **134720/-** |

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO | ITEM OF WORK | NO:L.B.D |  | QTY |  | RATE | UNIT | AMOUNT |

PART- earth filling

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 01 | Supplying and filling sand under floor and plugging in walls.(S.I NO: 29 P-26) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 6000 | Cft | 1141.25 | % CFt | 68475/- |
|  |  |  | Eleven hundred fourty one rupees twenty five ps: | | | | |  |
| 02 | Add: Extra for Lead 3-0 Miles | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 6000 | Cft | 579.41 | % Cft | 34765/- |
|  |  |  | Five hundred seventy nine rupees fourty one ps: | | | | |  |
| 03 | Cement concrete brick or stone ballast 1 1/2" to 2" gauge.1:6:12 (S.I NO: 4 (e)P.NO: 15) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 1980 | Cft | 8122.95 | % Cft | 160834/- |
|  |  |  | Eighty one hundred twenty two rupees ninty five ps: | | | | |  |
| 04 | Cement concrete plain including placing compacting, finishing and curing, complete (including screening and washing at stone aggregate without shuttering. (S.I NO: 5 (i)P-16) Ratio 1:2:4 | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 1500 | Cft | 14429.25 | % Cft | 216439/- |
|  |  |  | Fourteen thousand four hundred twenty nine rupees twenty five ps: | | | | |  |
|  |  |  |  |  |  | ======================== | | |
|  |  |  |  | **Total** |  |  |  | **480513/-** |

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR