**SCHEDULE-B**

**REMAINING WORK OF IMAM BARGAH AT VILLAGE MUHMMAD HAYAT SHAIKH NEAR KARMABAD TALUKA & DISTRICK KHAIRPUR.**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **SR#** | **ITEM OF WORKS** | **NO. L: B: D:** | **QTY:** | **RATE** | **UNIT** | **AMOUNT** |
| **01.** | Supplying and filling sand under floor and plugging in walls.(S.I.No.29 P.No.31). | |  |  |  |  |
|  |  |  | **555.00** | **1141/25** | **%Cft** | **Rs.6334/-** |
|  |  |  |  |  |  |  |
| **02.** | Cement concrete brick or stone ballast 1 ½” to 20 gauge ratio 1:6:12. (S.I.No.21 P.NO.56). | |  |  |  |  |
|  |  |  | **178.00** | **8122/95** | **%Cft** | **Rs.14459/-** |
|  |  |  |  |  |  |  |
| **03.** | R.C.C works in roof slab, beams columns rafts lintels and other structural members laid in situ recast laid in position complete in all respects ratio 1:2:4 90lbs cement 2cft sand 4cft shingle 1/8 to ¼ gauges (S.I.No.06 P.No.19). | |  |  |  |  |
|  |  |  | **657.00** | **337/-** | **P-Cft** | **Rs.221409/-** |
|  |  |  |  |  |  |  |
| **04.** | Fabrication of mild steel reinforcement for cement concrete including cutting bending, laying in position making joints and fastenings including cost of binding wire also including cost of binding wire also includes removal of rust from bars.(S.I.No.07 P.No.20). | |  |  |  |  |
|  |  |  | **32.263** | **5001/70** | **P-Cft** | **Rs.161372/-** |
|  |  |  |  |  |  |  |
| **05.** | Pacca brick in ground floor super structure cement & sand mortar ratio 1:6. (S.I.No.05 P.No.25). | |  |  |  |  |
|  |  |  | **797.00** | **12674/36** | **%Cft** | **Rs.101015/-** |
|  |  |  |  |  |  |  |
| **06.** | Cement plaster 1:6 upto 20 height ½ thick. (S.I.No.13 P.No.58). | |  |  |  |  |
|  |  |  | **2718.00** | **2206/60** | **%Sft** | **Rs.59975/-** |
|  |  |  |  |  |  |  |
| **07.** | Cement plaster 1:6 upto 20 height ½ thick. (S.I.No.13 P.No.58). | |  |  |  |  |
|  |  |  | **2718.00** | **2197/52** | **%Sft** | **Rs.59729/-** |
| **08.** | First class deodar wood wrought, joinery in doors & windows etc. fixed in position i/c Chowkhats holds fasts hinges, iron tower blts. Chocks cleats, handles and cords with hooks, etc. Deodar paneled or paneled and glazed or fully glazed (S.I.No.7 P.No.7). | |  |  |  |  |
|  |  |  | **100.00** | **1273/76** | **P-Sft** | **Rs.127376/-** |
| **09.** | Providing and laying 2”thick topping cement concrete 1:2:4 i/c surface finishing and dividing into panels. (S.I.No.16 (d) P.No.47). | |  |  |  |  |
|  |  |  | **1275.00** | **3275/50** | **%Sft** | **Rs.41763/-** |
|  |  |  |  | **TOTAL** | | **Rs.793432/-** |

% Above/Below (Amount to be added/deducted).

Rs. **Grand Total** Rs. **Note:-** Quantities and rates may be changed as per/according to the Technical Sanction by the competent authority.

|  |  |
| --- | --- |
| **CONTRACTOR** | **EXECUTIVE ENGINEER**  (BUILDINGS) WORKS & SERVICES  DEPARTMENT KHAIRPUR |