SCHEDULE-B **REHABLITATION OF MANGWAR MANDAR AT RAMA PIR DILBAR TALUKA KOT DIJI DISTRICT KHAIRPUR**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO | ITEM OF WORK | NO:L.B.D |  | QTY |  | RATE | UNIT | AMOUNT |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 01 | Excavation in foundation of Building Bridges and other structures including dag belling dressing, refilling around structure with excavated earth Watering and ramming lead upto 5 ft.(S.I NO: 18 P.NO: 4) | | | | | | | | | | | |  | |  | |
|  |  | |  | | = | | 1581 | | “ | | 3176.25 | | %0Cft | | 5022/- | |
|  |  | |  | | Thirty one hundreds seventy six rups twenty five ps: | | | | | | | | | |  | |
| 02 | Cement concrete brick or stone ballast 1 1/2" to 2" gauge.1:5:10 (S.I NO: 4 (e)P.NO: 15) | | | | | | | | | | | |  | |  | |
|  |  | |  | | = | | 316 | | “ | | 8694.95 | | %Cft | | 27476/- | |
|  |  | |  | |  | | Eighty six hundreds ninety four rups ninety five ps: | | | | | | | |  | |
| 04 | R.C.C work in roof slab, beams columns rafts, lintels and other structural members laid in situ or precast laid in position complete in all respects. Ratio (1 : 2: 4 ) 90 Lbs. cement 2 Cft. Sand 4 Cft. Shingle 1/8" to 1/4" gauge.(S.I NO: 6 (a)P-16) | | | | | | | | | | | |  | |  | |
|  |  | |  | | = | | 672 | | Cft | | 337/- | | P.Cft | | 2226464/- | |
|  |  | |  | |  | | Three hundred thirty seven rupes | | | | | | | |  | |
| 05 | Fabrication of mild steel reinforcement for cement concrete including cutting, bending, lying in position, making joints and fastenings including cost of binding wire (also includes removal of rust from bars.)(S.I NO: 8 P.NO: 17 | | | | | | | | | | | |  | |  | |
|  |  | |  | |  | |  | |  | |  | |  | |  | |
|  |  | |  | | = | | 30.0 | | cwt | | 5001.70 | | P.cwt | | 150051/- | |
|  |  | |  | |  | | Five thousands one rupees seventy ps: | | | | | | | |  | |
| 06 | Pacca brick work in FOUNDATION / Plinth 1:6 in Cement sand mortar 1:6(S.I NO: 4 ( )P: NO: 20) | | | | | | | | | | | |  | |  | |
|  |  | |  | | = | | 450 | | Cft | | 11948.36 | | % Cft | | 57035 | |
|  |  | |  | | Eleven thousand nine hundred forty eight rupees thirty six ps: | | | | | | | | | |  | |
| 07 | Pacca brick work in ground Floor in building in Cement sand mortar 1:6(S.I NO: 4 ( )P: NO: 20) | | | | | | | | | | | |  | |  | |
|  |  | |  | | = | | 1559 | | Cft | | 12674.36 | | % Cft | | 197593/-/- | |
|  |  | |  | | Twelve thousand six hundred seventy four rupees thirty six ps: | | | | | | | | | |  | |
| 08 | Providing and fixing G.I frames /Choukhats of size 7" x 2" or 4 1/2" x 3" for door using 20 gauge G.I sheet I/c welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage , tools and plants used in making and fixing.(CSI NO: 29 P-93) | | | | | | | | | | | |  | |  | |
|  |  | |  | |  | |  | |  | |  | |  | |  | |
|  |  | |  | | = | | 18 | | Rft | | 228.50 | | P.Rft | | 4120/- | |
|  |  | |  | | Two hundred twenty eight rupees fifty ps: | | | | | | | | | |  | |
| 08 | Providing and fixing G.I frames /Choukhats of size 7" x 2" or 4 1/2" x 3" for windows using 20 gauge G.I sheet I/c welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage , tools and plants used in making and fixing.(CSI NO: 28 P-93) | | | | | | | | | | | |  | |  | |
|  |  | |  | | = | | 47 | | Rft | | 240.50 | | P.Rft | | 11304/- | |
|  |  | |  | |  | | Two hundreds forty rupees fifty ps: | | | | | | | |  | |
| 09 | First class deodar wood wrought, joinery in doors and windows etc, fixxed in position including chowkats hold fasts hinges, iron tower bolts, chocks cleats, handles and cords with hooks, etc.(1 3/4" thick)(S.I NO: 7 P-58) | | | | | | | | | | | |  | |  | |
|  |  | |  | | = | | 51 | | Sft | | 902.93 | | P.Sft | | 46049/- | |
|  |  | |  | |  | | Nine hundreds two rupes ninty three ps: | | | | | | | |  | |
| S.NO | | ITEM OF WORK | | NO:L.B.D | |  | | QTY | |  | | RATE | | UNIT | | AMOUNT |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 10 | Supplying & Fixing R.S Girder (Material Schedule) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 11.866 | cwt | 3850/- | P.cwt | 45684/- |
|  |  |  |  | Thiry eight hundreds fifty rupees | | | |  |
| 11 | Supplying & Fixing R.S T-Iron (Material Schedule) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 8.651 | cwt | 3575/- | P.cwt | 30927/-/- |
|  |  |  |  | Thirty five hundreds seventy five rupees | | | |  |
| 12 | Second class tile roofing consisting of 4" earth and 1" mud plaster with Gobri leaping over 1/2"thick cement plaster 1:6 with 34 Lbs. Of hot bitumen coating sand blinded, provided over one layer of 12" x 6"x2" tiles laid in 1:6 cement mortar including 1:2 cement pointing under neath of tiles complete including curing etc.(S.I NO: 2 P-33) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 579 | Sft | 7607.25 | % Sft | 44046/- |
|  |  |  |  | Seventy six hundred seven rupees twenty five ps | | | |  |
| 13 | Supplying and filling sand under floor and plugging in walls.(S.I NO: 29 P-26) | | | | | |  |  |
|  |  |  | = | 1569 | Cft | 1141.25 | % CFt | 17906/- |
|  |  |  |  | Eleven hundreds forty one rupes twenty five ps: | | | |  |
| 14 | Cement concrete brick or stone ballast 1 1/2" to 2" gauge.1:6:12 (S.I NO: 4 (e)P.NO: 15) | | | | | |  |  |
|  |  |  | = | 259 | Cft | 8122.95 | % Cft | 21038/- |
|  |  |  | Eighty one hundred twenty two rupees ninty five ps: | | | | |  |
| 15 | Cement concrete plain including placing compacting, finishing and curing, complete (including screening and washing at stone aggregate without shuttering. (S.I NO: 5 (i)P-16) Ratio 1:3:6 | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 85 | Cft | 12595/- | % Cft | 10790/- |
|  |  |  | Twelve thousands five hundred ninty five rupees | | | | |  |
| 16 | Cement concrete plain including placing compacting, finishing and curing, complete (including screening and washing at stone aggregate without shuttering. (S.I NO: 5 (i)P-16) Ratio 1:2:4 | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 133 | Cft | 14429.25 | % Cft | 19191/- |
|  |  |  |  | Fourteen thousands four hundreds twenty nine rups: twenty five ps: | | | |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 17 | Cement plaster 1:6 upto 12' height.(b) 1/2" thick. (S.I NO: 13 P-52) | | | | | | |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 3386 | Sft | 2206.60 | % SFt | 74715/- |
|  |  |  | Twenty two hundreds six rupees sixty ps: | | | | |  |
| 18 | Cement plaster 1:4 upto 12' height.(b) 3/8” thick. (S.I NO: 13 P-52) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 3386 | Sft | 2197.52 | % Sft | 74408/-/- |
|  |  |  | Twenty one hundreds ninty seven rupees fifty two ps: | | | | |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 19 | Reinforced cement concrete spout including fixing in position 2 1/2" x 6" x 5".(S.I NO: 14 P-18) | | | | | |  |  |
|  |  |  | = | 04 | Nos | 261.25 | each | 1045/- |
|  |  |  | Two hundred sixty one rupees twenty five ps: | | | | |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 20 | Priming coat of chalk distemper.(S.I NO: 23 P.NO: 54) | | | | | |  |  |
|  |  |  | = | 3386 | Sft | 442.75 | % Sft | 14992/- |
|  |  |  | Four hundred fourty two rupees seventy five ps: | | | | |  |
| 21 | Distempering 02 two coats | | | | | |  |  |
|  |  |  | = | 3386 | Sft | 1043.90 | % Sft | 35346/- |
|  |  |  | One thousand fourty three rupees ninty ps: | | | | |  |
| 22 | Painting Door & Windows any type 02 coats (S.I NO: P.NO: ) | | | | | |  |  |
|  |  |  | = | 102 | Sft | 2116.41 | % Sft | 2159/- |
|  |  |  | Twenty one hundred sixteen rupees fourty one ps: | | | | |  |
| 23 | laying floors of approved coloured glazed tiles 1/4" thick laid in white cement and pigment on a bed of 3/4" thick cement mortar 1:2. (S.I NO: 25 P.NO: 4) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 211 | Sft | 27747.06 | % Sft | 58546/- |
|  |  |  |  | Twenty seven thousands seven hundreds fourty seven rupees six ps: | | | |  |
|  |  |  |  |  |  | ======================== | | |
|  |  |  |  | **Total** |  |  |  | **1389323/-** |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR