SCHEDULE-B CONSTRUCTION OF COMPOUND WALL , PATH & MUSAFIR KHANA @ DARGAH RATTAL SHAHEED TALUKA KOT DIJI DISTRICT KHAIRPUR

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO | ITEM OF WORK | NO:L.B.D |  | QTY |  | RATE | UNIT | AMOUNT |

Part- Compound wall i/c Main Gate

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 01 | Excavation in foundation of Building Bridges and other structures including dag belling dressing, refilling around structure with excavated earth Watering and ramming lead upto 5 ft.(S.I NO: 18 P.NO: 4) | | | | | |  |  |
|  |  |  | = | 1436 | “ | 3176.25 | %0Cft | 4561/- |
|  |  |  |  | Thirty one hundred seventy six rupees twenty five ps: | | | |  |
| 02 | Cement concrete brick or stone ballast 1 1/2" to 2" gauge.1:5:10 (S.I NO: 4 (e)P.NO: 15) | | | | | |  |  |
|  |  |  | = | 364 | “ | 8694.95 | %Cft | 31650/- |
|  |  |  |  | Eighty six hundred ninty four rupees ninty five ps: | | | |  |
| 03 | Random, rubble masonry (uncaused )Ratio 1:6 (S.I NO: 1 (iv)P.NO: 27) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 787 | Cft | 17723/- | % Cft | 139480/- |
|  |  |  | Seventeen thousand seven hundred twenty three rupees | | | | |  |
| 04 | Coursed Ruble masonry including hammer dressing.Ratio 1:6 (S.I NO: 2 P-NO: 27) | | | | | |  |  |
|  |  |  | = | 593 | Cft | 25321/- | % CFt | 150154/- |
|  |  |  | Twenty five thousand three hundred twenty one ps: | | | | |  |
| 05 | R.C.C work in roof slab, beams columns rafts, lintels and other structural members laid in situ or precast laid in position complete in all respects. Ratio (1 : 2: 4 ) 90 Lbs. cement 2 Cft. Sand 4 Cft. Shingle 1/8" to 1/4" gauge.(S.I NO: 6 (a)P-16) | | | | | |  |  |
|  |  |  | = | 299 | Cft | 337/- | P.Cft | 100763/- |
|  |  |  | three hundred thirty seven rupees | | | | |  |
| 06 | Fabrication of mild steel reinforcement for cement concrete including cutting, bending, lying in position, making joints and fastenings including cost of binding wire (also includes removal of rust from bars.)(S.I NO: 8 P.NO: 17 | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 13.348 | cwt | 5001.70 | P.cwt | 66763/- |
|  |  |  | Five thousands one rupees seventy ps: | | | | |  |
| 07 | Pacca brick work in Other than Buildings1:6 in Cement sand mortar 1:6(S.I NO: 4 ( )P: NO: 20) | | | | | |  |  |
|  |  |  | = | 1125 | Cft | 12346.65 | % Cft | 138900/- |
|  |  |  | Twelve thousand three hundred fourty six rupees sixty five ps: | | | | |  |
| 08 | Cement plaster 1:6 upto 12' height.(b) 1/2" thick. (S.I NO: 13 P-52) | | | | | | |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 1400 | Sft | 2206.60 | % SFt | 30892/- |
|  |  |  | Twenty two hundred six rupees sixty ps: | | | | |  |
| 09 | Cement plaster 1:4 upto 12' height.(b) 3/8” thick. (S.I NO: 13 P-52) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 1400 | Sft | 2197.52 | % Sft | 30765/- |
|  |  |  | Twenty one hundred ninty seven rupees fifty two ps: | | | | |  |
| 10 | Cement pointing struck joints on walls 1:2.(S.I NO: 19 (a) P-53) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 1400 | Sft | 1287.44 | % Sft | 18024/- |
|  |  |  | Twelve hundred eighty seven rupees fourty four ps: | | | | |  |
| 11 | Colour washing two coats (S.I NO: 25 P-54) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 2800 | Sft | 1034/- | % Sft | 28952/- |
|  |  |  | Ten hundred thirty four rupees | | | | |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO | ITEM OF WORK | NO:L.B.D |  | QTY |  | RATE | UNIT | AMOUNT |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 12 | Making & fixing steel grated door with 1/16" thick sheeting including angle iron frame 2" x 2" 3/8"and 3/4" square bars 4" centre to centre with locking arrangemtnt. (S.I NO: 24 P-92) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 70 | Sft | 726.72 | P.Sft | 50870/- |
|  |  |  | Seven hundred twenty six rupees seventy two ps: | | | | |  |
|  | Providing and laying HALA or pattern tiles glazed 6" x 6" x 1/4" on floor or wall facing in required colour and pattern of STILE specification jointed in white cement and pigment over a base of 1:2 grey cement mortar 3/4" thick including washing and filling of joints with slurry of white cement and pigment in desired shape with finishing, cleaning and cost of wax polish etc. complete including cutting tiles to proper profile.(S.I NO: 61P-48) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 64 | Sft | 47651.50 | % Sft | 30497/- |
|  |  |  | Fourty seven thousand six hundred fifty one rupees fifty ps: | | | | |  |
|  | Painting Door & Windows any type 02 coats (S.I NO: P.NO: ) | | | | | |  |  |
|  |  |  | = | 140 | Sft | 2116.41 | % Sft | 2963/- |
|  |  |  | Twenty one hundred sixteen rupees fourty one ps: | | | | |  |
|  |  |  |  |  |  | ======================== | | |
|  |  |  |  | **Total** |  |  |  | **825234/-** |

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO | ITEM OF WORK | NO:L.B.D |  | QTY |  | RATE | UNIT | AMOUNT |

Part- Musafir Khana

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 01 | Excavation in foundation of Building Bridges and other structures including dag belling dressing, refilling around structure with excavated earth Watering and ramming lead upto 5 ft.(S.I NO: 18 P.NO: 4) | | | | | | |  |  |
|  |  |  | | = | 292 | “ | 3176.25 | %0Cft | 927/- |
|  |  |  | | Thirty One Hundred Seventy Six TWENTY FIVE PS: | | | | |  |
| 02 | Cement concrete brick or stone ballast 1 1/2" to 2" gauge.1:5:10 (S.I NO: 4 (e)P.NO: 15) | | | | | | |  |  |
|  |  |  | | = | 208 | “ | 8694.95 | %Cft | 18085/- |
|  |  |  | | EIGHTY SIX HUNDRED NINTY FOUR RUPEES NINTY FIVE PS: | | | | |  |
| 03 | Random, rubble masonry (uncaused )Ratio 1:6 (S.I NO: 1 (iv)P.NO: 27) | | | | | | |  |  |
|  |  |  | |  |  |  |  |  |  |
|  |  |  | | = | 203 | Cft | 17723/- | % Cft | 35978/- |
|  |  |  | | Seventeen thousands seven hundred twenty three rupees. | | | | |  |
| 04 | Coursed Ruble masonry including hammer dressing.Ratio 1:6 (S.I NO: 2 P-NO: 27) | | | | | | |  |  |
|  |  |  | | = | 122 | Cft | 25321/- | % CFt | 30892/- |
|  |  |  | | Twenty five thousands three hundred twenty one rupees. | | | | |  |
| 05 | R.C.C work in roof slab, beams columns rafts, lintels and other structural members laid in situ or precast laid in position complete in all respects. Ratio (1 : 2: 4 ) 90 Lbs. cement 2 Cft. Sand 4 Cft. Shingle 1/8" to 1/4" gauge.(S.I NO: 6 (a)P-16) | | | | | | |  |  |
|  |  |  | | = | 136 | Cft | 337/- | P.Cft | 45832/- |
|  |  |  | | Three hundred thirty seven rupees | | | | |  |
| 06 | Fabrication of mild steel reinforcement for cement concrete including cutting, bending, lying in position, making joints and fastenings including cost of binding wire (also includes removal of rust from bars.)(S.I NO: 8 P.NO: 17 | | | | | | |  |  |
|  |  |  | |  |  |  |  |  |  |
|  |  |  | | = | 6.026 | cwt | 5001.70 | P.cwt | 30140/- |
|  |  |  | | Five thousands one rupees seventy ps: | | | | |  |
| 07 | Pacca brick work in Ground Floor 1:6 in Cement sand mortar 1:6(S.I NO: 4 ( )P: NO: 20) | | | | | | |  |  |
|  |  |  | | = | 558 | Cft | 12674.35 | % Cft | 70723/- |
|  |  |  | | Twelve thousands six hundred seventy four rupees thirty five ps: | | | | |  |
| 08 | Filling, watering and ramming earth in floors with surplus earth from foundation lead upto one chain and lift jupto 5 feet.(S.I NO: 21 P-4). | | | | | | |  |  |
|  |  |  | | = | 195 | Cft | 1512.50 | %0Cft | 295/- |
|  |  |  | | Fifteen hundred twelve rupees fifty ps: | | | | |  |
| 09 | Supplying and filling sand under floor and plugging in walls.(S.I NO: 29 P-26) | | | | | | |  |  |
|  |  |  | | = | 450 | Cft | 1141.25 | % Cft | 5136/- |
|  |  |  | | Eleveb hundred fourty one rupees twenty five ps: | | | | |  |
| 10 | Cement plaster 1:6 upto 12' height.(b) 1/2" thick. (S.I NO: 13 P-52) | | | | | | | |  |
|  |  |  | |  |  |  |  |  |  |
|  |  |  | | = | 1664 | Sft | 2206.60 | % SFt | 36718/- |
|  |  |  | | Twenty-two hundred six rupees sixty ups: | | | | |  |
| 11 | Cement plaster 1:4 upto 12' height.(b) 3/8” thick. (S.I NO: 13 P-52) | | | | | | |  |  |
|  |  |  | |  |  |  |  |  |  |
|  |  |  | | = | 1664 | Sft | 2197.52 | % Sft | 36567/- |
|  |  |  | | Twenty one hundred ninty seven rupees fifty two ps: | | | | |  |
| 12 | Providing and fixing G.I frames /Choukhats of size 7" x 2" or 4 1/2" x 3" for door using 20 gauge G.I sheet I/c welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage , tools and plants used in making and fixing.(CSI NO: 29 P-93) | | | | | | |  |  |
|  |  |  | |  |  |  |  |  |  |
|  |  |  | | = | 18 | Rft | 228.90 | P.Rft | 4120/- |
|  |  |  | | Two hundred twenty eight rupees ninty ps: | | | | |  |
| S.NO | ITEM OF WORK | | NO:L.B.D |  | QTY |  | RATE | UNIT | AMOUNT |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 13 | Providing and fixing G.I frames /Choukhats of size 7" x 2" or 4 1/2" x 3" for windows using 20 gauge G.I sheet I/c welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage , tools and plants used in making and fixing.(CSI NO: 28 P-93) | | | | | | |  |  |
|  |  |  | | = | 47 | Rft | 240.50 | P.Rft | 11322/- |
|  |  |  | | Two hundred fourty rupees fifty ps: | | | | |  |
| 14 | Supplying & Fixing R.S Girder (Material Schedule) | | | | | | |  |  |
|  |  |  | |  |  |  |  |  |  |
|  |  |  | | = | 8.839 | cwt | 3850/- | P.cwt | 34030/- |
|  |  |  | | Thirty eight hundred fifty rupees | | | | |  |
| 15 | Supplying & Fixing R.S T-Iron (Material Schedule) | | | | | | |  |  |
|  |  |  | |  |  |  |  |  |  |
|  |  |  | | = | 6.482 | cwt | 3575/- | P.cwt | 23173/- |
|  |  |  | | Thirty five hundred seventy five rupees | | | | |  |
| 16 | Second class tile roofing consisting of 4" earth and 1" mud plaster with Gobri leaping over 1/2"thick cement plaster 1:6 with 34 Lbs. Of hot bitumen coating sand blinded, provided over one layer of 12" x 6"x2" tiles laid in 1:6 cement mortar including 1:2 cement pointing under neath of tiles complete including curing etc.(S.I NO: 2 P-33) | | | | | | |  |  |
|  |  |  | |  |  |  |  |  |  |
|  |  |  | | = | 355 | Sft | 7607.25 | % Sft | 27006/- |
|  |  |  | | Seventy six hundred seven rupees twenty five ps: | | | | |  |
| 17 | Cement concrete plain including placing compacting, finishing and curing, complete (including screening and washing at stone aggregate without shuttering. (S.I NO: 5 (i)P-16) Ratio 1:3:6 | | | | | | |  |  |
|  |  |  | |  |  |  |  |  |  |
|  |  |  | | = | 51 | Cft | 12595/- | % Cft | 6423/- |
|  |  |  | | Twelve thousands five hundred ninty five rupees | | | | |  |
| 18 | First class deodar wood wrought, joinery in doors and windows etc, fixxed in position including chowkats hold fasts hinges, iron tower bolts, chocks cleats, handles and cords with hooks, etc.(1 3/4" thick)(S.I NO: 7 P-58) | | | | | | |  |  |
|  |  |  | |  |  |  |  |  |  |
|  |  |  | | = | 50 | Sft | 902.93 | P.Sft | 45147/- |
|  |  |  | | Nine hundred two rupees ninty three ps: | | | | |  |
| 19 | Priming coat of chalk distemper.(S.I NO: 23 P.NO: 54) | | | | | | |  |  |
|  |  |  | | = | 1664 | Sft | 442.75 | % Sft | 7367/- |
|  |  |  | | Four hundred fourty two rupees seventy five ps: | | | | |  |
| 20 | Distempering 02 two coats | | | | | | |  |  |
|  |  |  | | = | 1664 | Sft | 1043.90 | % Sft | 17370/- |
|  |  |  | | One thousand fourty three rupees ninty ps: | | | | |  |
| 21 | Painting Door & Windows any type 02 coats (S.I NO: P.NO: ) | | | | | | |  |  |
|  |  |  | | = | 88 | Sft | 2116.41 | % Sft | 1862/- |
|  |  |  | | Twenty one hundred sixteen rupees fourty one ps: | | | | |  |
| 22 | Supplying & fixing in position iron/steel grill of 3/4" x 1/4" size flat iron of approved design including painting 3 coats etc. complete (weight not to be less than 3.7 Lbs./Sq . Foot of finished grill).(S.I NO: 26 P-93) | | | | | | |  |  |
|  |  |  | | = | 32 | Sft | 180.50 | P.Sft | 5776/- |
|  |  |  | | One hundred eighty rupees fifty ps: | | | | |  |
| S.NO | ITEM OF WORK | | NO:L.B.D |  | QTY |  | RATE | UNIT | AMOUNT |
| 23 | Providing and laying tiles glazed 6" x 6" x 1/4" on floor or wall facing in required colour and apttern of STILE specification jointed in white cement and pigment over a base of 1:2 grey cement mortar 3/4" thick including washing and filling of joints with slaurry of white cement and pigment in desired shape with finishing, clearing and cost of wax polish etc. complete including cutting tiles to proper profile.(S.I NO: 60 P-47) | | | | | | |  |  |
|  |  |  | | = | 370 | Sft | 30509.77 | % SFt | 112886/- |
|  |  |  | | Thirty thousand five hundred nine rupees seveny seven ps: | | | | |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 24 | Reinforced cement concrete spout including fixing in position 2 1/2" x 6" x 5".(S.I NO: 14 P-18) | | | | | |  |  |
|  |  |  | = | 02 | Nos | 261.25 | each | 523/- |
|  |  |  | Two hundred sixty one rupees twenty five ps: | | | | |  |
|  |  |  |  |  | ============================== | | | |
|  |  |  |  | **Total** |  |  |  | **608298/-** |

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO | ITEM OF WORK | NO:L.B.D |  | QTY |  | RATE | UNIT | AMOUNT |

Part- Path

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 01 | Excavation in foundation of Building Bridges and other structures including dag belling dressing, refilling around structure with excavated earth Watering and ramming lead upto 5 ft.(S.I NO: 18 P.NO: 4) | | | | | |  |  |
|  |  |  | = | 270 | “ | 3176.25 | %0Cft | 858/- |
|  |  |  | Thirty one hundred seventy six rupees twenty five ps: | | | | |  |
| 02 | Cement concrete brick or stone ballast 1 1/2" to 2" gauge.1:5:10 (S.I NO: 4 (e)P.NO: 15) | | | | | |  |  |
|  |  |  | = | 360 | “ | 8694.95 | %Cft | 31302/- |
|  |  |  | Eighty six hundred ninty four rupees ninty five ps: | | | | |  |
| 03 | Formation , dressing and preparing sub-grade (b) on sloe (S.I NO: 1 P-74)) | | | | | |  |  |
|  |  |  | = | 360 | Cft | 453.75- | % Cft | 1634/- |
|  |  |  | Four hundred fifty three rupees seventy five ps: | | | | |  |
| 04 | Cement concrete plain including placing compacting, finishing and curing, complete (including screening and washing at stone aggregate without shuttering. (S.I NO: 5 (i)P-16) Ratio 1:2:4 | | | | | |  |  |
|  |  |  | = | 90 | Cft | 14429.25 | % CFt | 12986/- |
|  |  |  | Fourteen thousands four hundred twenty nine rupees twenty five ps: | | | | |  |
| 05 | Pacca brick work in foundation/plinth in building 1:6 in Cement sand mortar 1:6(S.I NO: 4 ( )P: NO: 20) | | | | | |  |  |
|  |  |  | = | 496 | Cft | 11948.36 | % Cft | 59263/- |
|  |  |  | Eleven thousand nine hundred fourty eight rupees thirty six ps: | | | | |  |
| 06 | Cement plaster 1:6 upto 12' height.(b) 1/2" thick. (S.I NO: 13 P-52) | | | | | | |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 960 | Sft | 2206.60 | % SFt | 21183/- |
|  |  |  | Twenty two hundred six rupees sixty ps: | | | | |  |
| 07 | Cement plaster 1:4 upto 12' height.(b) 3/8” thick. (S.I NO: 13 P-52) | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  | = | 960 | Sft | 2197.52 | % Sft | 21096/- |
|  |  |  | Twenty one hundred ninty seven rupees fifty two ps: | | | | |  |
|  |  |  |  |  | ============================== | | | |
|  |  |  |  | **Total** |  |  |  | **148322/-** |

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO | ITEM OF WORK | NO:L.B.D |  | QTY |  | RATE | UNIT | AMOUNT |

Part- Court Yard

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |
| 01 | Cement concrete brick or stone ballast 1 1/2" to 2" gauge.1:5:10 (S.I NO: 4 (e)P.NO: 15) | | | | | |  |  |
|  |  |  | = | 413 | “ | 8694.95 | %Cft | 35910/- |
|  |  |  | Eighty six hundred ninty four rupees ninty five ps: | | | | |  |
| 02 | Cement concrete plain including placing compacting, finishing and curing, complete (including screening and washing at stone aggregate without shuttering. (S.I NO: 5 (i)P-16) Ratio 1:2:4 | | | | | |  |  |
|  |  |  | = | 313 | Cft | 14429.25 | % CFt | 45164/- |
|  |  |  | Fourteen thousands four hundred twenty nine rupees twenty five ps: | | | | |  |
|  |  |  |  |  | ============================== | | | |
|  |  |  |  | **Total** |  |  |  | **81074/-** |

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR