***SCHEDULE OF QUANTITIES***

***WORK No: 03***

# 

**DISTRICT MUNICIPAL CORPORATION (WEST)**

**KARACHI, BALDIA ZONE**

***Estimated Cost Rs: 9,88,305/- Earnest Money Rs: 19,766/-***

***Time Limit: 45 Days Penalty Per Day Rs: 1,000/-***

**SUBJECT: *Providing & Laying Aggregate Base Course i/c Hiring of Machinery Tractor Blade***

***And R.C.C Ring Slab Manhole Covers at Imam Bargah Hussani, Pal Panjtan, Sajjadia***

***Hyderi, Sabil-Hussain Gulshan-e-Ghazi Sector 14/12 in UC-33-36, DMC (West) Baldia***

***Zone.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ***S.No:*** | ***DESCRIPTION OF WORK*** | ***QUANTITY*** | ***RATE*** | ***PER*** | ***AMOUNT*** |
| *1.* | *Manufacturing and supplying R.C.C main hole covers cast in situ 1:2:4 C.C. 3” inch deep in center reinforced with 3/8” dia M.S Bars welded on M.S. sheet i/c curing transportation. 21” dia.* | *100-Nos* | *913.63* | *Each* | *91363/-* |
| *2.* | *Manufacturing and supplying of R.C.C Ring Slab of 21” inside 36” dia outside 75 wide and to thick i/c 3/8” dia tor steel bar two concentric rings with 3/8” dia Nos. cross links bars welded and two sunk type hook, lasted in 1:1-1/2:3 concrete with embedded 15kg C.I frame in per feet position i/c terms partition charges for an average lead of 20 km per trip from casting yard to town office (A minimum of 25 slabs per trip will be transported.)* | *40-Nos* | *1906.60* | *Each* | *76264/-* |
| *3.* | *Shifting to the site and fixing 26” dia Ring Slab in perfect position on damage manhole i/c cutting of damage portion of mentioned in past shape and lying of cement concrete mortar of 2” thickness and disport of debris.* | *40-Nos* | *563.09* | *Each* | *22524/-* |
| *4.* | *Hiring of Tractor Blade for cleaning of road & street with P.O.L (A.R) P-Hours.* | *80* | *950* | *P-Hour* | *76000/-* |
| *5.* | *Providing & Laying Aggregate base course material over proper grade and camber having CBR 80% as per AASHTO standard specification i/c spreading an compacting by approve mechanical means (Motor harder, Vibratory roller and smooth wheel roller etc) watering to maintain the moisture content the compaction of each layer shall 100 percent to the max dry density (Rate i/c all cost of material T&P and carriage upto).* | *130330* | *5542.24* | *%Cft* | *722154/-* |
| ***Total Estimated Cost*** | | | | | ***9,88,305.00*** |

***PTO***

*Nomenclature, Quantities and Rates etc checked*

*and found correct.*

***ASSTT ENGINEER (B&R) ASSTT: EXECUTIVE ENGINEER (B&R)***

*BALDIA ZONE BALDIA ZONE*

*I/We hereby quoted Rates @ % above/below the S/R*

*The total amount is Rs: (Rupees:*

*(In Figure) (In Word)*

## *Contractor’s Signature:*

## 

## *Address:*