**SCHEDULE “B” CONSTRUCTION OF OXIDATION PONDS FOR ZONE-B & ZONE-C FOR DRAINAGE SCHEME KHIPRO DISTRICT SANGHAR.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.# | Description | Qty | Rate | Unit | Amount |

1. Excavation for tanks and reservoirs in soft soils including trimming and dressing sides to true alignment design section / profiles and shape leveling of beds of trenches to correct level and grade i/e laying of earth in 6” layers for construction of banks and dressing and disposal of surplus excavated earth with in one chains directed by In charge Engineer i/e providing fence guard light flats where as required lift up to 5 feet (1.52m) and lead up to one chain. (30.5m) (P.H.S.I.NO: 1 P 67).

266213.60 Cft Rs. 3000/- P%0 Cft Rs. 798641/-

2. Excavation for tanks and reservoirs in Wet Soils including trimming and dressing sides to true alignment design section / profiles and shape leveling of beds of trenches to correct level and grade i/e laying of earth in 6” layers for construction of banks and dressing and disposal of surplus excavated earth with in one chains directed by In charge Engineer i/e providing fence guard light flats where as required lift up to 5 feet (1.52m) and lead up to one chain. (30.5m) (P.H.S.I.NO: 14 / P 74).

1. 0-5 Depth

125181.94 Cft Rs. 4800/- P%0 Cft Rs. 600873/-

3. Earth work compaction laying earth in 6” layers leveling dressing and watering for compaction etc complete (GSI NO 13 P/4)

387120.93 Cft Rs: 354/- P% 0 Cft Rs: 137041/-

4. Providing Laying jointing and testing ASTM Pipe B Class cutting fitting and jointing with rubber ring i/c testing with water to a head of 183 meter or 600 ft (PHSI NO. 2 P/17)

18” dia 160.0 Rft Rs. 618/- P/Rft Rs. 98880/-

5. Cement concrete plain i/c placing compacting finishing curing etc complete i/c screening and washing or stone aggregate without shuttering Ratio 1:4:8 (GSI No:5 P-18) .

50.24 Cft. Rs: 11288/75 P% Cft. Rs: 5671/-

6. RCC work i/c all labor and material except the cost of steel reinforcement and Its labor for bending and binding which will be paid separately. This rate also Includes all kinds of forms mould lifting shuttering curing rendering and finishing the exposed surface (i/c screening and washing of shingle)a RCC work in roofs slabs beams columns rafts lintels and other structural members laid in situ or precast laid in position complete the all respect (I) Ratio 1:2:4 90 lbs cement 2cft sand 4 Cft shingle 1/8” to ¼”guage. (GSI No: 6 (a) P-19).

249.82 Cft. Rs: 337/- P/Cft. Rs. 84189/-

7. Fabrication of mild steel reinforcement cement concrete i/c cutting bending Laying in position and fastening i/c cost of binding wire etc. (GSI No: 7 (b) P-19)

10.00 Cwt. Rs: 5001/70 P/Cwt. Rs. 50017/-

Total Rs. 1775312/-

***CONDITIONS.***

*1. Any error omission in the specification quantity and unit will be governed by the relevant schedule items.*

*2. The rates should be inclusive of all taxes i.e. sales tax octori tax etc.*

*3. No separate carriage will be paid to the contractor.*

*4. No premium will be allowed for non-schedule items.*

*5. The decision of the Superintending Engineer, Public Health Engineering Circle Mirpurkhas will be final and binding the parties in any dispute.*

CONTRACTOR

EXECUTIVE ENGINEER

PUBLIC HEALTH ENGG: DIVISION

SANGHAR