**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT MUHAMMAD HASSAN HOUSE / SADDAM KHOSO / GHULAM KHASKHELI TO BACHAYO MALLAH TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT MANZAR PATHAN / BAHADUR PATHAN HOUSE TO HAZOOR BUX BROHI HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT SEEDO KHOSO / SHER BHATTI HOUSE ALTAF KHOSO HOUSE TO MOHAMMAD HASSAN HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT RANA GULZAR RAJPUT / RAHEEM KHOSO HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT MEGHWAR / GULL MUHAMMAD MALLAH TO MITHO MALLAH HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT HAZOOR BUX BROHI / HAJI KHAN RIND TO HUSSAIN BUX JASKANI TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT HAFIZ ABDUL REHMAN HOUSE / HAJI QURBAN HOUSE / SABAGO ODD HOUSE TO SEEDO KHOSO HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT HUSSAIN BUX JASKANI / QURBAN KHOSO HOUSE TO HAFIZ ABDUL REHMAN TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT MITHO MALLAH / BASHIR SEHTO TO SHAHNWAZ MALLAH HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT SHAHNWAZ MALLAH / JAMO GIRGILO / ALI BUX MACH TO HAKEEM GIRGILO HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT ABDUL RAZZAQ KHASKHELI HOUSE / MIRZA BARGAH TO SHER RAJPUT HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT GHULAM SHABBIR KHOSO HOUSE / THAHEEM HOUSE TO ALI BUX SAMMO HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT ABDUL MAJEED CHUTTO HOUSE / ABDUL HAMEED / ABDUL HAMEED SANG TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT ABDUL SATTAR RAJPUT HOUSE / IMTIAZ KHASKHELI HOUSE / PIYARO KHOSO HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT ABDULLAH WASAN HOUSE / KHAN MASAN HOUSE TO GHULAM SHABBIR KHOSA HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT ALLAH WARAYO SAMMO HOUSE / SAWAN KHASKHELI HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT DISPOSAL SOUZ ALI HOUSE / YAQOOB GRAVEYARD TO GHULAM QADIR RIND HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT AMEER SHAIKH HOUSE / SHAKEEL RAJPUT HOUSE / SHER REJPUT HOUSE / ZULIFQAR KHASKHELI HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT BACHAL MALLAH HOUSE / THARO KOHLI HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT BAQIE SANG / RASOOL BUX PINYARO TO ASLAM SANG HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT DAD WASAN / KAMRAN WAS AN HOUSE / MURTAZA WASAN HOUSE / INYAT WAS AN HOUSE / SALEEM WAS AN HOUSE TO SALEEM MUSKAN HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT ASLAM HOUSE / MACHI IMAM BARGAH TO HANIF SHAIKH HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT FARAH RABEEL HOUSE / HABALI MEDICAL / ASHOK DAS SHOP TO HAJI WALI MUHAMMAD TAHAHEEM HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT HANIF SHAIKH HOUSE / ZAFAR KHASKHELI HOUSE / LAKHANO SHAIKH HOUSE TO AMEER SHAIKH HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT GHULAM MUSTAFA CORNER / SHAH LAIF CLINIC / SHAHNWAZ MEDICAL TO AL ABBAS BOOK STORE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT AZAM SHAH MEDICAL TO SAFEER MITHO SHOP / JIYE LATIF SHOP TO BHITSHA GENERAL STORE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT KAMIL BHATTI HOUSE / WALO MALLAH HOUSE / ALLAH BACHAYO BHATTI HOUSE TO BACHAL MALLAH HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT MUHAMMAD RAFIQUE HOUSE TO FAQIR SAIN HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT LALU SAND HOUSE / GHULAM ABBAS PARHYAR HOUSE / IMDAD CHANDIO HOUSE TO GHULAM CHANDIO HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT WASAYO MAGHAR HAR / SYED KHUDA DINO SHAH / ARBAB RAHO HOUSE / DR. YOUSIF HOUSE TO MUHAMMAD RAFIQUE HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT SHAH LATIF PAKORA SHOP / USTAD SHABBIR AHMED CONSTRUCTION TO FAROOQUE AZAM CHOWK TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT SHABBIR AHMED HOUSE / GHULAM HASSAN HOUSE TO DR. YOUSIF HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT RAJA BHARI HOUSE / YOUSIF BOZDAR HOUSE TO YAR MUHAMMAD KHOSO HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT SALEEM RAJPUT HOUSE TO MUHAMMAD RAFIQUE HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT ARBAB RAHO HOUSE / DODO MALLAH / GHULAM FAQIR RAHO HOUSE / SAIN KHUDA DINO UTAK TO MUBARAK SHEEDI HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT RAJPUT CHOWK / KARBALA COFFEE / LALA KHER MUHAMMAD TO HAJI KABRANI HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT BAKSHO SEHTO HOUSE / MITHAL MACHI / HAJI PAKOTAI TO BALI BAKERY TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT BALI KI BAKERY / GHAFOOR KHASKHELI TO CHANDIO HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT GHAFOOR KHASKHELI / CHANDIO HOUSE TO RIAZ JUTT HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT HAJI KAMRANI / MOHRAM SHOP / GOTH SHOP TO HAIDER KHASKHELI HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT PRIMARY SCHOOL YAQOOB SHAHEED TO SALEEM RAJPUT HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT MASTER MOHAN HOUSE / PREETUM HOUSE TO LALU MEGHWAR HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT GHULAM MUHAMMAD PHANWER HOUSE / RAMZAN MACHI BARGAH / ALLAN SEHTO HOUSE TO BAKSHO SEHTO HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT PRIMARY SCHOOL / RAJAB JUTT HOUSE TO MIRZA HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT SHER RAJPUT HOUSE / JAMEEL ABBASI HOUSE RAJA DEWAN HOUSE TO GADHA SAIN PUMP TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT RAJA DEWAN HOUSE / BADAR SANG HOUSE TO MOULA BUX PARHYAL HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT MUHAMMAD BUX KHASKHELI HOUSE / YAR MUHAMMAD KHASKHELI HOUSE TO ABDUL SATTAR RAJPUT HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT NADEEM GENERAL STORE / DARGAH CHARI TO PRIMARY SCHOOL TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT THARO KOHLI HOUSE / HANIF PARYAL HOUSE / JUMAN HOUSE TO SHER MALLAH BARGAH KAMIL BHATTI HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT MIRZA JUTT HOUSE / PERAIZ SEHTO HOUSE TO MASJID ALI WALI-UL-LLAH HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT VIP ROAD / JAFFAR KHASKHELI HOUSE / MUHAMMAD KHAN WASAN HOUSE TO MUHAMMAD BUX KHASKHELI HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT FAQIR SAIN HOUSE TO FAROOQUE AZAM CHOWK TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT MASJID ALI WALI-UL-LLAH / DHANI BUX MALLAH HOUSE / KHAN KHASKHELI HOUSE TO ABDUL RAZZAQ KHASKHELI HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **PROVIDING & FIXING PAVER ROAD AT PIYARO KHOSO HOUSE / GHULAB KHASKHELI HOUSE TO ABDUL MAJEED CHUTTO HOUSE TOWN BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Earth work excavation undressed lead up to a single throw of kassi or pharwah or shovel in ordinary soil | | | |
| 1150.00 Cft | | @ Rs. 1361/- | P.% Cft | **Rs. 1,565/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2254.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 257,24/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 1845.75 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 173,801/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4. | Providing & Fixing cement paving blocks flooring having size of 197 x 97 x 80 (mm) of city / quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete (GSI Publication No.52 page # 50, Sr # 73). | | | |
| 3691.50 Sft | | @ Rs. 223.97 | P. Sft | **Rs. 826,785/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5. | Providing & Fixing pri-cost block 3750 psi industrial made size 6 inches thick x 12 inches long x 12 inches high including the cost of cartage, excavation from work for haunching, 1450 psi lean concrete, 2250 psi concrete for haunching 1:4 cement sand mortar (GSI Publication No.55 page # 16, Sr # 14). | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 40.00 Cft | | @ Rs. 14429.25 | P. Cft | **Rs. 5,772/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL** | **1,051,468/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT KAMIL BHATTI HOUSE / WALO MALLAH HOUSE / ALLAH BACHAYO BHATTI HOUSE / LALU SAND HOUSE TO GHULAM ABBAS PARHYAR HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT PIYARO KHOSO HOUSE / GHULAB KHASKHELI HOUSE / ABDUL MAJEED BHATTI HOUSE / JAM PHORO HOUSE TO ABDUL HAMEED SANG HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT GULL HASSAN THAHIM HOUSE / ALI BUX SAMMO HOUSE / TARO KOLHI HOUSE / HANIF PARHYAR HOUSE / SHER MALLAH BARGAH HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT HAB ALI MEDICAL / ASHOK DAS SHOP / GHULAM MUSTAFA CORNER TO SHAH LATIF CLINIC / SHAHBAZ MEDICAL TO AZAM SHAH MEDICAL BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT JAFFAR KHASKHELI HOUSE / MUHAMMAD KHAN WASAN HOUSE / MUHAMMAD BUX KHASKHELI HOUSE TO YAR MUHAMMAD KHASKHELI HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT SHER RAJPUT HOUSE RAJA DEWAN HOUSE TO BADAR SAND HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT SHAKEEL RAJPUT HOUSE / SHER RAJPUT HOUSE / TANVEER RAJPUT HOUSE / VIP ROAD TO JAFFAR KHASKHELI HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT ASLAM HOUSE TO MACHI IMAM BARGAH / HANIF SHAIKH HOUSE TO ZAFAR KHASKHELI HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT AZAM SHAH MEDICAL / G.A LARIF SHOP / NADEEM GENERAL STORE TO PRIMARY SCHOOL TO BARGAH MOHALLA BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT BADAR SANG HOUSE / RASOOL BUX TO ASLAM HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT HAJI PAKOTAI / BALI KI BAKERY / GHAFOOR KHASKHELI BARGAH / CHANDIO HOUSE TO RIAZ JUTT HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT MASTER MOHAN HOUSE / PREETAM HOUSE / LALU MENGHWAR / RAJAR CHOWK / LALA KHER MUHAMMAD RAHO TO HAJI KABRANI BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT GHULAM MUHAMMAD PHANWAR HOUSE / RAMZAN MACHI HOUSE / ALLAN SEHTO HOUSE / BAKSHO SEHTO HOUSE TO MITHAL MACHI HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT ARBAB RAHO HOUSE / DODO MALLAH HOUSE / GHULAM FAQIR RAHO HOUSE / SAIN KHUDA DINO SHAH UTAQ TO MUBARAK SHEEDI HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT SHAH LATIF PAKORA SHOP / USTAAD SHABBIR AHMED CONSTRUCTION / GULL HASSAN HOUSE TO DR. YOUSIF HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT FAQIR SAIN HOUSE / FAROOQUE AZAM CHOWK / WASAYO MANGHAR HAR / KHUDA DINO SHAH HOUSE TO ARBAB HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT DR. YOUSIF HOUSE / PRIMARY SCHOOL / YAQOOB SHAHEED / SALEEM RAJPUT HOUSE / MUHAMMAD RAFIQUE HOUSE TO FAQIR SAIN HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT HAJI KABRANI / MOHRAM SHOP / GOTH SHOP / HAIDER KHASKHELI / RAJA BHARGI HOUSE TO YOUSIF BOZDAR HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT YOUSIF BOZDAR HOUSE / RANA GULZAR RAJPUT HOUSE TO RAHEEM KHOSO HOSUE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT RAHEEM KHOSO HOUSE / MANZAR PATHAN HOUSE / BAHADUR KHAN HOUSE HAZOOR BUX BROHI HOUSE TO HAJI KHAN RIND HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT BASHIR SEHTO HOUSE / RAB NAWAZ MALLAH HOUSE / JAMMO GIRRILO / ALI BUX MACHI TO HAKEEM GIRGILO HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT ABDUL RAZAQ PHANWAR HOUSE / NOMORIO MEGHWAR / GULL MUHAMMAD MALLAH / MITHO MALLAH TO BASHEER SEHTO HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT ALTAF KHOSO HOUSE / MUHAMMAD HASSAN HOUSE / SADAM KHOSO HOUSE / GHULAM KHASKHELI / BACHAYO MALLAH HOUSE TO ABDUL RAZZAQ PHANWAR HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT HAJI KHAN RIND HOUSE / HUSSAIN BUX JASKANI HOUSE / QURBANI KHOSO HOUSE / HAFIZ ABDUL REHMAN HOUSE TO HAJI QURBAN HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT HAJI QURBAN HOUSE / SABAGO ODD HOUSE SEEDO KHOSO HOUSE / SHER BHATTI HOUSE TO ALTAF KHOSO HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT ZAFAR KHASKHELI HOUSE / LAKHANO SHAIKH HOUSE / AMEER BUX SHIKAH HOUSE TO SHAKEEL RAJPUT HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT PERVAIZ SEHTO HOUSE / MASJID ALI WALI-UL-LLAH / DHANI BUX MALLAH HOUSE TO KHAN KHASKHELI HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT KHAN KHASKHELI HOUSE / ABDUL RAZAQ KHASKHELI HOUSE / MIRZA BARGAH TO SHER RAJPUT HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT YAR MUHAMMAD KHASKHELI HOUSE / ABDUL SATTAR RAJPUT HOUSE / IMTIAZ KHASKHELI HOUSE TO PIYARO KHOSO HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT DAD WASAN HOUSE VIA MURTAZA HOUSE / KHOKHAR MUSKAN TO DISPOSAL SOZ AALI HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT BHAGIA MOHALLAH / RAJAB JUTT HOUSE TO MIRZA JUTT HOUSE BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |

**SCHEDULE-B**

|  |  |
| --- | --- |
| NAME OF WORK: | **RECONSTRUCTION OF C.C DRAIN / RCC SLAB AT GHULAM ABBAS PARHYAR HOUSE / IMDAD CHANDIO HOUSE / ALLAH WARAYO SAMMO HOUSE / SAWAN KHASKHELI HOUSE / FARAH RABEEL HOUSE TO HAB ALI MEDICAL BHITSHA DISTRICT MATIARI** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Supplying & Filling pit san under floor and plunging in to well. | | | |
| 2250.00 Cft | | @ Rs. 1141.25 | P.% Cft | **Rs. 25,678/-** |
| 2. | Dismantling C.C reinforcement ratio 1:2:4 i/c separating reinforcement from C.C & straightening the same. | | | |
| 360.00 Cft | | @ Rs. 5445/- | P.% Cft | **Rs. 19,602/-** |
| 3. | Dismantling Road mattaling. | | | |
| 600.00 Cft | | @ Rs. 605/- | P.% Cft | **Rs. 3,630/-** |
| 4. | Dismantling C.C plain 1:2:4. | | | |
| 160.00 Cft | | @ Rs. 3328/- | P.% Cft | **Rs. 5,325/-** |
| 5. | Dismantling Pucca brick work in lime or cement mortar 1:6. | | | |
| 270.00 Cft | | @ Rs. 1285.63 | P.% Cft | **Rs. 3,471/-** |
| 6. | Earth work excavation in irrigation channels drains or dressed to designed section grades or profiles excavated material disposed off lead with in soft. | | | |
| 3900.00 Cft | | @ Rs. 6490/- | P.% Cft | **Rs. 25,311/-** |
| 7. | C.C brick stone ballast 1 ½” to2” gauge ration 1:4:8 | | | |
| 975.00 Cft | | @ Rs. 9416.28 | P.% Cft | **Rs. 91,809/-** |
| 8. | Errection removal of centering for RCC or plain C.C work of vertical partal wood. | | | |
| 3900.00 Cft | | @ Rs. 3127.41 | P.% Sft | **Rs. 121,969/-** |
| 9. | Cement concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of aggregate w/o shuttering ration 1:2:4 80 x 1.00 x 0.050. | | | |
| 1950.00 Cft | | @ Rs. 14429.25 | P. % Cft | **Rs. 281,370/-** |
| 10. | Reinforced C.C work i/c all labour & material except the cost of steel reinforcement & its labour or bending & binding which will be paid separately. This rate is also i/c all kinds of forms, moulds, lifting, shuttering, curing, rendering & finishing exposed surface i/c screening & washing of shingle, ratio 1:2:4. | | | |
| 338.00 Cft | | @ Rs. 337/- | P. Cft | **Rs. 113,906/-** |
| 11. | Fabrication of M.S reinforced C.C i/c cutting jointing laying in position making joints & fastening i/c cost of binding wire & removal of rust from bars using tor bars. | | | |
| 12.00 Cwt | | @ Rs. 5001.70 | P. Cwt | **Rs. 60,020/-** |
| 12. | Cement concrete plain i/c placing compacting finishing & curring complete i/c screening & washing of aggregate w/o shuttering ratio 1:2:4 | | | |
| 60.00 Rft | | @ Rs. 297.01 | P. Rft | **Rs. 17,821/-** |
|  | |  | **TOTAL** | **787,154/-** |