**SCHEDULE “B”**

**CONSTRUCTION OF FEEDING CHANNEL FOR WATER SUPPLY SCHEME DAAR DISTRICT SANGHAR.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.# | Description | Qty | Rate | Unit | Amount |

1. Excavation in foundation of building and other structure i/c dag belling dressing

refilling arround the structure with excavated earth watering and ramming lead upto

one chain andlift upto 5’ (In ordinary soil) (GSI No: 18(b)P/5).

22500.0 Cft. Rs.3176/25 P% 0 Cft. Rs. 71466/-

2. Cement concrete brick stone ballast 1 ½” to 2” guage (Gsi no 5 (i) P/15).

3750.0 Cft. Rs: 9416/28 P% Cft. Rs: 353111/-

3. Pucca brick worik in foundation and plinth in cement sand mortor (1:6) (GSI o:4(e)P/21)

11250.0 Cft Rs: 11948/36 P% Cft Rs: 1344191/-

4. Cement concrete plain i/c placing compacting finishing curing etc complete i/c screening and washing or stone aggregate without shuttering Ratio 1:2:4 (GSI No:5(i) P-16) .

938.0 Cft. Rs:14429/25 P% Cft. Rs: 135346/-

5. Cement plaster (1:4) upto 12’ height ½” thick.(GSI No:11(b)P/52).

2000.0 Sft Rs: 2283/93 P% Sft Rs: 456786/-

6. RCC work i/c all labour and material except the cost of steel reinforcement and its labour for bending and binding which will be paid seperatly. This rate also includes all kinds of forms mould lifting shuttering curring rendering and finishing the exposed surface (i/c screening and washing of shingle)a RCC work in roofs slabs beams columns rafts lintels and other structural members laid in situ or precast liad in position complete the all respect (I) Ratio 1:2:4 90 lbs cement 2cft sand 4 cft shingle 1/8” to ¼”guage.(GSI No: 6 (a) P-19).

220.50 Cft. Rs: 337/- P/Cft. Rs: 74309/-

7. Fabrication of mild steel reinforcement cement concrete i/c cutting bending

laying in position and fastening i/c cost of binding wire etc.(GSI No:7(b)P-19)

8.86 Cwt. Rs: 5001/70 P/Cwt. Rs: 44315/-

Total Rs. 2479524/-

**CONDITIONS.**

1. *Any error omission in the specification quantity and unit will be governed by the relevant schedule items.*
2. *The rates should be inclusive of all taxes i.e sales tax octori tax etc.*
3. *No separate carriage will be paid to the contractor*
4. *No premium will be allowed for no-schedule items.*
5. *The decision of the Superintending Engineer, Public Health Engineering Circle Mirpurkhas will be final and binding the parties if in any dispute.*

EXECUTIVE ENGINEER

PUBLIC HEALTH ENGG: DIVISION

SANGHAR

CONTRACTOR