**OFFICE OF THE**



**ADDL. INSPECTOR GENERAL OF POLICE,**

**KARACHI RANGE**

No. AB/A-II/ / Karachi.

dated - -2016

To,

The Director (Advertisement),

Public Relation Department,

Govt. of Sindh,

Block-95 Sindh Secretariat, Karachi

SUBJECT: PUBLICATION OF TENDER NOTICE.

Enclosed please find herewith a draft Tender / inviting Notice for Publication in the daily Newspapers in English, Urdu and Sindhi at the Earliest.

***Sd/-***

***(MUSHTAQ AHMED MAHAR)SI, PPM,PSP***

*Addl. Inspector General of Police,*

*Karachi Range*

Copy to the following for information please.

1. *The Inspector General of Police Sindh Karachi*
2. *The Manager* ***(Assessment)****, Government of Sindh Public Procurement Regulatory Authority, (SPPRA) Barrack No.8 Sindh Secretariat No.4 Court Road Karachi*
3. *The Director* ***I.T. Sindh Police*** *for advertisement display on Sindh Police Official website (www.sindh police.gov.pk).*

***( SYED AFZAL HUSSAIN )***

*DSP / Welfare*

*For. Addl. Inspector General of Police,*

*Karachi Range*

OFFICE OF THE



ADDL. INSPECTOR GENERAL OF POLICE,

KARACHI RANGE

No. AB/A-I/ / Karachi.

Dated: - -2016.

**TENDER NOTICE.**

Sealed Tender on Standard Book Documents are hereby inviting for repair / renovation work of the KPO Building Karachi.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Name of Work | Estimated Cost | Earnest Money | Tender Cost | Completion time | Opening Date | Opening place |
| Repair / renovation work, 03 Watch Tower with Ladders, Reception Room , Compound Wall , Iron Barrier , Grill etc | 3.0 million | 2,5% | 2500/- | 45 days | 18-02-2016 at 1500 hrs | Addl.IGP/Karachi Conference Room |

**CONDITIONS :**

1. The interested parties/contractors/companies can be head tender documents for the above quoted work from Account Branch of **Addl.IGP/Karachi** office by submitting an application on company’s letter head alongwith **Tender Fee** with effect from **04-03-2016 to 18-03-2016.**
2. The last date to deposit tender will be **18-03-2016 at 1200** hours.
3. The tender shall be open on **18-03-2016 at 1500 hours** in presence of committee and representatives of participants in Addl.IGP/Karachi Conference Room 4th Floor, KPO Building near Saddar PS Karachi
4. Contractors must be provided registration of Pakistan Engineering Council income Tax and Sale Tax according to the SPPRA Rule-2010.
5. The Tender inviting notice can also be seen on Sindh Police website.
6. The Addl.IGP/Karachi Range reserves the rights to **ACCEPT** or **REJECT** any or all offers according to **SPPRA rules 2010.**

***( SYED AFZAL HUSSAIN )***

*DSP / Welfare*

*For. Addl. Inspector General of Police,*

*Karachi Range*

*OFFICE OF THE*



*ADDL. INSPECTOR GENERAL OF POLICE,*

*KARACHI RANGE*

*No. AB/A-II / / Karachi.*

*Dated: - -2016*

*ORDER.*

*The Addl.IGP/Karachi is hereby approved* ***“Procurement Committee’s”*** *mentioned below for completion Tender Procuring Award of work & all necessary formalities as per SPPRA Rule-2010 on account of repair/renovation work of KPO Building, Karachi.*

***TENDER PROCURMENT COMMITTEE.***

*Mr. Fida Hussain Janwari,* ***Chairman***

*SSP/City South Zone Karachi*

1. *Mr. Hassan Khan Marwat Member*

*DSP/Clothing, HQ Garden, Karachi*

1. *Mr. Anwar Ali Sommro Member*

*DSP/M.T. Karachi (KPO)*

***INSPECTION REDRESSAL OF GRIVEVANCEES***

***AND SETTLEMENT OF DISPUTES COMMITTEE.***

*Mr. Ghulam Shabbir Memon,* ***Chairman***

*ADIGP/Legal, Karachi (KPO)*

1. *Mr. Kunwar Asif Sarfraz, Member*

*DSP/Saddar, Karachi*

1. *Mr. Sohail Shah Member*

*DSP/PCA Karachi (KPO)*

***Sd/-***

*(MUSHTAQ AHMED MAHAR)SI, PPM,PSP*

*Addl. Inspector General of Police,*

*Karachi Range*

*1. Copy to the ADIGP / Legal, Karachi Range for information.*

*2. Copy to the SSP / City South Zone, Karachi for information.*

*3. Copy to the DSP / Saddar, South Zone Karachi for information.*

*4. Copy to the DSP / Clothing HQ Garden Karachi for information*

*5. Copy to the DSP / M.T. Karchi (KPO) for information*

*6. Copy to the DSP / PCA Karchi (KPO) for information*

*7 The Manager (CB) Govt. of Sindh (SPPRA) Barrack No.8 Sindh Secretariat No.4 Court Road Karachi for information.*

*8. The Audit Officer-I CPO Sindh Karachi*

***( SYED AFZAL HUSSAIN )***

*DSP / Welfare*

*For. Addl. Inspector General of Police,*

*Karachi Range*

**Name of Work repair / renovation of Karachi Police Office**

**(Rough Cost Estimated)**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.NO** | **DESCRIPTON** | **QTY** | **RATE** | **UNIT** | **AMOUNT** |
| 01 | Dismantling of Reception | 01 | 12000 | Each | 12000 |
| 02 | Excavation in foundation of building bridges & other structure including deg-belling dressing refilling around structure with excavated earth watering & ramming lead upto 5 ft (IN ORDINARY SOIL) | 750 | 20 | P.CFT | 15000 |
| 03 | Cement concrete brick or stone ballast 1 1/2 to 2” gauge ratio 1:4: 8 | 350 | 110 | P.CFT | 38500 |
| 04 | Reinforced cement concrete work including all labor & material except the cost of steel reinforcement and its labor for bending & binding which will be paid separately. This rate also includes all kinds of forms moulds lifting shuttering curing rendering & finishing the exposed surface (including screening and washing of shingle) (a) R.C Work in roof slab, beams columns rafts, lintels & other structural members laid in situ or precast laid in position complete in all respects. (ii) Ratio 1:1/2:3 | 2125 | 550 | P.CFT | 1168750 |
| 05 | Fabrication of mild steel reinforcement for cement concrete including cutting, bending, laying in position, making joints and fastening including cost of binding wire (also includes removal of rust) ( using tor bars.) | 25 | 6200 | P.CWT | 155333 |
| 06 | P/L 1:3:6 cement concrete solid block masonary set in 1:6 cement sand mortar in plinth & foundations including raking out joints and curing etc complete Foundation. | 950 CFT | 110 | P.CFT | 104500 |
| 07 | Cement Plaster 1:6 upto 20 “ height | 2500 | 26 | P.Sft | 65000 |
| 08 | P/L porcelain tiles 18”x18” 1/4 on floor facing in required color & pattern of jointed in white cement and pigment over a base of 1:2 grey cement mortar 3/4 thick including washing & filling of joints with slurry of white cement and pigment in de. | 50 | 350 | P.Sft | 175000 |
| 09 | CC toping over roof and chemical treatment 2” thick | 250 | 55 | S.FT | 13750 |
| 10 | Scraping the old distemper preparing the surface & supplying two cost of distemper of specified make & color as directed by Engineer in-charge | 5212 | 15 | P.Sft | 78180 |
| 11 | Providing and fixing R.C.C. barricade size 4’x 8 think 1 foot finishing and quarrying and cartage | 40 | 15500 | Each | 620000 |
| 12 | Providing and fixing heavy duty GI Angle Iron Doors | 63 | 1120 | SFT | 70560 |
| 13 | Providing and fixing GI PIPE 3’ dia Iron Barrier | 2 | 120000 | Each | 240000 |
| 14 | Providing & fixing Girll ½ “Square bar Open side including Coloring and painting. | 300 | 550 | P.SFT | 165000 |
| 15 | Supplying and fixing Energy Savers | 29 | 350 | Each | 10150 |
| 16 | Providing & fixing panel board shutter to accommodate having duty circuit breaker bus bars including painting with enameled paint & for other similar jobs on surface | 3 | 1150 | P.Sft | 3450 |
| 17 | Providing circuit breaker 6 amps to 36 amps D.P. | 3 | 11,00 | Each | 3300 |
| 18 | Providing and laying wiring main with 2-7/. 044 PVC China patti | 300 | 120 | P.Rft | 36000 |
| 19 | Wiring for light of fan point with 1/1 12(31029) PVC insulated wire in 200 mm including channel patti fancy piano type switch 15 AMP China make including holder, complete | 30 | 850 | Each | 25500 |
|  | Grant Total |  |  |  | 2999973 |

**Sub- Engineer**