**Tender Reference No. 01(19)/ 2015-2016**

**SCHEDULE RATE BASED ON (2012)**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **S. NO** | **DESCRIPTION OF ITEMS** | **QTY** | **RATE IN FIGURE** | **RATE IN WORD** | **UNIT** | **AMOUNT** |
| 1. | Excavation of pipe line trenches pipe all kind of soil murum i/c trimming dressing leveling beds trenches correct level and graded cutting joints holes disposal of surplus earth with in 1 chains as directed by the Engg: Inch: P. fence guard lights flags temporary crossing non vehicler traffic where ever req: a lift upto 5 ft & lead up to 1 chain. | 9000/Cft | 4650/- | Rupees Four Thousand Six Hundred & Fifty Only | %0Cft | 41850/- |
| 2. | P. Rcc pipe ASTM class class ‘C’ 76-62 T/C 76-70 class II wall ‘B’ and fixing in trenches i/c cutting fitting jointing with rubber ring i/c testing with water to specified pressure 9″ & 12″dia pipe. | 1000/P.Rft | 412/- | Rupees Four Hundred & Twelve Only | P.Rft | 412000/- |
| 3. | Const of Main Holes 4 inside with Rcc covers 21″dia 3×¾ with flat iron frame 5ft depth 1:2:4 in laying CC cost in situ 9″ thick wall and disposal of surplus stuff etc comp: | 42 No | 13028/- | Rupees Thirteen Thousand & Twenty Eight Only | Each | 547176/- |
| 4. | Add or deduct for depth of man holes above or beyond 5 ft (RA). | 52.5/Rft | 2245/55 | Rupees Two Thousand Two Hundred Forty Five & Fifty Five Paisa Only | P.Rft | -117891/- |
| 5. | Refilling the excavated stuff in trenches 6″ thick layer i/c watering ramming to full compaction etc comp: | 8100/Cft | 2760/- | Rupees Two Thousand Seven Hundred & Sixty Only | %0Cft | 22356/- |
| 6. | Earth work of Excavation undressed lead upto single throw of Kassi Phwarah of shavel in ordinary siol . | 25071/Cft | 1663.75 | Rupees One Thousand Six Hundred Sixty Three & Seventy Five Paisa Only | %0Cft | 41712/- |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **S. NO** | **DESCRIPTION OF ITEMS** | **QTY** | **RATE IN FIGURE** | **RATE IN WORD** | **UNIT** | **AMOUNT** |
| 7. | Cartage of 100 Cft 5 tons all materials like stone aggregate spwals lime surkhi BG rail fasting points crossing bridge guders pipe sheet M/S Brass sheets 1000 trenches 10×5×3" 1000 tiles 12×6×2" 150 cft timber 100 mould fuel wood by trenches owned by the contractor withing 10 miles etc comp: | 20057/Cft | 902.20 | Rupees Nine Hundred & Two Only | %Cft | 180954/- |
| 8. | CC plain i/c placing compacting finishing and curing complete i/c screening and washing of stone aggregate without shuttering ratio 1:4:8 | 19936/Cft | 9416.28 | Rupees Nine Thousand Four Hundred Sixteen & Twenty Eight Paisa Only | %Cft | 1877230/- |
| 9. | P/L 2" thick toping cement concrete 1:2:4 i/c surface finishing and dividing into panels etc completed. | 60413/Sft | 3275.50 | Rupees Three Thousand Two Hundred Seventy Five & Fifty Paisa Only | %Sft | 1978828/- |
| **Total Amount of Schedule Items** | | | | | | **49,84,215/-** |