***BIDDING DATA***

***(The Section Should Be Filed In The Engineer /Production Agency Before Issuance Of The Bidding Documents)***

|  |  |  |
| --- | --- | --- |
| ***a)*** | *Name of procuring agency:* | ***Executive Engineer Public Health Engineering Division II Khairpur @ Ranipur*** |
| ***b*** | *Briel description of work :* | Surface Drains and CC Block for Village Malherani Solangi UC Gadeji Taluka Sobhodero |
| ***c*** | *procuring agency’s Address* | **Taluka Sobhodero District Khairpur** |
| ***d*** | Estimated Cost | Rs. 14, 00, 000/- |
| ***e*** | Amount of BID Security | **2%** |
| ***f*** | Period of bid validity (Security) | **15 Days** |
| ***g*** | Security Deposit(including Bid Security) | **N/A** |
| ***h*** | Dead Line for bid submission of bid along with time | **N/A** |
| ***i*** | Venue time and date of bid opening | ***At Executive Engineer Public Health Engineering Division II Khairpur @ Ranipur*** |
| ***j*** | Time for completion form written order of commence | 12 Months |
| ***k*** | Liquidity damages | N/A |
| ***l*** | Deposit receipt No: date amount (kin word & Figure) | N/A |
|  |  |  |

***(Executive Engineer/Authority issuing bedding document)***

|  |  |
| --- | --- |
| ***Assistant Engineer***  ***Public Health Engineering***  ***Sub Division Sobhodero*** | ***Executive Engineer***  ***Public Health Engineering***  ***Division II Khairpur @ Ranipur*** |

**SCHEDULE B**

**NAME OF WOORK: CONSTUCTION OF SURAFCE DRAINS & C.C BLOCK FOR VILLAGE MALHERANI SOLANGI U/C SETHARJA BALLATALUKASOBHO DERO DISTRICT KHAIRPUR.**

**SUB HEAD NO.1 Surface drains**

1. Excavation in foundation of building bridges and other structure

i/c dag belling refilling around the structure with excavated

earth watering ramming lead up to one chain and lift up to 5 ft

. (PH Sch. No.18 P.NO.4)

Qty.3128.58 Cft. @Rs.3176/25 P%0 Cft. Rs 9,937/-

1. Cement concrete plain i/c placing compacting finishing curing

complete i/c screening and washing stone aggregate w/o

shuttering (CSI No.5(i) P.NO.17) **(a) Ratio 1:4:8**

Qty. 759.0 Cft. @Rs.11288/75 P% Cft. Rs.85,682/-

1. Pacca Brick work in foundation and plinth in cement sand Ratio (1;6) (CSI No.7 P.NO.23)

Qty. 2124.0 Cft @Rs.11948/36 P% Cft Rs.2,53,783/-

1. Countli block……………….

Qty.600.0 Rft. @Rs.94/- P. Rft. Rs.56,400 /-

T–II Drain

Qty.400.0 Rft. @Rs:174/- P. Rft. Rs.69,600/

1. Cement plaster 1:4 20’ height ½” thick (CSI No.11 P.NO.57)

Qty. 3100.0 Sft @Rs.2283/93 P% Sft Rs.70,803/-

1. RCC work in roof slab, beams columns rafts, lintels, and other

structure members laid in situ of pre cost laid in position

complete in all respect 1:2:4 (CSI No.7 P.NO.17)

Qty. 410.50 Cft @Rs.337/93 P.Cft Rs:138339/-

1. Fabricationof mild steel reinforcement for cement concrete i/c

cutting bending laying in position making K=joints and

fastering i/c cost of binding wire also i/c removal of rust from

Qty. 14.66 Cwt @Rs.4820/20 P.CwtRs:70,664/-

Total Rs:7,55,207/-

**SUB HEAD NO.II C.C Block**

1.Barrow pit excavation undressed lead up to 100 ft in

ordinary soil (CSI-3(a) P-1)

Qty. 3150.0 CFT @Rs.2117/50 P%0 Cft. Rs.6670/-

2. Lying Earth in 6” layers & leveling dressing &

Wateringfor Etc complete. (CSI-13(b)P-3)

Qty: 3150.0 Cft @Rs.354/- P%0 Cft Rs.1115/-

3.Extra for every 50”ft additional lead or part there of

(C.S.I No: 8 (a) P-3)

Qty: 3150.0 Cft @Rs.5039/- P%0 Cft Rs.1587./-

4. Cement concrete brick or stone ballast 1 ½” to 2” guage

Ratio 1:4:8 (CSI No.4(b)9 P. 15).

Qty. 1386.0 CFT @Rs.9416/28 P% Cft. Rs.1,30,510/-

5.Cement concrete plain 1:2:4 i/c placing compacting

finishing and curing complete i/c screening and washing

of stone aggregate without shuttering

(CSI No.5 P.No.16)

Qty. 1050.0 CFT@Rs.14429/-P% Cft. Rs.151507/-

6.Errection & removal for centering of therefore of Rcc

Partial wood (CSI.No. ) Ratio: 1:2:4.

Qty.191.98 SFT @Rs.7693/13 P% Sft. Rs.14769/-

**TotalRs.3,20,444/-**

**ABSTRACT**

PART-I **Surface Drains** Rs.7,55,207/-

PART-II **C.C Topping** Rs.3,20,444/-

**Total** **Rs.1075651/-**

C O N D I T I O N S

01. Any error / omission in the description of items of work rate original schedule

Will correct accordingly under executive engineer Public Health Engineering

Division II Khairpur @ Ranipur.

02. Premium will be allowed as non, schedule items.

03. The work will be carried out as per P.W.D. specification and approval details.

Workingestimates.

**CONTRACTOR EXECUTIVE ENGINEER**

PUBLIC HEALTH ENGINEERING

DIVISION-II KHAIRPUR @ RANNIPUR