***BIDDING DATA***

***(The Section Should Be Filed In The Engineer /Production Agency Before Issuance Of The Bidding Documents)***

|  |  |  |
| --- | --- | --- |
| ***a)*** | *Name of procuring agency:* | ***Executive Engineer Public Health Engineering Division II Khairpur @ Ranipur*** |
| ***b*** | *Briel description of work :* | Surface Drains and CC Block for MohallaKoral Khan Khuhro UC Madd Taluka Sobhodero |
| ***c*** | *procuring agency’s Address* | **Taluka Sobhodero District Khairpur** |
| ***d*** | Estimated Cost | Rs. 14, 00, 000/- |
| ***e*** | Amount of BID Security | **2%** |
| ***f*** | Period of bid validity (Security) | **15 Days** |
| ***g*** | Security Deposit(including Bid Security) | **N/A** |
| ***h*** | Dead Line for bid submission of bid along with time | **N/A** |
| ***i*** | Venue time and date of bid opening | ***At Executive Engineer Public Health Engineering Division II Khairpur @ Ranipur*** |
| ***j*** | Time for completion form written order of commence | 12 Months |
| ***k*** | Liquidity damages | N/A |
| ***l*** | Deposit receipt No: date amount (kin word & Figure) | N/A |
|  |  |  |

***(Executive Engineer/Authority issuing bedding document)***

|  |  |
| --- | --- |
| ***Assistant Engineer***  ***Public Health Engineering***  ***Sub Division Sobhodero*** | ***Executive Engineer***  ***Public Health Engineering***  ***Division II Khairpur @ Ranipur*** |

**SCHEDULE B**

**NAME OF WORK: CONSTRUCTION OF SURFACE DRAINS &C.C BLOCK FOR VILLAGE KORAL KHANKHURO U/C MADD TALUKA SOBHODERODISTRICT KHAIRPUR**

**PART- I** **SURFACE DRAINS**

1. Excavation in foundation of building bridges and other

structure i/c dag belling refilling around the structure

with excavated earth watering ramming lead up to one

chain and lift up to 5 ft. (C S I No.18 (b) P.NO.4)

Qty. 484.0 Cft @ Rs.3176/25 P %Cft. Rs: 1,537/-

1. Cement concrete plain i/c placing compacting finishing

curing complete i/c screening and washing stone

aggregate w/o shuttering (CSI No.5(i) P.NO.16)

**(a) Ratio 1:4:8**

Qty:121.0Cft . @Rs.11288/75 P %Cft Rs.13659/-

1. Pacca Brick work in foundation and plinth in cement sand

Ratio (1;6) (CSI No.4 (e) P.NO.21)

Qty275.0 Cft @Rs.11948/3 P% Cft Rs.32,858/-

1. Construction of standard of open drains cunette block

of cement concrete 1:2:4 in situ to design profile i/c cost

ofmould as per drawing i/c applying floating coat of

cement 1/32” thick to the exposed face finished smooth

curingetc complete as per detail drawing

(PHSI No. D P.NO.44)

Qty. 200.0 Rft @Rs.94/- P Rft. Rs.1880/-

1. Cement plaster 1:4 20’ height ½” thick

(CSI No.13 P.NO.52)

Qty. 532.0Sft @Rs.2283/93 P% **Sft.** Rs.12151/**-**

1. RCC work in roof slab, beams columns rafts, lintels,

and other structure members laid in situ of pre cost

laid in position complete in all respect 1:2:4

(CSI No.7 P.NO.17).

Qty**.143.53** Cft @Rs.337/- P% **Sft.** Rs.48370/-

1. Fabricationof mild steel reinforcement for cement

concrete i/c cutting bending laying in position

making K=joints and festering i/c cost of binding

wire also i/c removal of rust from bars

(CSI No.7(ii) P.NO.19).

Qty.5.12 Cwt. @Rs.4820/20 P cwt Rs.24679/-

***Total*** Rs1,52.054/

**PART- II C.C Topping**

1. Barrow pit excavation undressed lead up to 100 ft in

ordinary soil (CSI-3(a) P-1)

Qty. 14524.82 CFT @Rs.2117/50 P%0 Cft. Rs.30756/-

2. Lying Earth in 6” layers & leveling dressing &

Watering for Etc complete. (CSI-13(b)P-3)

Qty:14524.82CFT @Rs.354/- P%0 Cft Rs.5142/-

3. Extra for every 50”ft additional lead or part there of

(C.S.I No: 8 (a) P-3)

Qty:14524.82CFT @Rs.5039/- P%0 Cft Rs.73191/-

4. Cement concrete brick or stone ballast 1 ½” to 2” guage

Ratio 1:4:8 (CSI No.4(b)9 P. 15).

Qty.3375.48 CFT @Rs.9416/28 P% Cft. Rs.317845/-

5. Cement concrete plain 1:2:4 i/c placing compacting

finishing and curing complete i/c screening and

washing of stone aggregate without shuttering

(CSI No.5 P.No.16)

Qty.2557.18 CFT @Rs.14429/25 P% Cft. Rs.162329/-

6. Errection& removal for centering of therefore ofRcc

Partial wood (CSI .No. ) Ratio: 1:2:4.

Qty.1356.04 SFT @Rs.3127/41 P% Sft. Rs.42409/-

**Total Rs.8,38,325 /-**

**GENERAL ABSTRACT OF COST**

**PART- I Surface Drains**  Rs:2,02,261/-

**PART- II C.C. Topping** Rs:11,93,615/-

**Total Rs:13,95,876/-**

***C O N D I T I O N S***

01. Any error / omission in the description of items of work rate original schedule

will correct accordingly under executive engineer Public Health Engineering

division II Khairpur @ Ranipur .

02. premium will be allowed as non , schedule items.

03. The work will be carried out as per P.W.D. specification and approval details.

working estimates .

|  |  |
| --- | --- |
| CONTRACTOR | EXECUTIVE ENGINEER  PUBLIC HEALTH ENGINEERING  DIVISION-II KHAIRPUR @ RANNIPUR |