***BIDDING DATA***

***(The Section Should Be Filed In The Engineer /Production Agency Before Issuance Of The Bidding Documents)***

|  |  |  |
| --- | --- | --- |
| ***a)*** | *Name of procuring agency:* | ***Executive Engineer Public Health Engineering Division II Khairpur @ Ranipur*** |
| ***b*** | *Briel description of work :* | urface Drains and CC Block for City Madd UC Madd Taluka Sobhodero. |
| ***c*** | *procuring agency’s Address* | **Taluka Sobhodero District Khairpur** |
| ***d*** | Estimated Cost | Rs. 19, 00, 000/- |
| ***e*** | Amount of BID Security | **2%** |
| ***f*** | Period of bid validity (Security) | **15 Days** |
| ***g*** | Security Deposit(including Bid Security) | **N/A** |
| ***h*** | Dead Line for bid submission of bid along with time | **N/A** |
| ***i*** | Venue time and date of bid opening | ***At Executive Engineer Public Health Engineering Division II Khairpur @ Ranipur*** |
| ***j*** | Time for completion form written order of commence | 12 Months |
| ***k*** | Liquidity damages | N/A |
| ***l*** | Deposit receipt No: date amount (kin word & Figure) | N/A |
|  |  |  |

***(Executive Engineer/Authority issuing bedding document)***

|  |  |
| --- | --- |
| ***Assistant Engineer***  ***Public Health Engineering***  ***Sub Division Sobhodero*** | ***Executive Engineer***  ***Public Health Engineering***  ***Division II Khairpur @ Ranipur*** |

**SCHEDULE B: CONSTRUCTION OF SURFACE DRAINS AND CC BLOCK FOR**

**CITY MADD UC MADD TALUKA SOBHODERO DISTRICT KHAIRPUR.**

**SUB HEAD No.1** **SURFACE DRAINS**

1. Excavation in foundation of building bridges and other

structure i/c dag belling refilling around the structure

with excavated earth watering ramming lead up to one

chain and lift up to 5 ft. (C S I No.18 (b) P.NO.4)

Qty. 2983.50 Cft @ Rs.3176/25 P %Cft. Rs: 9,476/-

1. Cement concrete plain i/c placing compacting finishing

curing complete i/c screening and washing stone

aggregate w/o shuttering (CSI No.5(i) P.NO.16)

**(a) Ratio 1:4:8**

Qty: 841.50 Cft @Rs.11288/75 P %Cft Rs:94995/-

1. Pacca Brick work in foundation and plinth in cement sand

Ratio (1;6) (CSI No.4 (e) P.NO.21)

Qty: 2542.50 Cft @Rs.11948/36 P% Cft Rs:3,03,787/-

1. Construction of standard of open drains cunette block

of cement concrete 1:2:4 in situ to design profile i/c cost

of mould as per drawing i/c applying floating coat of

cement 1/32” thick to the exposed face finished smooth

curing etc complete as per detail drawing

(PHSI No. D P.NO.44)

Type –I

Qty.900.0 Rft @Rs.94/- P Rft. Rs.84,600/-

Type –II

Qty.300.0 Rft @Rs.174/- P Rft. Rs.52,200/-

1. Cement plaster 1:4 20’ height ½” thick

(CSI No.13 P.NO.52)

Qty.5622.0Sft @Rs.2283/93 P% **Sft.** Rs.1,28,403/**-**

1. RCC work in roo
2. f slab, beams columns rafts, lintels,

and other structure members laid in situ of pre cost

laid in position complete in all respect 1:2:4

(CSI No.7 P.NO.17).

Qty**.** 239.79 **Cft** @Rs.337/- P% **Sft.** Rs:80,809/-

1. Fabrication of mild steel reinforcement for cement

concrete i/c cutting bending laying in position

making K=joints and festering i/c cost of binding

wire also i/c removal of rust from bars

(CSI No.7(ii) P.NO.19).

Qty.8.563 Cwt. @Rs.5001/70 P cwt Rs.42830/-

***Total*** Rs:9,97,100/-

SUB HEAD No.II **C.C Blcok**

1. Barrow pit excavation undressed lead up to 100 ft in

ordinary soil (CSI-3(a) P-1)

Qty.7520.0 CFT @Rs.2117/50 P%0 Cft. Rs.15924/-

2. Lying Earth in 6” layers & leveling dressing &

Watering for Etc complete. (CSI-13(b)P-3)

Qty: 7520.0 CFT @Rs.354/- P%0 Cft Rs.2662/-

3. Extra for every 50”ft additional lead or part there of

(C.S.I No: 8 (a) P-3)

Qty: 7520.0 CFT @Rs.5039/- P%0 Cft Rs.37893/-

4. Cement concrete brick or stone ballast 1 ½” to 2” guage

Ratio 1:4:8 (CSI No.4(b)9 P. 15).

Qty. 2481.60 CFT @Rs.9416/28 P% Cft. Rs.2,33,674/-

5. Cement concrete plain 1:2:4 i/c placing compacting finishing and curing complete i/c

screening and washing of stone aggregate without shuttering

(CSI No.5 P.No.16)

Qty.1880.0 CFT @Rs.14429/25 P% Cft. Rs.271270/-

6. Errection & removal for centering of therefore of Rcc

Partial wood (CSI .No. ) Ratio: 1:2:4.

Qty:512.14 Sft @Rs.3127/41 P% Sft. Rs.17051/-

**Total Rs.578474 /-**

**GENERAL ABSTRACT OF COST**

**SUB HEAD NO: 1 Surface Drains Rs:997100/-**

**SUB HEAD NO: 2 C.C. Topping Rs:578474/-**

**Total Rs:1575574/-**

C O N D I T I O N S

01. Any error / omission in the description of items of work rate original schedule

will correct accordingly under executive engineer Public Health Engineering

division II khairpur @ Ranipur .

02. premium will be allowed as non , schedule items.

03. The work will be carried out as per P.W.D. specification and approval details. working estimates .

|  |  |
| --- | --- |
| Contractor | Executive Engineer  Public Health Engineering  Division II Khairpur @ Ranipur |