|  |  |
| --- | --- |
| **NAME OR WORK :-** | **M/R TO SINDH SECRETARIAT NO.III, ( OLD KDA BUILDING ) KARACHI ( COLOURING, PAINTINGS, FALSE CEILING, FLOOR TILES, & OTHER WORKS IN OFFICE OF ADVISOR TO CHIEF MINISTER MR. SAJID BHANBHAN ).** |

**“ SCHEDULE ‘B’ “**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION OF ITEMS** | **QTY:** | **RATE** | **UNIT** | **AMOUNT** |
|  | **SCHEDULE ITEMS PART-“A” ( CIVIL WORK )** |  |  |  |  |
| 1. | Dismantling glazed or encaustic tiles etc.( SI.55 / P-13 ). | 387.32  Sft | 786/50 | %Sft | 3046/- |
|  | Rupees. Seven hundred eighty six. And. Fifty. Paisa | | | | |
| 2. | Scraping ( b) Ordinary distemper oil bound distemper or Pain on Walls. ( SI.54-(b) / P-13 ). | 1583.81  Sft | 226/88 | %Sft | 3593/- |
|  | Rupees. Two hundred twenty six. And. Eighty eight. Paisa | | | | |
| 3. | Preparing the surface and painting with matt finish paint of approved make to old matt finish ( b ). 2nd & subsequent coat. ( SI.37(A+B) / P-55 ). | 1583.81  Sft | 1772/38 | %Sft | 28071/- |
|  | Rupees. One thousand seven hundred seventy two. And. Thirty eight. Paisa | | | | |
| 4. | Providing and fixing approved quality mortice lock. ( SI.21 / P-60 ). | 04  Nos | 1786/13 | Each | 7148/- |
|  | Rupees. One thousand seven hundred eighty six. And. Thirteen. Paisa | | | | |
|  | **NON-SCHEDULE ITEMS PART-“B”** | **Total Part-“A” Rs.** | | | **41855/-** |
| 1. | P/L Porcelain tiles glazed or matt glazed Master or equivalent jointed in white cement and laid over 1:2 grey cement sand mortar ¾” thick in/c finishing & filling of joints with slurry of white cement or tile grout in desired shape in/c cutting of tiles to proper profile (on floor or facing) **size 16”x16”x1/4”.** | 387.32  Sft |  | P.Sft |  |
| 2. | P/F false ceiling of Gypsum board panels of required design & size in/c frame work of aluminum T-Section hanged with nail wire to ceiling etc complete. | 333.56  Sft |  | P.Sft |  |
| 3. | P/F false ceiling spot light fancy type round shape with glass and 2 holder and energy saver of approved make & quality including fixing in false ceiling by cutting hole as directed by the Engineer Incharge. | 26  Nos |  | Each |  |
| 4. | P/F fine quality roller type blind with approved design false & in/c steel angle fixing with steel screws as per window as required @ site as directed by the Engineer Incharge. | 262.50  Sft |  | P.Sft |  |
| 5. | S/F hydraulic door closer heavy (Yale /KGI) in/c fixing in door frame with necessary screws and adjusting speed as directed by the Engineer Incharge. | 02  Nos |  | Each |  |
| 6. | P/F wall bracket fan 18” dia of approved make & quality (Royal/Pak, Millat or equivalent) in/c fixing on wall as directed by the Engineer Incharge | 02  Nos |  | Each |  |
| 7. | French polish of doors windows ventilators stair floor work etc includes preparing surface and polishing by using lakh Dana, Sprit, thinner, pigment, ICI lacquer, Regmal (Germany) material ICI sealer tar pine oil, polishing as per satisfaction of competent authority etc complete.. | 157.50  Sft |  | P.Sft |  |
| 8 | P/F wooden cabinet with shutter of lassani sheet 3/4" thick and frame work of 1st class partal wood 2”x1” pasted with classic Formica 18” deep in/c necessary hinges, catchers, handles, sliding wheels in doors, nails, screws etc with approved design and shape. The cost also in/c necessary tools and plants to be used in making etc complete as directed by the Engineer Incharge. | 62.00 Sft. |  | P/Sft. |  |
|  |  | **Total Part-“B” Rs.** | | |  |
|  |  | **Total Part-“A” Rs.** | | |  |
|  |  | **G: Total Part ( A+B ) Rs.** | | |  |
|  |  | **Say Rs.** | | |  |

**CONDITION.**

1). Typographical errors in the schedule-“B” are the subject to the correction with reference to the schedule of rate ( Gen: Vol: III, Part-II, inforced: 2012, as approved by the standing rates committee.

2). No Cartage will be paid on any items of works.

3). No premium shall be paid on Non-Schedule items.

4). Water shall be arranged by the Contractor.

**CONTRACTOR.**

|  |  |
| --- | --- |
| **ASSISTANT ENGINEER**  **PROVINCIAL BUILDINGS SUB-DIVISION-V,**  **KARACHI.** | **EXECUTIVE ENGINEER**  **PROVINCIAL BUILDINGS DIVISION-II,**  **KARACHI.** |