|  |  |
| --- | --- |
| **NAME OF WORK :-** | **M/R TO SINDH SECRETARIAT BUILDING NO-V, KARACHI**  **(P/F FIBER GLASS TANK, UPVC / GI PIPE & FITTINGS OVER ROOF)** |

**“ SCHEDULE ‘B’ “**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION OF ITEMS** | **QTY:** | **RATE** | **UNIT** | **AMOUNT** |
| 1 | Providing and fixing New Fibre Glass tank having wall thickness upto 8mm of approved quality & design and wall thickness as specified in/c. cost of nuts & Bolts and fixing on plate form and making connection for inlet outlet & over flow inlet / outlet floor pipes etc. complete (Master Brand). The cost include carriage from shop to site & lifting from ground floor to roof of any floor as directed by the Engineer Incharge. |  |  |  |  |
| a. | **1000 gallons** | 02 Nos |  | Each. |  |
| b. | **500 gallons** | 01 Nos |  | Each. |  |
| 2 | P/F UPVC water supply pipe of AGM or Pak Arab make schedule 40(E) ASTM standard D-1785 with all necessary fittings like elbow, bend, tee etc. This includes fixing on walls with clamps or Jubilee clips upto height of 50’-0 in vertical or horizontal position using Jhoola or long ladder or scaffolding and jointing pipe & fittings with approved solvent / JTG solution. The rate includes all cost of labour, material, and cartage, as directed by Engineer Incharge |  |  |  |  |
| a. | **1-1/2" dia** | 80.00 Rft. |  | P/Rft. |  |
| b. | **1/2" dia** | 40.00 Rft. |  | P/Rft. |  |
| 3 | P/F UPVC fittings of schedule 40(E) ASTM –D-1785 Standard (AGM or Pak Arab make) with the cost of breaking through walls and roof in/c jointing with PVC solvent/JTG solution and fixing at any height/floor using Jhoola or long ladder or scaffolding in horizontal or vertical position as directed by the Engineer Incharge |  |  |  |  |
| a. | 1-1/2” dia Valve Socket | 07 Nos |  | Each |  |
| b. | 1-1/2” dia Tee. | 12 Nos |  | Each. |  |
| c. | 1-1/2” dia Handle valve | 04 Nos |  | Each. |  |
| d. | 1-1/2” dia Socket | 09 Nos |  | Each. |  |
| e. | 1/2" dia valve Socket. | 02 Nos |  | Each. |  |
| f. | 1/2" dia Handle valve | 02 Nos |  | Each. |  |
| 4 | P/F sanitary fitting chrome plated heavy gauge of approved quality (Irfan or equivalent make) fitted with completed accessories as directed by the Engineer Incharge.  **Bib Cock ½” dia** | 02 Nos |  | Each. |  |
| 5 | Removing debries from Sindh Secretariat Buildings in/c collecting from different floors, throwing to stair to ground floor at proper place and then loading on truck and throwing out of city government premises, fuel & hire charges of truck, loading & unloading etc complete. | 07 Nos |  | P/Truck |  |
|  |  |  | **Total Rs.** | |  |
|  |  |  | **Say Rs.** | |  |

**CONDITION.**

1). Typographical errors in the schedule-“B” are the subject to the correction with reference to the schedule of rate ( Gen: Vol: III, Part-II, inforced: 2012, as approved by the standing rates committee.

2). No Cartage will be paid on any items of works.

3). No premium shall be paid on Non-Schedule items.

4). Water shall be arranged by the Contractor.

**CONTRACTOR.**

|  |  |
| --- | --- |
| **ASSISTANT ENGINEER**  **PROVINCIAL BUILDINGS SUB-DIVISION-V,**  **KARACHI.** | **EXECUTIVE ENGINEER**  **PROVINCIAL BUILDINGS DIVISION-II,**  **KARACHI.** |