**SCHEDULE “B”**

**CONSTRUCTION OF KATCHA DRAINS SUI KANDAR MINOR TO MITHO KHOSO VIA MAJEED DERO TALUKA TANDO ADAM DISTRICT SANGHAR.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.# | Description | Qty | Rate | Unit | Amount |

# 1. Excavation for tanks and reservoirs in Wet Soil i/c trimming and dressing sides to alignment design section/profile and shape leveling of beds of trenches to correct level and grade i/c laying of earth in 6” layers of construction of tanks and crossing and disposal of surplus excavated earth with one chain as directed by Engineer in charge providing fence guards lights flags where-ever required lift upto 5’(1.52m)lead upto one chain (30.5m)( PHSI No:14 P/74).

302400.0 cft. Rs.4800/- P%0cft Rs.1451520/-

# 2. Excavation for tanks and reservoirs in slushy or daldaly soil i/c trimming and dressing sides to alignment design section/profile and shape leveling of beds of trenches to correct level and grade i/c laying of earth in 6” layers of construction of tanks and crossing and disposal of surplus excavated earth with one chain as directed by Engineer in charge providing fence guards lights flags where-ever required lift upto 5’(1.52m) lead upto one chain (30.5m)( PHSI No:15 P/74).

181440.0 Cft Rs.7200/- P%0 Cft. Rs.1306368/-

3. Compaction by rolling (This does note include hire charges of the roller (GSI No. 13 P/3)

322560.0 cft Rs. 756/- P% Cft Rs. 241920/-

**Total Rs. 2999808/-**

**CONDITIONS.**

1. *Any error omission in the specification quantity and unit will be governed by the relevant schedule items.*
2. *The rates should be inclusive of all taxes i.e sales tax octori tax etc.*
3. *No separate carriage will be paid to the contractor*
4. *No premium will be allowed for no-schedule items.*
5. *The decision of the Superintending Engineer, Works & Services Department Sanghar will be final and binding the parties if in any dispute.*

EXECUTIVE ENGINEER

PUBLIC HEALTH ENGG: DIVISION

SANGHAR

CONTRACTOR