**SCHEDULE B.**

NAME OF WORK: **S/R TO SECRETARY BUNGALOW NO.04 AT SJC KARACHI.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.NO. | ITEMS OF WORK | QTY | RATE | UNIT | AMOUNT |
| 1 | First class deodar wood wrought joinery work in wire gauze door & windows with 22 SWG galvanized wire gauze 144 mesh per sq inch iron fittings complete. 1 ½” thick deodar wood framing in wire gauze with ordinary hinges (S.I.14-b/p-59) | 25.00  Sft | 562/98 | P. Sft | 14075 |
| 2 | P/f deodar wooden ward rob i/c boxing with back shaves shutters drawers, and brass fitting such as handles locking arrangement hanger rod shoe rod and mirror measuring 2’x3’x1’ complete as per approved design (S.I.24/61) | 23.34 | 2364/63 | P. Sft | 55190 |
|  | **Total A** |  |  |  | **69265** |
|  | **PART B.** |  |  |  |  |
| 1 | Laying white marble flooring fine dressed on the surface without winding set in lime mortar 1:2. In/c rubbing and polishing of the joints (a) ¾” thick flooring (s.i.No.28-a/43) | 10.00 | 567/48 | p. Sft | 5675 |
|  | **Total** |  |  |  | **5675** |
|  | **Less % Below** |  |  |  |  |
|  | **Total B** |  |  |  |  |
|  | **PART C, Non Schedule Items:** |  |  |  |  |
| 1 | P/F wooden floor approved color and design 3/8” thick, by nerlapping the tiles with solution etc, complete. | 565.00 |  | p. Sft |  |
| 2 | P/F colored pvc floor standard thickness with solution etc, complete. (12”x12” ). | 58.00 |  | p. Sft |  |
| 3 | P/F glass windows (color) I/c cutting fitting etc, complete (Imported Make). | 302.00 |  | P. Sft |  |
| 4 | P/F checker tiles 12”x12” over cement sand mortar 1:6. ¾” thick, cleaning & finishing etc, complete. | 2730.0 |  | p. Sft |  |
| 5 | Making and fixing wooden kitchen cabinet with shutters of lasani wood sheet ¾” thick frame work of first class deodar wood 2”x1” pasted with classic Formica and 18” deep including necessary hinges catcher handle sliding wheels in draws nails /screws etc with approved design and shape. The cost also includes necessary tools and plants to be used in making etc complete as directed by the engineer Incharge etc complete. | 31.00 |  | p. Sft |  |
| 6 | P/F stainless steel sink double bowl approved quality with necessary fittings i/c fixed in marble top fitting with cement mortor & curing etc complete. | 1-Nos |  | Each |  |
| 7 | Providing and fixing 3’ burner oven as approved quality fire burner with double door/Sutter including all cost of labour material cartage and fixing charges in all respect. | 1-Nos |  | Each |  |
| 8 | S/F fancy type wall light with glass and fancy frame work as approved design and shape i/c reassembling and necessary electric wiring and connection etc complete. | 54-Nos |  | Each |  |
| 9 | S/F fancy type fine quality imported make schandlier light as approved quality and design i/c necessary electric wiring and connection etc, complete. | 3-Nos |  | Each |  |
|  | **Total** |  |  |  |  |
|  | **‘G’ Total Rs,** |  |  |  |  |
|  | **Say,** |  |  |  |  |

**TERMS AND CONDITION**

1. Any typographical errors in the schedule B are subject to the correction with

Reference to the Schedule of rate General 2012 enforced from 12.07.2012 as

Approved by the S R C, Sindh Karachi

1. Arbitration clause stands deleted from the agreement.
2. No premium shall be paid on a Non schedule items.
3. 100% WELL Graded crushed bajri shall be used in items of work without any

extra payment

1. No Any items of exvceed then the Quantity Provided in the Schedule B without

Prior of the Executive Engineer.

6. All sample of items should be got approved by the Executive Engineer.

CONTRACTOR ASSISTANT ENGINEER

PROVINCIAL BUILDINGS SUB DIVISION-I

KARACHI.