|  |  |
| --- | --- |
| **NAME OR WORK :-** | **M/R SINDH SECRETARIAT BUILDINGS NO.III ( OLD KDA BUILDINGS ) KARACHI**  **(FLOOR TILES, ROLLER BLINDS, COLOURING, PAINTING IN OFFICE OF ADDITIONAL SECRETARY SOCIAL WELFARE DEPARTMENT 4TH FLOOR).** |

**“ SCHEDULE ‘B’ “**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION OF ITEMS** | **QTY:** | **RATE** | | **UNIT** | **AMOUNT** |
|  | **PART-“A” SCHEDULE ITEMS ( CIVIL WORK )** | |  | |  |  |
| **1** | Dismantling glazed or encaustic tiles etc ( SI.55 / P-13 ). | 498.88-Sft | 786/50 | | %Sft | 3924/- |
|  | Rupees. Seven hundred eighty six. And. Fifty. Paisa | | | | | |
| **2** | Scraping ( b) Ordinary distemper oil bound distemper or Pain on Walls.( SI.54-(b) / P-13). | 635.00-Sft | 226/88 | | %Sft | 1441/- |
|  | Rupees. Two hundred twenty six. And eighty eight. Paisa | | | | | |
| **3** | A).Preparing the surface & painting with matt finish paint of approved make to old matt finish surface. B). 2nd & subsequent coat. (SI.37(A+B+B) / P-55 ). | 635.00-Sft | 1772/38 | | %Sft | 11254/- |
|  | Rupees. One thousand seven hundred seventy two. And. Thirty eight. Paisa | | | | | |
| **4** | Distempering (b) two coats (si.24-B/p-54) | 421.00 Sft | 1043/90 | | %Sft | 4395/- |
|  | Rupees. One thousand & forty three. And. Ninety. Paisa | | | | | |
|  | **(A). Total Rs.** | | | | | **21014/-** |
|  |  | | | | |  |
|  | **PART-“B” NON-SCHEDULE ITEMS** |  | |  |  |  |
| **1** | P/L Porcelain tiles glazed or matt glazed Master or equivalent jointed in white cement and laid over 1:2 grey cement sand mortar ¾” thick in/c finishing & filling of joints with slurry of white cement or tile grout in desired shape in/c cutting of tiles to proper profile (on floor or facing) **size 16”x16”x1/4”** | 498.88-Sft | |  | PSft |  |
| **2** | P/F door lock (Handle type ) of approved quality with Colombo handle & machines of Yale & fixing with brass screws as directed by the Engineer Incharge. | 02 Nos | |  | Each. |  |
| **3** | Providing and fixing door closer heavy type KGI or equivalent make i/c. fixing on door with screws and adjusting speed as required etc. complete and as directed by Engineer Incharge. | 01 No | |  | Each. |  |
| **4** | P/F fine quality roller type blind with approved design false & in/c steel angle fixing with steel screws as per window as required @ site as directed by the Engineer Incharge. | 147.00 -Sft | |  | PSft |  |
| **5** | S/F 1-40 watts tube light with 40 watts rod, chock, starter & base fitted on wall ceiling with 23/.076 flexible wire in/c connection to ceiling rose as directed by the Engineer Incharge.(Phillips make ) or equivalent | 06-Nos | |  | Each |  |
| **6** | P/f power plug 15-Amp (Imported make) with plastic board & shet in/c necessary connection. | 04-Nos | |  | Each |  |
|  |  | **Part-“B” Total Rs.** | | | |  |
|  |  | **Part-“A” Total Rs.** | | | |  |
|  |  | **G: Total Part ( A + B + C ) Rs.** | | | |  |
|  |  | **Say Rs.** | | | |  |

**CONDITION.**

1). Typographical errors in the schedule-“B” are the subject to the correction with reference to the schedule of rate ( Gen: Vol: III, Part-II, inforced: 2012, as approved by the standing rates committee.

2). No Cartage will be paid on any items of works.

3). No premium shall be paid on Non-Schedule items.

4). Water shall be arranged by the Contractor.

**CONTRACTOR.**

|  |  |
| --- | --- |
| **ASSISTANT ENGINEER**  **PROVINCIAL BUILDINGS SUB-DIVISION-V,**  **KARACHI.** | **EXECUTIVE ENGINEER**  **PROVINCIAL BUILDINGS DIVISION-II,**  **KARACHI.** |