|  |  |
| --- | --- |
| **NAME OR WORK :-** | **MR TO SINDH SECRETARIAT NO.V,**  **(P/F FALSE CEILING, LED LIGHTS, WOODEN CABINETS / ALMIRAH ETC Works IN DIFFERENT OFFICES.)** |

**“ SCHEDULE ‘B’ “**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION OF ITEMS** | **QTY:** | **RATE** | **UNIT** | **AMOUNT** |
|  | **PART (A) SCHEDULE ITEMS (CIVIL WORKS)** |  |  |  |  |
|  | Providing and fixing deodar Almirah 9” – 12” depth including boxing with back shelves, shutters brass fittings complete. ( SI.23 / P-61 ). | 78.00 Nos | 1778/50 | P.Sft | 138723/- |
|  | Rupees. One thousand seven hundred seventy eight. And fifty paisa | | | | |
|  |  | **(A). Total Rs.** | | | **138723/-** |
|  |  |  | | |  |
|  |  |  | | |  |
|  | **PART (B) NON-SCHEDULE ITEMS** |  | | |  |
| 1. | P/F false ceiling of Gypsum board panels of required design & size in/c frame work of aluminum T-Section hanged with nail wire to ceiling etc complete. | 582.39 P.Sft |  | P.Sft |  |
| 2 | S/F LED spot light China make with 7 Nos lamps each 6 watts fitted on walls, ceiling of approved quality as directed by the Engineer Incharge. | 18- Nos |  | Each |  |
| 3 | S/F Power Plug 3 pin 15 amp with earthen ware bas of approved quality make as directed  by the Engineer Incharge. . | 02 Nos |  | Each |  |
| 4 | P/F wooden cabinet shutter at bottom of kitchen made up of frame work of 1st class partal wood 2”x1” fitted on existing masonary pillars & fixing shutter of laminated lassani sheet 3/4” thick in/c providing & fixing wooden leaping or gola around lassani shutter or making gola by router in approved shape & design & polishing etc. The cost in/c necessary hinges, catchers, handles, sliding wheels, draws lock, nails screws etc. The cost includes necessary tools, plants to be used in making etc complete as directed by the Engineer Incharge. | 21.90 P.Sft |  | P.Sft |  |
| 5 | Providing and fixing New Fibre Glass tank 500 gallons having wall thickness upto 8mm of approved quality & design and wall thickness as specified in/c. cost of nuts & Bolts and fixing on plate form and making connection for inlet outlet & over flow inlet / outlet floor pipes etc. complete (Master Brand). The cost include carriage from shop to site & lifting from ground floor to roof of any floor as directed by the Engineer Incharge. | 01 Nos |  | Each |  |
| 6 | Removing debries from Sindh Secretariat Buildings in/c collecting from different floors, throwing to stair to ground floor at proper place and then loading on truck and throwing out of city government premises, fuel & hire charges of truck, loading & unloading etc complete. | 05  Nos |  | P.Truck |  |
| 7 | Supplying & fixing earthen ware European commode set (Porta / USA make) coupled with flush tank & seat cover complete with internal fittings, fixtures, clamps, necessary lead connection and making requisite No of holes in wall plinth or floor for pipe connection & making good in c.c. 1:2:4 as directed by the Engineer Incharge. | 01 Nos |  | Each |  |
| 8 | P/F Iron Steel grill using solid square bars of size 1/2" x 1/2” placed @ 4” centre to centre in approved design and pattern in/c frame of flat iron Patti of 3/4"x1/8” fixed with screws or pins and painting with two or required coats after first coat of red oxide. The cost in/c all cartage, tools, plants, welding machine etc used in making as directed by the Engineer Incharge. | 29.47 Sft |  | P/Sft |  |
| 9 | P/F collapsible gate with channel framing of section ¾” x 5/16” @ 4” in/c refitted with ¾” x 1/8” flat iron Patti placed diagonally and provided with top & bottom T-section 1”x1”x1/8” along with rollers also in/c locking arrangement and fixing in floor or wall in/c painting 03-coats with 1st coat of red-oxide paint as per instruction of Engineer Incharge. | 54.25 Sft |  | P/Sft |  |
|  |  | **(B). Total Rs** | | |  |
|  |  | **(A). Total Rs** | | |  |
|  |  | **(A+B) Total Rs.** | | |  |
|  |  | **Say** | | |  |

**CONDITION.**

1). Typographical errors in the schedule-“B” are the subject to the correction with reference to the schedule of rate ( Gen: Vol: III, Part-II, inforced: 2012, as approved by the standing rates committee.

2). No Cartage will be paid on any items of works.

3). No premium shall be paid on Non-Schedule items.

4). Water shall be arranged by the Contractor.

**CONTRACTOR.**

|  |  |
| --- | --- |
| **ASSISTANT ENGINEER**  **PROVINCIAL BUILDINGS SUB-DIVISION-V,**  **KARACHI.** | **EXECUTIVE ENGINEER**  **PROVINCIAL BUILDINGS DIVISION-II,**  **KARACHI.** |