**SCHEUDULE “B” CONSTRUCTION OF C.C BLOCK AT KHASKHELI PARO & ABDULLAH SHAH PARO FOR RURAL DRAINAGE SCHEME KHAHI DISTRICT SANGHAR.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.# | Description | Qty | Rate | Unit | Amount |

1. Barrow pit excavation undressed lead upto 100’ ft (GSI NO 3 P/1)

32000.0 Cft Rs: 2117/50 P%0 Cft Rs: 67760/-

2. Earth work compaction laying earth in 6” layers leveling dressing and watering for compaction etc complete (GSI NO 13 P/4)

32000.00 Cft Rs: 354/- P% 0 Cft Rs: 11328/-

3. Cement concrete brick or stone ballast 1 ½” thick gauge (GSI No 4 P/15)

10560.00 Cft Rs: 9416/28 P% Cft Rs. 994359/-

4. Cement concrete plain i/c placing compacting finishing curing etc complete i/c screening and washing of stone aggregate with out shuttering (Ratio 1:2:4)(GSI No: 5 P/17 )

8000.0 Cft Rs: 14429/25 P% Cft Rs: 1154340/-

5. Errection and removal of centring for RCC or plain.C.C work or Partal wood

(GS.I.NO:19 (b) P/18)

1532.0 Rs. 3127/41 P% Cft Rs. 47912/-

6. Extra for every 50’ additional lead or part thereof for earth work soft or ordinary hard or very hard soil (GSI No. 8 P/3)

32000.0 Cft Rs.5039/- P% Cft Rs. 161248/-

Rs. 2436947/-

**CONDITIONS.**

1. Any error omission in the specification quantity and unit will be governed by the relevant schedule items.
2. The rates should be inclusive of all taxes i.e sales tax octori tax etc.
3. No separate carriage will be paid to the contractor
4. No premium will be allowed for no-schedule items.
5. The decision of the Superintending Engineer, Public health Engineering Circle Mirpurkhas will be final and binding the parties if in any dispute.

EXECUTIVE ENGINEER

PUBLIC HEALTH ENGG: DIVISION

SANGHAR