|  |  |
| --- | --- |
| **NAME OR WORK :-** | **M/R TO SINDH SECRETARIAT BUILDINGS NO.I (NEW BUILDING) KARACHI**  **(P/F SEARCH LIGHTS AROUND SINDH SECRETARIAT NO-I GREEN AREA) ).** |

**“SCHEDUDLE ‘B’ “**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION OF ITEMS** | **QTY:** | **RATE** | | **UNIT** | **AMOUNT** |
|  | **PART-“A” SCHEDULE ITEMS ( CIVIL WORK )** | |  | |  |  |
| **1** | Manufacturing providing & fixing GI single Arm double arch as per site requirement with the help of hydraulic crane Instruction of EI with following Specification. GI pipe 2” dia 10 SWG 5’ long 2 Nos MS clamps with nuts & bolts. (SI.144/P-21). | 10 Nos | 2866/- | | Per No | 28660/- |
|  | Rupees (Two thousand eight hundred sixty six ) only. | | | | | |
| **2** | Providing & Fixing of street light 125 watts (HPMV) having IP54 classification with 125w lamp, choke, capacitor & Internal wiring complete in all respect at the height up to 21 ft as per site requirement and instruction of EI. Make of the above light is as follow.(SI.159/P-25) | 10  Nos | 6365/- | | Per No | 63650/- |
|  | Rupees ( Six thousand three hundred sixty five ) only. | | | | | |
| **3** | P/F circuit breaker 15, 20, 30, 40, 50, & 60 amps TP (XE-100CS ( CB ) on prepared board as required ( SI.206 / P-31 ). | 01 No | 5521/- | | Each | 5521/- |
|  | Rupees (Five thousand five hundred twenty one ) only. | | | | | |
| **4** | Providing & fixing Magnetic Contractor FC50N as required & as per instruction of EI.(SI.252/P-37) | 01 N | 9301/- | | Per No | 9301/- |
|  | Rupees (Nine thousand three hundred one ) only. | | | | | |
| **5** | P/F 10 Amps Photo cell (National Japan) after removing of existing burnt/damage /old photo cell after disconnection of main power supply & reconnection the same after fixing of photo cell as required as per instruction of EI.(SI.287/P/41) | 01 No | 4494/- | | Per No | 4494/- |
|  | Rupees ( Four thousand four hundred ninety four ) only. | | | | | |
| **6** | P/F circuit breaker 6,10,15,20,30,40,50, & 63 amp DP (TB-5S) on prepared board as required. (SI.204/P-31) | 08 Nos | 2456/- | | Each. | 19648/- |
|  | Rupees (Two thousand four hundred fifty six ) only. | | | | | |
| **7** | Providing & Fixing of flood light 400 watts ( HPIT ) having IP65 classification with 400w lamp, choke, capacitor, igniter & Internal wiring complete in all respect at the height up to 40ft with the help hydraulic crane and manual labour as per site requirement and manual labour as per site requirement and instruction of EI.( SI.167 / P-26 ) | 10 Nos | 16980/- | | Each | 169800/- |
|  | Rupees (Sixteen thousand nine hundred eighty) only. | | | | | |
| **8** | Providing & fixing 250 watts (SON) lamp @ the height as per site Requirement & instruction of Engineer Incharge. (SI.174/P-27) | 04 Nos | 1240/- | | Per No | 4960/- |
|  | Rupees (One thousand two hundred forty) only. | | | | | |
| **9** | Providing & fixing 250 watts (SON-T) chowk @ the height with the help of hydraulic crane as per site Requirement & instruction of Engineer Incharge.(S.I 174/P-27) | 04 Nos | 3990 | | Per No | 15960/- |
|  | Rupees (Three thousand nine hundred ninety ) only. | | | | | |
| **10** | Providing & fixing 250 watts (SON) ignitor in all respect at the height up to 40 ft with the help of hydraulic crane & manual labor as per site requirement and instruction of EI.(SI.181/P28) | 04 Nos | 1202/- | | Per No | 4808/- |
|  | Rupees ( One thousand two hundred two ) only. | | | | | |
| **11** | Providing & fixing 400 watts (HPTT) lamp @ the height with the help of hydraulic crane as per site Requirement & instruction of engineer in charge. ( SI.185 / P-29 ). | 06 Nos | 2380/- | | Each | 14280/- |
|  | Rupees (Two thousand three hundred eighty) only. | | | | | |
| **12** | Providing & fixing 400 watts (HPIT) chowk @ the height with the help of hydraulic crane as per site Requirement & instruction of Engineer Incharge. (SI.186/P-29) | 06 Nos | 4375/- | | Per No | 26250/- |
|  | Rupees (Four thousand three hundred seventy five ) only. | | | | | |
|  | **(A). Total Rs.** | | | | | **367332/-** |
|  | **Above / Below Rs.** | | | | |  |
|  |  | | | | |  |
|  | **PART-“B” NON SCHEDULE ITEMS.** |  | |  |  |  |
| **1** | P/F distribution board 16 gauge of accommodate for mains or sub-mains, circuit breaker, bus bar, and other similar Job double shutter painted with enemelled paint as directed by the Engineer Incharge. | 01.50 Sft | |  | P/Sft |  |
|  |  | **(B). Total Rs.** | | | |  |
|  |  |  | | **(A). Total Rs.** | |  |
|  |  | **G. Total ( A + B ) Rs:** | | | |  |
|  |  | **Say Rs.** | | | |  |

**CONDITION.**

1). Typographical errors in the schedule-“B” are the subject to the correction with reference to the schedule of rate ( Gen: Vol: III, Part-II, inforced: 2012, as approved by the standing rates committee.

2). No Cartage will be paid on any items of works.

3). No premium shall be paid on Non-Schedule items.

4). Water shall be arranged by the Contractor.

**CONTRACTOR.**

|  |  |
| --- | --- |
| **ASSISTANT ENGINEER**  **PROVINCIAL BUILDINGS SUB-DIVISION-V,**  **KARACHI.** | **EXECUTIVE ENGINEER**  **PROVINCIAL BUILDINGS DIVISION-II,**  **KARACHI.** |