***BIDDING DATA***

***Work No:* Tender No.(5)/ (2015-2016)**

(This section should be filled by the Engineer/Procuring Agency before issuance of the Bidding Documents).

**(a).Name of Procuring Agency** Deputy Commissioner, District Central-Karachi

**(b).Brief Description of Works** Rehabilitation / Improvement of Main roads & Links roads in the area of District Central Karachi.

**(c).Procuring Agency’s address:-** Near Sakhi Hassan, North Nazimabad Karachi

**(d).Estimated Cost:- ­­­­­­­­­­­­­­­­­­­­­­­­\_\_**25.000**\_**Million**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**(e).Amount of Bid Security:-** Rs.10,00,000/- \_(Fill in lump sum amount or in % age of bid amount/estimated cost, but not exceeding 5%

**(f).Period of Bid Validity (days):- \_\_\_\_\_\_\_\_**90 Days\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**(g).Security Deposit :-( including bid security):-** \_\_\_\_\_\_\_\_10%\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(in % age of bid amount/estimated cost equal to 10%)

**(h).Percentage, if any, tobe deducted from bills:-** 7.5% Income Tax for filer\_\_\_\_\_\_\_\_\_\_\_\_

**(i).Deadline for Submission of Bids along with time:-** Dated: 01-06-2016\_2:00 PM\_\_

**(j).Venue, Time, and Date of Bid Opening:-** Office of the Deputy Commissioner, Karachi-Central Near Sakhi Hassan, North Nazimabad Karachi. At 3:00 PM Dated:-\_01-06-2016

**(k).Time for Completion from written order of commence:-** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**(l).Liquidity damages:-\_\_\_\_\_\_**0.10%**\_\_\_\_\_\_\_\_**0.05 of Estimated Cost of Bid cost per day of delay, but total not exceeding 10%).

**(m)Tender Cost Receipt Pay Order No:\_\_\_\_\_\_\_\_\_\_\_\_Date:\_\_\_\_\_\_\_\_\_\_Amount:\_\_\_\_\_\_\_**

**(n).Deposit Receipt Pay Order No:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Date:\_\_\_\_\_\_\_\_\_\_Amount:\_\_\_\_\_\_\_**

Name of Bank\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**(o).Bidding Documents issued to:M/s.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**ISSUING AUTHORITY**

**DISTRICT MUNICIPAL CORPORATION (CENTRAL) KARACHI**

**BILL OF QUANTITIES**

NAME OF WORK:- Rehabilitation / Improvement of Main roads & Links roads in the area of District Central Karachi..

**Tender No.(5)/ (2015-2016)**

**(PART-A: ITEM BASED ON SCHEDULE RATE)**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **SR#** | **Description of Item** | **Qty** | **Rate** | **Unit** | **Amount** |
|  | SCARIFYING THE EXISTING ROAD SURFACE.  (VOL-III PART-VI PG-13/51 2012 | 30000 SFT | 116.16 | % SFT | 34848/= |
|  | EARTH WORK EXCAVATION OF ROAD SIDE NAALIS I/C FORMING ITS BANKS OR PUTTING THE SAME ON EMBANKMENT AS DIRECTED CLOD BREAKING ETC COMPLETED.(THROW WORK) (IN ORDINARY SOIL)  VOL-III PART-VI PG-1/4 2012 | 40000 CFT | 1437.00 | %0 CFT | 57480 /= |
|  | CARTAGE OF % CFT 5 TONS ALL MATERIALS LIKE STONE AGGREGATE SPAWL COAL LIME SURKHI EARTH ETC COMPLETE 7 MILES LEAD. | 44800 CFT | 804.52 | % CFT | 360425 /= |
|  | P/L AGGREGATE BASE COURSE IN PROPER GRADE ABD CAMBER HAVING CBR 80% AS PER ASSHTO STANDARD SPECIFICATION I/C SPREADING AND COMPACTING BY APPROVED MECHANICAL MEANS (MOTOR GRADER VIBRATORY ROLLER AND SMOOTH WHEEL ROLLER ETC ) WATER TO MAINTAIN THE MOISTURES CONTAIN THE COMPACTION OF EACH LAYER SHALL 100 % TO THE MAX DRY DENSITY (RATE I/C ALL COST OF MATERIAL T&P AND CARRIAGE UP TO 3 CHAIN)  VOL-III PART-VI PG-05/13B 2012. | 60000 CFT | 5542.24 | % CFT | 3325344 /= |
|  | P/L 1 ½ “ THICK ASPHALT CONCRETE WEARING COURSE PLANT MIXED LAYING MECHANICALLY TO PROPER LINE AND GRADE PLANT MIXED ASPHALT CONCRETE SPEIFIED FORMULA ACCORDING TO JOB MIX FORMULA APPROVED BY THE ENGINEER INCHARGE ROLLING & FINISHING TO DESIGN PROPER GRADE LINE LEVEL AND GRADE LINE LEVEL AND CAMBER ETC ( MACHINERY WITH **POLS** COST OF MATERIAL CARRIAGE). | 80000 SFT | 6873.79 | % SFT | 5499032 /= |
|  | 2” (50mm) Thick Asphalt Concrete Wearing Course Plant Mix  Laying to proper line and grade plant mixed asphalt concrete paver finished (Hydraulic / Electronic control) prepared to specified formula according to job mix formula approved by engineer incharge including rolling and finishing to proper line, grade level and camber etc (machinery with POLs cost of material carriage) | 56598.53 SFT | 8274.73 | % SFT | 4683376 /= |
|  | P/L TO PROPER LINE AND GRADE 1” THICK PRE MIXED CARPET WITH PAVOR MACHINE. PREPARED TO SPECIFIED FORMULA ACCORDING TO JOB MIX FORMULA APPROVED BY ENGINEER INCHARGE I/C ROLLING AND FINISHING TO PROPER LINE AND GRADE LEVEL AND CAMBER ETC RATE ALL COST OF MATERIAL T&P CARRIAGE UP TO 3 CHAIN.  VOL-III PART-VI PG-08/21B 2012. | 60000 SFT | 4107.84 | % SFT | 2464704/= |
|  | SUPPLYING AND FIXING OF REFLECTORIZE ROAD STUD DOUBLE FACE FLUSH SURFACE TYPE. | 3675 NOS | 596.23 | EACH | 2191145/= |
|  | PAVEMENT MARKING IN REFLECTIVE THERMOPLASTIC PAINTS FOR LINES IN 6” WIDTH. | 40000 RFT | 41.24 | P.RFT | 1649600/= |
|  | **TOTAL COST OF SCHEDULE ITEMS RS:-** | | | | **18047954-** |

NAME OF WORK:- Rehabilitation / Improvement of Main roads & Links roads in the area of District Central Karachi.

**Tender No.(5)/ (2015-2016)**

**(PART-B: ITEM BASED ON NON SCHEDULE ITEM APPROVED RATE)**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **SR#** | **Description of Item** | **Qty** | **Rate** | **Unit** | **Amount** |
|  | P/F PRECAST KERB BLOCK 3750 PSI MADE SIZE 06” THICK 12” LONG 18” HEIGHT I/C THE COST OF EXCAVATION 1:3:6 LEAN I/C CARTAGE RACKING OUT JOINTS 1:4 CEMENT SAND MORTOR. | 5702.RFT | 220.00 | P.RFT | 1254440/- |
|  | CONSTRUCTION OF MONOMENT AS PER DRAWING AND DESIGN BY THE DEPARTMENT, REMOVING ALL TYPE OF DISMENTLING WORK RCC OR CC AT SITE. INCLUDING ALL KIND OF RCC WORK, CC PLATEFORM COMPLETE WITH REQUIRED GLAZED TILES INCLUDING REQUIRED FIBER WORK ELECTRICAL WORK, BEAUTIFICATION WORK AND FOUNTAIN OF MONOMENT COMPLETE WITH ALL RESPECT AS PER DIRECTED BY THE ENGINEER INCHARGE. | ONE JOB | 25,00,000/- | P/JOB | 25,00,000/- |
|  | **TOTAL COST OF NON SCHEDULE ITEMS RS:-** | | | | **3754440/-** |

Nomenclature quantities and

Rates have been checked by us

ASSTT:EX:ENGINEER EXECUTIVE ENGINEER

DMC (CENTRAL) DMC(CENTRAL

NAME OF WORK:- Rehabilitation / Improvement of Main roads & Links roads in the area of District Central Karachi.

**Tender No.(5)/ (2015-2016)**

**QUOTED BID SUMMERY**

I/We hereby quoted as follows.

|  |  |  |  |
| --- | --- | --- | --- |
|  | | **In Figures** | **In Words** |
| 1. | PART-A (Item Based on S/R) amounting Rs **18047954-** \_\_\_\_\_\_\_\_%Above/Below of the S/R | Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_ |  |
| 2. | PART-**B** (Item Based on Non S/I Approved Rate) amounting  Rs. **3754440/-** \_\_\_\_\_\_\_\_%Above/Below of the A/R | Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_ |  |
| 3. | **GRAND TOTAL (A+B)** | Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_ |  |

**NOTE:**

* Tender must be quoted in figure & in work both otherwise liable to be cancelled.
* All over writing & correction if any must be initialed & stamped by the bidder.
* I / We read the Standard Bidding Documents available in SPPRA website ([www.pprasindh.govt.pk](http://www.pprasindh.govt.pk)) and agreed to abide all of them and also provide all these documents with our signatures as & when directed.

Signature of the Contractor

with Stamp\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Address:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_