Name of work: M/R to Secretary Bungalow No.1 Town Houses GOR III Karachi (Electric Work)

Schedule B

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.No. | Description | Qty | Rate | Unit | Amount |
| 1 | Wiring for light or fan point with 3/029 PVC insulated wire in 20mm (3/4)channel patti on surface as required.(S.I.129/18) | 23-Nos | 910/- | Each | 20930 |
| 2 | Wiring for Plug point with 3/029 PVC insulated wire in 20mm (3/4)channel patti on surface as required.(S.I.134/15) | 6-Nos | 742/- | Each | 4452 |
| 3 | Wiring for Call bell point with 3/029 PVC insulated wire in 20mm (3/4)channel patti on surface as required.(S.I.134/15) | 1-No | 1590/- | Each | 1590 |
| 4 | P/L main or Sub main PVC insulated with size 2-7/044 (4mm2) copper conductor in ¾ ” dia PVC conduit on surface.(S.I.4/1) | 250.00  Meter | 305/- | p.Meter | 76250 |
| 5 | P/L main or Sub main PVC insulated with size 2-7/036 (4mm2) copper conductor in ¾ ” dia PVC conduit on surface.(S.I.4/1) | 50.00  Meter | 200/- | p.Meter | 10000 |
| 6 | P/F Circuit Brackers 6,10,15,20, 30,40,50 & 63 amps SP (TB SS) on a prepared board as required.(S.I.203/31) | 3-Nos | 916/- | Each | 2748 |
| 7 | P/F Circuit Brackers 6,10,15,20, 30,40,50 & 63 amps DP (TB SS) on a prepared board as required.(S.I.203/31) | 3-Nos | 2456/- | Each | 7368 |
|  | Total |  |  |  | 123338 |
|  | Part B N.S.I |  |  |  |  |
| 1 | P/F Power Plug 15-Amps Imported quality i/c board etc complete. | 9-Nos |  | Each | 5850 |
| 2 | P/F Universal 5-10 amps imported quality i/c board etc complete. | 4-Nos |  | “ | 1800 |
| 3 | P/F Fancy Wall Light i/c shade holder i/c necessary electric connection etc complete. | 18-Nos |  | “ | 33300 |
| 4 | P/F Ceiling Light with holder i/c electric connection etc complete. | 16-Nos |  | “ | 36000 |
|  | P/F Fancy False Ceiling Light with glass holder i/c electric connection etc complete. | 10-Nos |  |  |  |
| 5 | P/F Exhaust Fan Plastic Body equelent quality i/c necessary electric connection as per approved quality etc complete. | 6-Nos |  | Each |  |
| 6 | P/F Ceiling Fan 56” Sweep make Pak or equelent quality i/c necessary electric connection etc complete. | 10-Nos |  | “ |  |
| 7 | P/F Energy Saver 25 watt i/c holder as per approved quality i/c necessary electric connection etc complete. | 16-Nos |  | “ |  |
| 9 | P/F Gate Light with holder i/c electric connection etc complete. | 2-Nos |  | “ |  |
| 10 | **P/F Fancy Tube Light 2-40 watt fancy shade i/c chock & starter i/c necessary electric connection etc complete.** | **8-Nos** |  | **“** |  |
| 11 | P/F Wall Bracket Fan 18” Sweep make Pak or equelent quality i/c necessary electric connection etc complete. | **10-Nos** |  | **“** |  |
|  | Total B |  |  |  |  |
|  | G Total |  |  |  |  |
|  | Say Rs |  |  |  |  |

TERMS & CONDITION

1. Any typographical errors in the schedule B are subject to the correct condition with Reference to the schedule of rate General 2012 enforced from 12-07-2012 as approved by the SRC Sindh.
2. Arbitraction clause stands deleted from the agreement.
3. No Premium shall be paid on Non Schedule Items
4. 100% well Graded crushed bajri shall be used in items of work without any extra payment.
5. No any items of exveceed then the quantity provided in the schedule B without prior of the Executive Engineer.
6. All sample of items should be got approved by the Executive Engineer

Contractor

Assistant Engineer,

Provincial Electrical sub Division-XII,

Karachi