Name of work: M/R TO SECRETARY BUNGALOW 01 TO 08 AT GOR III TOWN HOUSES (EXTERNAL ELECTRIFICATION)

Schedule B

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.No. | Description | Qty | Rate | Unit | Amount |
| 1 | P/L main or Sub main PVC insulated with size 2-7/044 (6mm2) copper conductor in 1” dia PVC conduit on surface.(S.I.5/1) | 140.54  Meter | 305/- | P.Meter | 42865 |
| 2 | P/L main or Sub main PVC insulated with size 2-7/036 (4mm2) copper conductor in ¾ ” dia PVC conduit on surface.(S.I.4/1) | 145.64  Meter | 200/- | p.Meter | 29128 |
| 3 | P/F Circuit Brackers ,15,20, 30,40,50 60,&75&100 amps TP (XS-100NS) on a prepared board as required.(S.I.207/31) | 2-Nos | 9261/- | Each | 18522 |
| 5 | P/F Circuit Brackers ,6,10,15,20,30,40,50,&63 amp DP (TBSS) on prepared board as required.,(S.I.204/31) | 4-Nos | 2456/- | Each | 9824 |
| 6 | P/F circuit bracker 6,10,15,20,30 40,50,&63 amp TP EX(100)CS (CB) on Prepared board as required.(S.I.31/204) | 3-No | 5521/- | Each | 16563 |
| 7 | P/F of Stree Light 400 watts (SON) having IPSS classification with 400 w lamp choke, ignator, & internal wiring complete in all respect at the height with the help hydraulic crane and manual labour as per site requirement and inst | 10-Nos | 26330/- | Each | 263300 |
|  | Total A |  |  |  | **382200** |
|  | PART B N.S.I |  |  |  |  |
| 1 | M/F Distribution board to accommodate main or sub main brackers i/c P/F Pilot lamp i/c locking arrangement & painting 2-coats etc c | **4.17**  **Sft** |  | **Sft** |  |
| 2 | P/F Gate Light fancy type approved make & design heavy pattern with Glass shade Cover and Bulb holder best quality i/c fixing on existing position with Internal electric connection i/c all cost of labour material and necessary required as directed by the E.I | **16-Nos** |  | **Each** |  |
| 3 | P/F Ceiling Light fancy type approved make & design heavy pattern with Glass shade Cover and Saver Bulb 18-watts holder best quality i/c fixing on existing position with Internal electric connection i/c all cost of labour material and necessary required as directed by the Engineer Incharge etc compl | **16-Nos** |  | **Each** |  |
|  | Total B |  |  |  |  |

TERMS & CONDITION

1. Any typographical errors in the schedule B are subject to the correct condition with Reference to the schedule of rate General 2012 enforced from 12-07-2012 as approved by the SRC Sindh.
2. Arbitraction clause stands deleted from the agreement.
3. No Premium shall be paid on Non Schedule Items
4. 100% well Graded crushed bajri shall be used in items of work without any extra payment.
5. No any items of exveceed then the quantity provided in the schedule B without prior of the Executive Engineer.
6. All sample of items should be got approved by the Executive Engineer

Contractor

Assistant Engineer,

Provincial Electrical sub Division-XII,

Karachi