**BILL OF QUANTITIES**

**(A) Description and rate of Items based on Composite Schedule of Rates.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Item No** | **Quantities** | **Description of item to be executed at site** | **Rate** | **Unit** | **Amount in Rupees** |
| **1** | **2** | **3** | **4** | **5** | **6** |
| 1 | 60000 | Earth work excavation undressed lead upto extra one miles Kassi or Phawrah or Shovel in ordinary soil (G.S.I.NO. 1/B- P/1) | 5431.25 | P%oCft | 325875 |
| 1 | 25200 | Cement concrete stone ballast 1 1/2" to 2 guage (G.S.I.NO. 4/B- P/15) | 9416.28 | P%Cft | 2372903 |
| 1 | 19800 | Cement concerts plain including placing compacting, finishing and curing, complete (including screening and washing at stone aggregate without shuttering (G.S.I.NO. 5/F- P16 | 14429.25 | P%Cft | 2856992 |

**Amount TOTAL (a) (Rs: 5555770/-)**

**--------------------- % above/below on the rates of CSR.** **Amount to be added/deducted on the basis**

**Of premium quoted.** **TOTAL (b)**

**Total (A) = a+b in words & figures:**

**Contractor Municipal Engineer/Procuring Agency**