**BILL OF QUANTITIES**

**(A) Description and rate of Items based on Composite Schedule of Rates.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Item No** | **Quantities** | **Description of item to be executed at site** | **Rate** | **Unit** | **Amount in Rupees** |
| **1** | **2** | **3** | **4** | **5** | **6** |
| 1 | 2475 | Earth work excavation undressed upto a single throw of kassi phawrah or shovel extra lead one mile. (G.S.I 1/B P/1) | 5431.25 | P%oCft | 13442 |
| 1 | 495 | Cement concrete stone ballast 1 1/2" to 2 guage (G.S.I 4/b P/15) | 9416.28 | P%Cft | 46611 |
| 1 | 15000 | Filling watering ramming earth in floor with new earth excvated from out side Lead upto one chain and lift upto 5'ft i/c extra lead 6 Mile (GSI.NO. 22 P-4) | 3630.00 | P%oCft | 54450 |
| 1 | 3520 | Erection and removal of centering for R.C.C or plain cement concrete wowrk of vertical wood for partal (G.S.I 19/B-ii P/18) | 3124.41 | P%Sft | 110085 |
| 1 | 5280 | Cement Conrete Plain including placing compacting finishing and curing complete GSI.No. 5/f P-16) | 14429.25 | P%Cft | 761864 |
| 1 | 151 | Pacca Brick work in cement mortar 1:6 (G.S.I 5/E- P/21) | 12674.36 | P%Sft | 19078 |
| 1 | 538 | Cement plaster 1:6 upto 12ft height (B) 1/2" thick (G.S.I. No 13/B- P/52) | 2206.60 | P%Sft | 11863 |
| 1 | 42 | Fabrication of heavy steel work with angles, tees flat iron, round itronand sheet iron for making trusses, girdes, tands etc including cutting tanks etc including cutting, drilling rivertting , handling assembling and fixing but excluding erecton in positoin (G.S.I.No: 2/6 P/91) | 5114.83 | P.Cwt | 2124 |
| 1 | 24000 | Borrow Pit Excavation undressed extra lead upto 3 Miles in ordinary Soil (G.S.I NO. 3/a-P/1) | 7911.60 | P%oCft | 189878 |
| 1 | 300 | Supplying Mannure | 298.12 | P.Cart | 89436 |
| 1 | 12000 | Supply & Lawns with Dacca Grass mixed with manure the bed of 6" layer of bhallo SAND . This Rate i/c turfing lawn,cost of turf bhaloo sand ,filling ,watering ,dressing and maintenance of lawn for one month etc complete.(R.A.A.Attached ) | 20.50 | P.Sft | 246000 |
| 1 | 8 | Providing / fixing Golden Stone garden banches size 4-00' x 1' -6" i/c sotne padistals duly fixed on garden surface in C.C 1:2:4 | 14500.00 | Each | 116000 |
| 1 | 100 | Providing / planning Different plants of flowers, this rate i/c cost of three plant, digging the tranch upto required depth errecting plant and refillling excavated swoil mixing with manure etc complete in all respects i/c maintenance for 30-days. | 350.00 | Each | 35000 |
| 1 | 10 | Providing and Garden lightfixing fancy park lights 45/w T/Lamp/Bulbs 14ft hights i/c wiring, foundation with accessories etc complete. R.A | 38000.00 | Each | 380000 |
| 1 | 2700 | Providing and fixing cement paving blocks flooring having size of 197 x 197 x 80 (mm) of city / quddra / cobble shape with pigmented having strenght b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / patter and design etc: complete (G.S.I 74- P/50) | 248.17 | P.Sft | 670059 |
| 1 | 450 | Providing G.I pipe and special etc including fixing cutting fitting complete with & i/c the cost of cutting trench up 2-1/2" feet deep reafiling waterng ramming and disposal of surplus earth winthin one chain painting two coats of bitumen pain to pipes special after cleaing hassing cloth scaked in maxphalt composition of wraped tightly round pipe adn tesing to a pressure head of 200 ft heandingly (W.S.S.F. No 1/V- P/14) | 183.58 | P.Rft | 82611 |
| 1 | 1 | Donki Pump wit electric motor (M.R ) | 12000.00 | Each | 12000 |
| 1 | 2472 | Oil Paint (G.S.I 4/1 P/68) | 657.91 | P%Sft | 16264 |
| 1 | 3178 | Distempering (B) 2 coats (G.S.I 24/B P/54) | 1043.90 | P%Sft | 33171 |

**Amount TOTAL (a) (Rs: 2889936/-)**

**--------------------- % above/below on the rates of CSR.** **Amount to be added/deducted on the basis**

**Of premium quoted. TOTAL (b)**

**Total (A) = a+b in words & figures:**

**Contractor Municipal Engineer/Procuring Agency**